Release 6.3i Map G.38
Xilinx Mapping Report File for Design 'system'

Design Information
------------------
Command Line   : map -o system_map.ncd -pr b system.ngd system.pcf 
Target Device  : 3s400
Target Package : ft256
Target Speed   : -4
Mapper Version : spartan3 -- $Revision: 1.16.8.2 $
Mapped Date    : Thu Jul 28 13:34:01 2005

Design Summary
--------------
Number of errors:      0
Number of warnings:   71
Logic Utilization:
  Number of Slice Flip Flops:       1,536 out of   7,168   21%
  Number of 4 input LUTs:           1,859 out of   7,168   25%
Logic Distribution:
  Number of occupied Slices:                        1,595 out of   3,584   44%
    Number of Slices containing only related logic:   1,595 out of   1,595  100%
    Number of Slices containing unrelated logic:          0 out of   1,595    0%
      *See NOTES below for an explanation of the effects of unrelated logic
Total Number 4 input LUTs:          2,320 out of   7,168   32%
  Number used as logic:              1,859
  Number used as a route-thru:          44
  Number used for Dual Port RAMs:      256
    (Two LUTs used per Dual Port RAM)
  Number used as Shift registers:      161
  Number of bonded IOBs:               85 out of     173   49%
    IOB Flip Flops:                    81
  Number of Block RAMs:                8 out of      16   50%
  Number of MULT18X18s:                3 out of      16   18%
  Number of GCLKs:                     2 out of       8   25%
  Number of BSCANs:                    1 out of       1  100%

   Number of RPM macros:            5
Total equivalent gate count for design:  589,067
Additional JTAG gate count for IOBs:  4,080
Peak Memory Usage:  97 MB

NOTES:

   Related logic is defined as being logic that shares connectivity -
   e.g. two LUTs are "related" if they share common inputs.
   When assembling slices, Map gives priority to combine logic that
   is related.  Doing so results in the best timing performance.

   Unrelated logic shares no connectivity.  Map will only begin
   packing unrelated logic into a slice once 99% of the slices are
   occupied through related logic packing.

   Note that once logic distribution reaches the 99% level through
   related logic packing, this does not mean the device is completely
   utilized.  Unrelated logic packing will then begin, continuing until
   all usable LUTs and FFs are occupied.  Depending on your timing
   budget, increased levels of unrelated logic packing may adversely
   affect the overall timing performance of your design.


Table of Contents
-----------------
Section 1 - Errors
Section 2 - Warnings
Section 3 - Informational
Section 4 - Removed Logic Summary
Section 5 - Removed Logic
Section 6 - IOB Properties
Section 7 - RPMs
Section 8 - Guide Report
Section 9 - Area Group Summary
Section 10 - Modular Design Summary
Section 11 - Timing Report
Section 12 - Configuration String Information
Section 13 - Additional Device Resource Counts

Section 1 - Errors
------------------

Section 2 - Warnings
--------------------
WARNING:Pack:249 - The following adjacent carry multiplexers occupy different
   slice components.  The resulting carry chain will have suboptimal timing.
   	microblaze_0/microblaze_0/Debug_I/address_data_hit_20/MUXCY_Pre
   	microblaze_0/microblaze_0/Debug_I/address_data_hit_20/MUXCY_data_13
WARNING:Pack:249 - The following adjacent carry multiplexers occupy different
   slice components.  The resulting carry chain will have suboptimal timing.
   	microblaze_0/microblaze_0/Data_Flow_I/Zero_Detect_I/I_Part_Of_Zero_Detect7
   	microblaze_0/microblaze_0/Decode_I/MUXCY_JUMP_CARRY
WARNING:Pack:249 - The following adjacent carry multiplexers occupy different
   slice components.  The resulting carry chain will have suboptimal timing.
   	microblaze_0/microblaze_0/Decode_I/MUXCY_JUMP_CARRY
   	microblaze_0/microblaze_0/Decode_I/MUXCY_JUMP_CARRY2
WARNING:Pack:249 - The following adjacent carry multiplexers occupy different
   slice components.  The resulting carry chain will have suboptimal timing.
   	microblaze_0/microblaze_0/Debug_I/address_hit_I0/MUXCY_Pre
   	microblaze_0/microblaze_0/Debug_I/address_hit_I0/MUXCY_13
WARNING:Pack:249 - The following adjacent carry multiplexers occupy different
   slice components.  The resulting carry chain will have suboptimal timing.
   	microblaze_0/microblaze_0/Debug_I/address_data_hit_10/MUXCY_Pre
   	microblaze_0/microblaze_0/Debug_I/address_data_hit_10/MUXCY_data_13
WARNING:Pack:249 - The following adjacent carry multiplexers occupy different
   slice components.  The resulting carry chain will have suboptimal timing.
   	microblaze_0/microblaze_0/Debug_I/address_hit_I1/MUXCY_Pre
   	microblaze_0/microblaze_0/Debug_I/address_hit_I1/MUXCY_13
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I31/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I29/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I27/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I25/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I23/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I21/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I19/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I17/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I15/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I13/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I11/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I9/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I7/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I5/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I3/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I1/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I31/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I29/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I27/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I25/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I23/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I21/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I19/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I17/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I15/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I13/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I11/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I9/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I7/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I5/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I3/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I1/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I30/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I28/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I26/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I24/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I22/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I20/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I18/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I16/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I14/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I12/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I10/r
   eg2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I8/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I6/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I4/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I2/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I0/re
   g2_Data_Low is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I30/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I28/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I26/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I24/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I22/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I20/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I18/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I16/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I14/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I12/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I10/r
   eg2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I8/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I6/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I4/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I2/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:331 - Blockcheck: Dangling G output. G of comp
   microblaze_0/microblaze_0/Data_Flow_I/Register_File_I/Register_File_Bit_I0/re
   g2_Data_High is configured, but output is not used.
WARNING:DesignRules:372 - Netcheck: Gated clock. Clock net
   opb_intc_0/opb_intc_0/INTC_CORE_I/INTR_DET_I/interrupts<0> is sourced by a
   combinatorial pin. This is not good design practice. Use the CE pin to
   control the loading of data into the flip-flop.

Section 3 - Informational
-------------------------
INFO:LIT:95 - All of the external outputs in this design are using slew rate
   limited output drivers. The delay on speed critical outputs can be
   dramatically reduced by designating them as fast outputs in the schematic.
INFO:MapLib:562 - No environment variables are currently set.
INFO:MapLib:535 - The following Virtex BUFG(s) is/are being retargetted to
   Virtex2 BUFGMUX(s) with input tied to I0 and Select pin tied to constant 0:
   BUFGP symbol "bufgp_71" (output signal=dlmb_port_BRAM_Clk),
   BUFG symbol "debug_module/debug_module/BUFG_DRCK1" (output
   signal=debug_module/bscan_drck1),
   BUFG symbol "debug_module/debug_module/BUFG_DRCK2" (output signal=DBG_CLK_s)
INFO:MapLib:159 - Net Timing constraints on signal sys_clk_pin are pushed
   forward through input buffer.

Section 4 - Removed Logic Summary
---------------------------------
 320 block(s) removed
  87 block(s) optimized away
 316 signal(s) removed

Section 5 - Removed Logic
-------------------------

The trimmed logic report below shows the logic removed from your design due to
sourceless or loadless signals, and VCC or ground connections.  If the removal
of a signal or symbol results in the subsequent removal of an additional signal
or symbol, the message explaining that second removal will be indented.  This
indentation will be repeated as a chain of related logic is removed.

To quickly locate the original cause for the removal of a chain of logic, look
above the place where that logic is listed in the trimming report, then locate
the lines that are least indented (begin at the leftmost edge).

Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I24" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I25" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I26" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I30" (SFF)
removed.
 The signal "mb_opb_OPB_ABus<30>" is loadless and has been removed.
  Loadless block "mb_opb/mb_opb/OPB_ABus_I/_n00921" (ROM) removed.
   The signal "mb_opb_M_ABus<30>" is loadless and has been removed.
    Loadless block
"microblaze_0/microblaze_0/Data_Flow_I/ALU_I/ALU_Bit_I30/I_ABus_DFF" (SFF)
removed.
   The signal "mb_opb_M_ABus<62>" is loadless and has been removed.
    Loadless block "microblaze_0/microblaze_0/Iopb_Interface_I/IM_ABus_I30" (ROM)
removed.
     The signal "microblaze_0/microblaze_0/Instr_Addr_Stored<30>" is loadless and has
been removed.
      Loadless block "microblaze_0/microblaze_0/Iopb_Interface_I/ABus_FF_I30" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I31" (SFF)
removed.
 The signal "mb_opb_OPB_ABus<31>" is loadless and has been removed.
  Loadless block "mb_opb/mb_opb/OPB_ABus_I/_n00951" (ROM) removed.
   The signal "mb_opb_M_ABus<31>" is loadless and has been removed.
    Loadless block
"microblaze_0/microblaze_0/Data_Flow_I/ALU_I/ALU_Bit_I31/I_ABus_DFF" (SFF)
removed.
   The signal "mb_opb_M_ABus<63>" is loadless and has been removed.
    Loadless block "microblaze_0/microblaze_0/Iopb_Interface_I/IM_ABus_I31" (ROM)
removed.
     The signal "microblaze_0/microblaze_0/Instr_Addr_Stored<31>" is loadless and has
been removed.
      Loadless block "microblaze_0/microblaze_0/Iopb_Interface_I/ABus_FF_I31" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I0" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I1" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I10" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I11" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I12" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I13" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I14" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I15" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I16" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I17" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I18" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I19" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I2" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I20" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I21" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I22" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I23" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I24" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I25" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I26" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I27" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I28" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I29" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I3" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I4" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I5" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I6" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I7" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I8" (SFF)
removed.
Loadless block "opb_intc_0/opb_intc_0/OPB_INTFC_I/OPB_DBUS_REG_BIT_I9" (SFF)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_EMC/ADDR_CNTRMUX_I/ADDRCNT_I/MUXCY_i10" (MUX)
removed.
 The signal
"sram_256kx32/sram_256kx32/I_EMC/ADDR_CNTRMUX_I/ADDRCNT_I/gen_cry_kill_n<0>" is
loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_EMC/ADDR_CNTRMUX_I/ADDRCNT_I/MULT_AND_i10" (AND)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_ADDRESS_DECODER/MEM_SELECT_I2/MUX
CY_I0" (MUX) removed.
 The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt6"
is loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt6" (ROM)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_ADDRESS_DECODER/MEM_SELECT_I3/MUX
CY_I0" (MUX) removed.
 The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt5"
is loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt5" (ROM)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_ADDRESS_DECODER/MEM_SELECT_I4/MUX
CY_I0" (MUX) removed.
 The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt4"
is loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt4" (ROM)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_ADDRESS_DECODER/MEM_SELECT_I5/MUX
CY_I0" (MUX) removed.
 The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt3"
is loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt3" (ROM)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_ADDRESS_DECODER/MEM_SELECT_I6/MUX
CY_I0" (MUX) removed.
 The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt2"
is loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt2" (ROM)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_ADDRESS_DECODER/MEM_SELECT_I7/MUX
CY_I0" (MUX) removed.
 The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt1"
is loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt1" (ROM)
removed.
Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_ADDRESS_DECODER/MEM_SELECT_I8/MUX
CY_I0" (MUX) removed.
 The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt"
is loadless and has been removed.
  Loadless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Bus2IP_Addr_sa<11>_rt" (ROM)
removed.
The signal "opb_intc_0/opb_intc_0/INTC_CORE_I/INTR_DET_I/clear<1>" is sourceless
and has been removed.
The signal
"opb_intc_0/opb_intc_0/INTC_CORE_I/INTR_DET_I/DETECT_INTR_I/LVL_DET_BIT_I1/clk_e
nable" is sourceless and has been removed.
The signal "opb_intc_0/opb_intc_0/INTC_CORE_I/int_status<1>" is sourceless and
has been removed.
 Sourceless block
"opb_intc_0/opb_intc_0/INTC_CORE_I/INTR_DET_I/DETECT_INTR_I/LVL_DET_BIT_I1/clk_e
nable1" (ROM) removed.
The signal "opb_intc_0/N4481" is sourceless and has been removed.
The signal "opb_intc_0/opb_intc_0/INTC_CORE_I/int_ack<1>" is sourceless and has
been removed.
The signal
"opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/WR_REG_DECODE_I/Int_ack_en<0>1_SW2/O"
is sourceless and has been removed.
The signal "opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/Int_ack_i<1>1_SW1/O" is
sourceless and has been removed.
The signal "opb_intc_0/opb_intc_0/OPB_INTFC_I/_n00001/O" is sourceless and has
been removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<0>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<1>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<2>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<3>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<4>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<5>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<6>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<7>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<8>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<9>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<10>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<11>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<12>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<13>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<14>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<15>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<16>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<17>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<18>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<19>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<20>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<21>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<22>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<23>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<24>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<25>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<26>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<27>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<28>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<29>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<30>" is sourceless and has been
removed.
The signal "opb_bram_if_cntlr_1_bram/BRAM_Din_B<31>" is sourceless and has been
removed.
The signal "microblaze_0/microblaze_0/Decode_I/Use_Store_Instr_Addr" is
sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<31>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<0>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<30>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<1>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<0>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<31>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<1>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<30>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<2>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<29>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<3>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<28>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<4>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<27>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<5>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<26>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<6>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<25>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<7>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<24>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<8>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<23>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<9>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<22>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<10>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<21>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<11>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<20>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<12>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<19>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<13>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<18>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<14>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<17>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<15>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<16>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<16>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<15>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<17>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<14>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<18>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<13>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<19>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<12>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<20>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<11>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<21>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<10>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<22>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<9>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<23>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<8>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<24>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<7>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<25>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<6>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<26>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<5>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<27>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<4>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<28>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<3>" is sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Mmux_PC_EX_Result<29>1" (ROM)
removed.
  The signal "microblaze_0/PC_EX<2>" is sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<0>" is sourceless and
has been removed.
The signal "microblaze_0/Trace_AS" is sourceless and has been removed.
The signal "microblaze_0/Trace_Data_Write" is sourceless and has been removed.
The signal "microblaze_0/Trace_Data_Read" is sourceless and has been removed.
The signal "microblaze_0/Trace_Data_Address<31>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<30>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<29>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<28>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<27>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<26>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<25>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<24>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<23>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<22>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<21>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<20>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<19>" is sourceless and has been
removed.
The signal "microblaze_0/microblaze_0/Reg_Write_N9759" is sourceless and has
been removed.
 Sourceless block "microblaze_0/microblaze_0/Reg_Write" (SFF) removed.
  The signal "microblaze_0/REG_WRITE" is sourceless and has been removed.
The signal "microblaze_0/Trace_Data_Address<18>" is sourceless and has been
removed.
The signal "microblaze_0/REG_ADDR<0>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Data_Address<17>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<16>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<15>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<14>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<13>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<12>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<11>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<6>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<5>" is sourceless and has been
removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<1>" is sourceless and
has been removed.
The signal "microblaze_0/Trace_Data_Address<10>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<9>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<8>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<7>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<4>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<3>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<2>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<1>" is sourceless and has been
removed.
The signal "microblaze_0/Trace_Data_Address<0>" is sourceless and has been
removed.
The signal "microblaze_0/microblaze_0/Decode_I/Load_Store_Instr_Addr_Stored" is
sourceless and has been removed.
 Sourceless block "microblaze_0/microblaze_0/Decode_I/_n01061" (ROM) removed.
  The signal "microblaze_0/microblaze_0/Decode_I/_n0106" is sourceless and has
been removed.
   Sourceless block "microblaze_0/microblaze_0/Decode_I/Use_Store_Instr_Addr" (FF)
removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<31>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<30>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<29>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<28>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<27>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<26>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<25>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<24>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<23>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<22>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<21>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<20>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<19>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<18>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<17>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<16>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<15>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<14>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<13>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<12>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<11>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<10>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<9>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<8>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<7>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<6>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<5>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<4>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<3>" is sourceless and
has been removed.
The signal "microblaze_0/microblaze_0/Instr_Addr_Stored_1<2>" is sourceless and
has been removed.
The signal "microblaze_0/REG_ADDR<4>" is sourceless and has been removed.
The signal "microblaze_0/REG_ADDR<3>" is sourceless and has been removed.
The signal "microblaze_0/REG_ADDR<2>" is sourceless and has been removed.
The signal "microblaze_0/REG_ADDR<1>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<9>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<8>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<7>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<6>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<5>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<4>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<3>" is sourceless and has been removed.
The signal "microblaze_0/MSR_REG<2>" is sourceless and has been removed.
The signal "microblaze_0/PREFETCH_ADDR<3>" is sourceless and has been removed.
The signal "microblaze_0/PREFETCH_ADDR<2>" is sourceless and has been removed.
The signal "microblaze_0/PREFETCH_ADDR<1>" is sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Decode_I/_n0164" is sourceless and has
been removed.
 Sourceless block "microblaze_0/microblaze_0/Decode_I/Interrupt_Taken" (FF)
removed.
  The signal "microblaze_0/INTERRUPT_TAKEN" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<6>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<0>" is sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Decode_I/_n0155" is sourceless and has
been removed.
 Sourceless block "microblaze_0/microblaze_0/Decode_I/Branch_Instr" (FF) removed.
  The signal "microblaze_0/Trace_Branch_Instr" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<17>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<8>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<9>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<10>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<22>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<31>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<11>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<12>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<13>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<14>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<7>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<1>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<2>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<3>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<16>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<15>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<19>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<18>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<21>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<20>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<28>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<27>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<24>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<23>" is sourceless and has been removed.
The signal "microblaze_0/Trace_Instr_EX<29>" is sourceless and has been removed.
The signal "microblaze_0/MB_Halted" is sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Decode_I/Ker282611/O" is sourceless and
has been removed.
The signal
"microblaze_0/microblaze_0/Decode_I/PreFetch_Buffer_I/buffer_Addr_MUXCY_L1/LO"
is sourceless and has been removed.
The signal
"microblaze_0/microblaze_0/Decode_I/PreFetch_Buffer_I/buffer_Addr_MUXCY_L1/O" is
sourceless and has been removed.
 Sourceless block
"microblaze_0/microblaze_0/Decode_I/PreFetch_Buffer_I/buffer_Addr_MUXCY_L1/MUXCY
_L_BUF" (BUF) removed.
The signal "microblaze_0/microblaze_0/Iopb_Interface_I/request_Drop_In" is
sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Iopb_Interface_I/Iopb_Interrupt" is
sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Dopb_Interface_I/Dopb_Interrupt" is
sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Dopb_Interface_I/request_Drop_In" is
sourceless and has been removed.
The signal "microblaze_0/microblaze_0/Data_Flow_I/Exceptions_Enabled<0>" is
sourceless and has been removed.
The signal
"microblaze_0/microblaze_0/Data_Flow_I/PC_Module_I/PC_Bit_I0/Carry_Out" is
sourceless and has been removed.
The signal
"microblaze_0/microblaze_0/Data_Flow_I/PC_Module_I/PC_Bit_I0/MUXCY_X/O" is
sourceless and has been removed.
 Sourceless block
"microblaze_0/microblaze_0/Data_Flow_I/PC_Module_I/PC_Bit_I0/MUXCY_X/MUXCY_L_BUF
" (BUF) removed.
The signal "mb_opb/CHOICE107" is sourceless and has been removed.
 Sourceless block "mb_opb/mb_opb/OPB_dwAck_I/_n000913_SW0" (ROM) removed.
  The signal "mb_opb/N10447" is sourceless and has been removed.
   Sourceless block "mb_opb/mb_opb/OPB_dwAck_I/_n000913" (ROM) removed.
    The signal "mb_opb/OPB_dwAck" is sourceless and has been removed.
The signal "mb_opb/OPB_hwXfer" is sourceless and has been removed.
The signal "mb_opb/OPB_fwXfer" is sourceless and has been removed.
The signal "mb_opb/OPB_dwXfer" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<0>" is sourceless and has been removed.
The signal "mb_opb/OPB_beXfer" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<31>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<30>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<29>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<28>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<27>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<26>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<25>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<24>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<23>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<22>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<21>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<20>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<19>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<18>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<17>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<16>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<15>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<14>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<13>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<12>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<11>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<10>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<9>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<8>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<7>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<6>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<5>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<4>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<3>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<2>" is sourceless and has been removed.
The signal "mb_opb/OPB_wrDBus<1>" is sourceless and has been removed.
The signal "mb_opb/CHOICE115" is sourceless and has been removed.
 Sourceless block "mb_opb/mb_opb/OPB_beAck_I/_n000913_SW0" (ROM) removed.
  The signal "mb_opb/N10467" is sourceless and has been removed.
   Sourceless block "mb_opb/mb_opb/OPB_beAck_I/_n000913" (ROM) removed.
    The signal "mb_opb/OPB_beAck" is sourceless and has been removed.
The signal "mb_opb/CHOICE123" is sourceless and has been removed.
 Sourceless block "mb_opb/mb_opb/OPB_fwAck_I/_n000913_SW0" (ROM) removed.
  The signal "mb_opb/N10499" is sourceless and has been removed.
   Sourceless block "mb_opb/mb_opb/OPB_fwAck_I/_n000913" (ROM) removed.
    The signal "mb_opb/OPB_fwAck" is sourceless and has been removed.
The signal "mb_opb/CHOICE75" is sourceless and has been removed.
 Sourceless block "mb_opb/mb_opb/OPB_errAck_I/_n000913_SW0" (ROM) removed.
  The signal "mb_opb/N10507" is sourceless and has been removed.
   Sourceless block "mb_opb/mb_opb/OPB_errAck_I/_n000913" (ROM) removed.
    The signal "mb_opb_OPB_errAck" is sourceless and has been removed.
     Sourceless block "microblaze_0/microblaze_0/Iopb_Interface_I/IOPB_Interrupt_I"
(ROM) removed.
     Sourceless block "microblaze_0/microblaze_0/Dopb_Interface_I/DOPB_Interrupt_I"
(ROM) removed.
The signal "mb_opb/OPB_toutSup" is sourceless and has been removed.
The signal "mb_opb/CHOICE131" is sourceless and has been removed.
 Sourceless block "mb_opb/mb_opb/OPB_hwAck_I/_n000913_SW0" (ROM) removed.
  The signal "mb_opb/N10531" is sourceless and has been removed.
   Sourceless block "mb_opb/mb_opb/OPB_hwAck_I/_n000913" (ROM) removed.
    The signal "mb_opb/OPB_hwAck" is sourceless and has been removed.
The signal "debug_module/debug_module/drck1_i" is sourceless and has been
removed.
 Sourceless block "debug_module/debug_module/BUFG_DRCK1" (CKBUF) removed.
  The signal "debug_module/bscan_drck1" is sourceless and has been removed.
The signal "debug_module/bscan_reset" is sourceless and has been removed.
The signal "debug_module/bscan_sel1" is sourceless and has been removed.
The signal "debug_module/debug_module/MDM_Core_I1/tx_Buffer_Empty_Pre" is
sourceless and has been removed.
 Sourceless block "debug_module/debug_module/MDM_Core_I1/Interrupt1" (ROM)
removed.
  The signal "debug_module/Interrupt" is sourceless and has been removed.
The signal "debug_module/debug_module/MDM_Core_I1/status_Reg<5>" is sourceless
and has been removed.
 Sourceless block "debug_module/debug_module/MDM_Core_I1/TX_Buffer_Empty_FDRE"
(SFF) removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<2>" is sourceless and
has been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_qwen_reg_2"
(SFF) removed.
  The signal "sram_256kx32/Mem_QWEN<2>" is sourceless and has been removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<1>" is sourceless and
has been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_qwen_reg_1"
(SFF) removed.
  The signal "sram_256kx32/Mem_QWEN<1>" is sourceless and has been removed.
The signal
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_SLAVE_ATTACHMENT/_n0035" is
sourceless and has been removed.
 Sourceless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_SLAVE_ATTACHMENT/sln_errack_i"
(SFF) removed.
  The signal
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_SLAVE_ATTACHMENT/sln_errack_i" is
sourceless and has been removed.
   Sourceless block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_SLAVE_ATTACHMENT/Sln_errAck1"
(ROM) removed.
    The signal "mb_opb_Sl_errAck<3>" is sourceless and has been removed.
     Sourceless block "mb_opb/mb_opb/OPB_errAck_I/_n00098" (ROM) removed.
The signal "sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/Rst2Bus_Error" is
sourceless and has been removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_be_int<2>" is sourceless and has
been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<2>1" (ROM)
removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_be_int<1>" is sourceless and has
been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<1>1" (ROM)
removed.
The signal
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_SLAVE_ATTACHMENT/_n0034" is
sourceless and has been removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<3>" is sourceless and
has been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_qwen_reg_3"
(SFF) removed.
  The signal "sram_256kx32/Mem_QWEN<3>" is sourceless and has been removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_be_int<3>" is sourceless and has
been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<3>1" (ROM)
removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_be_int<0>" is sourceless and has
been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<0>1" (ROM)
removed.
  The signal "sram_256kx32/sram_256kx32/I_EMC/mem_qwen_int<0>" is sourceless and
has been removed.
   Sourceless block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_qwen_reg_0"
(SFF) removed.
    The signal "sram_256kx32/Mem_QWEN<0>" is sourceless and has been removed.
The signal "sram_256kx32/sram_256kx32/I_EMC/mem_rpn_int" is sourceless and has
been removed.
 Sourceless block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_rpn_reg"
(SFF) removed.
  The signal "sram_256kx32/Mem_RPN" is sourceless and has been removed.
The signal "sram_256kx32/Mem_RNW" is sourceless and has been removed.
The signal "sram_256kx32/Mem_CE<0>" is sourceless and has been removed.
The signal "push_buttons_3bit/GPIO_IO_T<2>" is sourceless and has been removed.

The trimmed logic reported below is either:
   1. part of a cycle
   2. part of disabled logic
   3. a side-effect of other trimmed logic

The signal "mb_opb_OPB_seqAddr" is unused and has been removed.
 Unused block "mb_opb/mb_opb/OPB_seqAddr_I/_n00021" (ROM) removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<11>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_11" (SFF)
removed.
The signal "dlmb_LMB_ABus<31>" is unused and has been removed.
 Unused block
"microblaze_0/microblaze_0/Byte_Doublet_Handle_I/LOW_ADDR_OUT_RIGHT_I" (ROM)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<10>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_10" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<9>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_9" (SFF)
removed.
The signal "dlmb_LMB_ABus<30>" is unused and has been removed.
 Unused block
"microblaze_0/microblaze_0/Byte_Doublet_Handle_I/LOW_ADDR_OUT_LEFT_I" (ROM)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<8>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_8" (SFF)
removed.
The signal "net_vcc9<8>" is unused and has been removed.
 Unused block "XST_VCC" (ONE) removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<7>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_7" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<6>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_6" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<5>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_5" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<4>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_4" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<3>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_3" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<2>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_2" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<1>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_1" (SFF)
removed.
The signal "fpga_0_SRAM_256Kx32_Mem_A_split<0>" is unused and has been removed.
 Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_a_reg_0" (SFF)
removed.
The signal "mb_opb_Sl_errAck<0>" is unused and has been removed.
 Unused block "opb_intc_0/opb_intc_0/OPB_INTFC_I/ERR_ACK_I" (SFF) removed.
Unused block
"debug_module/debug_module/MDM_Core_I1/JTAG_CONTROL_I/TX_Buffer_Empty1" (ROM)
removed.
Unused block "mb_opb/mb_opb/OPB_beAck_I/_n00098" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_beXfer_I/_n00021" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_dwAck_I/_n00098" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_dwXfer_I/_n00021" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_fwAck_I/_n00098" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_fwXfer_I/_n00021" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_hwAck_I/_n00098" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_hwXfer_I/_n00021" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_toutSup_I/_n000913" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00021" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00051" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00081" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00111" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00141" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00171" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00201" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00231" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00261" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00291" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00321" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00351" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00381" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00411" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00441" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00471" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00501" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00531" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00561" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00591" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00621" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00651" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00681" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00711" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00741" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00771" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00801" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00831" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00861" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00891" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00921" (ROM) removed.
Unused block "mb_opb/mb_opb/OPB_wrDBus_I/_n00951" (ROM) removed.
Unused block "microblaze_0/microblaze_0/Debug_I/MB_Halted" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_0" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_1" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_10" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_11" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_12" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_13" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_14" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_15" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_16" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_17" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_18" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_19" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_2" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_20" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_21" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_22" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_23" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_24" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_27" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_28" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_29" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_3" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_31" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_6" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_7" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_8" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Instr_EX_9" (FF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Ker282611" (ROM) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/Load_Store_Instr_Addr_Stored"
(SFF) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/_n01551" (ROM) removed.
Unused block "microblaze_0/microblaze_0/Decode_I/_n01641" (ROM) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_0" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_1" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_10" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_11" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_12" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_13" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_14" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_15" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_16" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_17" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_18" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_19" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_2" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_20" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_21" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_22" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_23" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_24" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_25" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_26" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_27" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_28" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_29" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_3" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_30" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_31" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_4" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_5" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_6" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_7" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_8" (FF) removed.
Unused block "microblaze_0/microblaze_0/Instr_Addr_Stored_1_9" (FF) removed.
Unused block "microblaze_0/microblaze_0/Prefetch_Addr_1" (FF) removed.
Unused block "microblaze_0/microblaze_0/Prefetch_Addr_2" (FF) removed.
Unused block "microblaze_0/microblaze_0/Prefetch_Addr_3" (FF) removed.
Unused block "microblaze_0/microblaze_0/Reg_Addr_0" (FF) removed.
Unused block "microblaze_0/microblaze_0/Reg_Addr_1" (FF) removed.
Unused block "microblaze_0/microblaze_0/Reg_Addr_2" (FF) removed.
Unused block "microblaze_0/microblaze_0/Reg_Addr_3" (FF) removed.
Unused block "microblaze_0/microblaze_0/Reg_Addr_4" (FF) removed.
Unused block "microblaze_0/microblaze_0/Reg_Write_Sclr_INV1" (ROM) removed.
Unused block "microblaze_0/microblaze_0/Trace_AS" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_0" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_1" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_10" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_11" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_12" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_13" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_14" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_15" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_16" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_17" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_18" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_19" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_2" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_20" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_21" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_22" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_23" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_24" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_25" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_26" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_27" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_28" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_29" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_3" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_30" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_31" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_4" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_5" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_6" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_7" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_8" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Address_9" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Read" (FF) removed.
Unused block "microblaze_0/microblaze_0/Trace_Data_Write" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_2" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_3" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_4" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_5" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_6" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_7" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_8" (FF) removed.
Unused block "microblaze_0/microblaze_0/msr_2_9" (FF) removed.
Unused block "opb_intc_0/opb_intc_0/INTC_CORE_I/INTR_DET_I/clear<1>1" (ROM)
removed.
Unused block "opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/Int_ack_i<1>1" (ROM)
removed.
Unused block "opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/Int_ack_i<1>1_SW1" (ROM)
removed.
Unused block
"opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/WR_REG_DECODE_I/Int_ack_en<0>1_SW2"
(ROM) removed.
Unused block
"opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/WR_REG_DECODE_I/Int_ack_en<0>1_SW5"
(ROM) removed.
Unused block "opb_intc_0/opb_intc_0/OPB_INTFC_I/_n00001" (ROM) removed.
Unused block "push_buttons_3bit/XST_VCC" (ONE) removed.
Unused block "sram_256kx32/sram_256kx32/I_EMC/DATA_PATH_I/_n02981" (ROM)
removed.
Unused block "sram_256kx32/sram_256kx32/I_EMC/DATA_PATH_I/_n03011" (ROM)
removed.
Unused block "sram_256kx32/sram_256kx32/I_EMC/DATA_PATH_I/_n03421" (ROM)
removed.
Unused block "sram_256kx32/sram_256kx32/I_EMC/DATA_PATH_I/_n03431" (ROM)
removed.
Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_ce_reg_0" (SFF)
removed.
Unused block "sram_256kx32/sram_256kx32/I_EMC/IO_REGISTERS_I/mem_rnw_reg" (SFF)
removed.
Unused block "sram_256kx32/sram_256kx32/I_EMC/mem_rpn_int1" (ROM) removed.
Unused block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_RESET_CONTROL/I_RESET_CONTROLLER/
Reset_Error1" (ROM) removed.
Unused block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_SLAVE_ATTACHMENT/_n00341" (ROM)
removed.
Unused block
"sram_256kx32/sram_256kx32/I_OPB_IPIf/IPIF_I/I_SLAVE_ATTACHMENT/_n00351" (ROM)
removed.
Unused block
"microblaze_0/microblaze_0/Data_Flow_I/PC_Module_I/PC_Bit_I0/MUXCY_X" (MUX)
removed.
Unused block
"microblaze_0/microblaze_0/Decode_I/PreFetch_Buffer_I/buffer_Addr_MUXCY_L1"
(MUX) removed.

Optimized Block(s):
TYPE 		BLOCK
GND 		XST_GND
GND 		debug_module/XST_GND
VCC 		debug_module/XST_VCC
GND 		dlmb/XST_GND
VCC 		dlmb/XST_VCC
GND 		dlmb_cntlr/XST_GND
VCC 		dlmb_cntlr/XST_VCC
GND 		ilmb/XST_GND
VCC 		ilmb/XST_VCC
GND 		ilmb_cntlr/XST_GND
VCC 		ilmb_cntlr/XST_VCC
LUT3 		ilmb_cntlr/ilmb_cntlr/_n00021
LUT3 		ilmb_cntlr/ilmb_cntlr/_n00041
LUT3 		ilmb_cntlr/ilmb_cntlr/_n00061
LUT3 		ilmb_cntlr/ilmb_cntlr/_n00081
GND 		led_anodes/XST_GND
FD 		led_anodes/led_anodes/gpio_core_1/gpio_Data_In_0
   optimized to 0
FD 		led_anodes/led_anodes/gpio_core_1/gpio_Data_In_1
   optimized to 0
FD 		led_anodes/led_anodes/gpio_core_1/gpio_Data_In_2
   optimized to 0
FD 		led_anodes/led_anodes/gpio_core_1/gpio_Data_In_3
   optimized to 0
GND 		led_cathodes/XST_GND
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_0
   optimized to 0
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_1
   optimized to 0
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_2
   optimized to 0
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_3
   optimized to 0
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_4
   optimized to 0
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_5
   optimized to 0
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_6
   optimized to 0
FD 		led_cathodes/led_cathodes/gpio_core_1/gpio_Data_In_7
   optimized to 0
GND 		leds_8bit/XST_GND
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_0
   optimized to 0
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_1
   optimized to 0
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_2
   optimized to 0
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_3
   optimized to 0
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_4
   optimized to 0
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_5
   optimized to 0
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_6
   optimized to 0
FD 		leds_8bit/leds_8bit/gpio_core_1/gpio_Data_In_7
   optimized to 0
GND 		lmb_bram/lmb_bram/XST_GND
GND 		mb_opb/XST_GND
VCC 		mb_opb/XST_VCC
LUT4 		mb_opb/mb_opb/OPB_rdDBus_I/_n00794
LUT4 		mb_opb/mb_opb/OPB_rdDBus_I/_n01494
LUT4 		mb_opb/mb_opb/OPB_rdDBus_I/_n01594
LUT4 		mb_opb/mb_opb/OPB_retry_I/_n000913
LUT4 		mb_opb/mb_opb/OPB_retry_I/_n000913_SW0
LUT3 		mb_opb/mb_opb/OPB_retry_I/_n00098
LUT4 		mb_opb/mb_opb/OPB_toutSup_I/_n00094
GND 		microblaze_0/XST_GND
VCC 		microblaze_0/XST_VCC
GND 		microblaze_0/microblaze_0/Data_Flow_I/MSR_Reg_I/XST_GND
GND 		microblaze_0/microblaze_0/Data_Flow_I/MUL_Unit_I/XST_GND
VCC 		microblaze_0/microblaze_0/Data_Flow_I/MUL_Unit_I/XST_VCC
VCC 		microblaze_0/microblaze_0/Data_Flow_I/Operand_Select_I/XST_VCC
GND 		microblaze_0/microblaze_0/Data_Flow_I/PC_Module_I/XST_GND
VCC 		microblaze_0/microblaze_0/Data_Flow_I/Result_Mux_I/XST_VCC
GND 		microblaze_0/microblaze_0/Data_Flow_I/Shift_Logic_Module_I/XST_GND
GND 		microblaze_0/microblaze_0/Data_Flow_I/Zero_Detect_I/XST_GND
VCC 		microblaze_0/microblaze_0/Data_Flow_I/Zero_Detect_I/XST_VCC
FDR 		microblaze_0/microblaze_0/Dopb_Interface_I/Request_Drop_I
   optimized to 0
LUT2 		microblaze_0/microblaze_0/Dopb_Interface_I/Request_Drop_In_I
GND 		microblaze_0/microblaze_0/Dopb_Interface_I/XST_GND
VCC 		microblaze_0/microblaze_0/Dopb_Interface_I/XST_VCC
FDR 		microblaze_0/microblaze_0/Iopb_Interface_I/Request_Drop_I
   optimized to 0
LUT2 		microblaze_0/microblaze_0/Iopb_Interface_I/Request_Drop_In_I
GND 		microblaze_0/microblaze_0/Iopb_Interface_I/XST_GND
VCC 		microblaze_0/microblaze_0/Iopb_Interface_I/XST_VCC
LUT1 		microblaze_0/microblaze_0/Iopb_Interface_I/request_Drop_N1
GND 		opb_bram_if_cntlr_1/XST_GND
GND 		opb_bram_if_cntlr_1_bram/opb_bram_if_cntlr_1_bram/XST_GND
GND 		opb_intc_0/XST_GND
VCC 		opb_intc_0/XST_VCC
FDRE
		opb_intc_0/opb_intc_0/INTC_CORE_I/INTR_DET_I/DETECT_INTR_I/LVL_DET_BIT_I1/ACTI
VE_HIGH_LVL_I
   optimized to 0
FDR 		opb_intc_0/opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I1
   optimized to 0
FDR 		opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/ISR_REG_BIT_I1
   optimized to 0
FDR 		opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I1
   optimized to 0
LUT4_L
		opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/RD_REG_MUX_I/Mmux_Bus_out_inst_lut3_4
1
LOCALBUF
		opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/RD_REG_MUX_I/Mmux_Bus_out_inst_lut3_4
1/LUT4_L_BUF
LUT4 		opb_intc_0/opb_intc_0/INTC_CORE_I/REGS_I/rd_reg_sel<0>1_SW4
GND 		push_buttons_3bit/XST_GND
GND 		rs232/XST_GND
VCC 		rs232/XST_VCC
GND 		sram_256kx32/XST_GND
VCC 		sram_256kx32/XST_VCC

To enable printing of redundant blocks removed and signals merged, set the
detailed map report option and rerun map.

Section 6 - IOB Properties
--------------------------

+------------------------------------------------------------------------------------------------------------------------+
| IOB Name                           | Type    | Direction | IO Standard | Drive    | Slew | Reg (s)  | Resistor | IOB   |
|                                    |         |           |             | Strength | Rate |          |          | Delay |
+------------------------------------------------------------------------------------------------------------------------+
| anode<0>                           | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| anode<1>                           | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| anode<2>                           | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| anode<3>                           | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<0>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<1>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<2>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<3>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<4>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<5>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<6>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| cathode<7>                         | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<0> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<1> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<2> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<3> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<4> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<5> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<6> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin<7> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_Push_Buttons_3Bit_GPIO_in_p | IOB     | INPUT     | LVCMOS25    |          |      | INFF1    |          | IFD   |
| in<0>                              |         |           |             |          |      |          |          |       |
| fpga_0_Push_Buttons_3Bit_GPIO_in_p | IOB     | INPUT     | LVCMOS25    |          |      | INFF1    |          | IFD   |
| in<1>                              |         |           |             |          |      |          |          |       |
| fpga_0_Push_Buttons_3Bit_GPIO_in_p | IOB     | INPUT     | LVCMOS25    |          |      | INFF1    |          | IFD   |
| in<2>                              |         |           |             |          |      |          |          |       |
| fpga_0_RS232_RX_pin                | IOB     | INPUT     | LVCMOS25    |          |      | INFF1    |          | IFD   |
| fpga_0_RS232_TX_pin                | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<12>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<13>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<14>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<15>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<16>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<17>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<18>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<19>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<20>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<21>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<22>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<23>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<24>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<25>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<26>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<27>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<28>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_A_pin<29>  | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_BEN_pin<0> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_BEN_pin<1> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_BEN_pin<2> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_BEN_pin<3> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_CEN_1_pin< | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW |          |          |       |
| 0>                                 |         |           |             |          |      |          |          |       |
| fpga_0_SRAM_256Kx32_Mem_CEN_pin<0> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW |          |          |       |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<0>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<1>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<2>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<3>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<4>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<5>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<6>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<7>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<8>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<9>  | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<10> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<11> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<12> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<13> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<14> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<15> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<16> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<17> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<18> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<19> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<20> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<21> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<22> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<23> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<24> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<25> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<26> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<27> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<28> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<29> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<30> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_DQ_pin<31> | IOB     | BIDIR     | LVCMOS25    | 12       | SLOW | INFF1    |          | IFD   |
| fpga_0_SRAM_256Kx32_Mem_OEN_pin<0> | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| fpga_0_SRAM_256Kx32_Mem_WEN_pin    | IOB     | OUTPUT    | LVCMOS25    | 12       | SLOW | OFF1     |          |       |
| sys_clk_pin                        | IOB     | INPUT     | LVCMOS25    |          |      |          |          |       |
| sys_rst_pin                        | IOB     | INPUT     | LVCMOS25    |          |      |          |          |       |
+------------------------------------------------------------------------------------------------------------------------+

Section 7 - RPMs
----------------
microblaze_0_write_address_hit00        
microblaze_0_read_address_hit00         
microblaze_0_address_hit01              
microblaze_0_address_hit00              
microblaze_0                            

Section 8 - Guide Report
------------------------
Guide not run on this design.

Section 9 - Area Group Summary
------------------------------
No area groups were found in this design.

Section 10 - Modular Design Summary
-----------------------------------
Modular Design not used for this design.

Section 11 - Timing Report
--------------------------
This design was not run using timing mode.

Section 12 - Configuration String Details
-----------------------------------------
Use the "-detail" map option to print out Configuration Strings

Section 13 - Additional Device Resource Counts
----------------------------------------------
Number of JTAG Gates for IOBs = 85
Number of Equivalent Gates for Design = 589,067
Number of RPM Macros = 5
Number of Hard Macros = 0
DCIRESETs = 0
CAPTUREs = 0
BSCANs = 1
STARTUPs = 0
DCMs = 0
GCLKs = 2
ICAPs = 0
18X18 Multipliers = 3
Block RAMs = 8
Total Registers (Flops & Latches in Slices & IOBs) not driven by LUTs = 682
IOB Dual-Rate Flops not driven by LUTs = 0
IOB Dual-Rate Flops = 0
IOB Slave Pads = 0
IOB Master Pads = 0
IOB Latches not driven by LUTs = 0
IOB Latches = 0
IOB Flip Flops not driven by LUTs = 75
IOB Flip Flops = 81
Unbonded IOBs = 0
Bonded IOBs = 85
Shift Registers = 161
Static Shift Registers = 6
Dynamic Shift Registers = 155
16x1 ROMs = 0
16x1 RAMs = 0
32x1 RAMs = 0
Dual Port RAMs = 128
MUXFXs = 183
MULTANDs = 33
4 input LUTs used as Route-Thrus = 44
4 input LUTs = 1859
Slice Latches not driven by LUTs = 0
Slice Latches = 0
Slice Flip Flops not driven by LUTs = 607
Slice Flip Flops = 1536
SliceMs = 321
SliceLs = 1274
Slices = 1595
Multiplier(16,16) = 1
Multiplier(18,16) = _0_SRAM_256Kx32_Mem_OEN_pin<0>
Number of LUT signals with 4 loads = 63
Number of LUT signals with 3 loads = 51
Number of LUT signals with 2 loads = 349
Number of LUT signals with 1 load = 1241
NGM Average fanout of LUT = 2.68
NGM Maximum fanout of LUT = 128
NGM Average fanin for LUT = 3.2539
Number of LUT symbols = 1859
Number of IPAD symbols = 6
Number of IBUF symbols = 38
Number of BSCAN_VIRTEX2 symbols = 1
Number of BIPAD symbols = 32
