Release 6.3i - xst G.38
Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.
--> 
TABLE OF CONTENTS
  1) Synthesis Options Summary
  2) HDL Compilation
  3) HDL Analysis
  4) HDL Synthesis
  5) Advanced HDL Synthesis
     5.1) HDL Synthesis Report
  6) Low Level Synthesis
  7) Final Report
     7.1) Device utilization summary
     7.2) TIMING REPORT


=========================================================================
*                      Synthesis Options Summary                        *
=========================================================================
---- Source Parameters
Input Format                       : MIXED
Input File Name                    : opb_intc_0_wrapper_xst.prj

---- Target Parameters
Target Device                      : xc3s400ft256-4
Output File Name                   : ../implementation/opb_intc_0_wrapper/opb_intc_0_wrapper.ngc

---- Source Options
Top Module Name                    : opb_intc_0_wrapper

---- Target Options
Add IO Buffers                     : NO

---- General Options
Optimization Effort                : 2
Optimization Goal                  : speed
RTL Output                         : YES
Hierarchy Separator                : /

=========================================================================


=========================================================================
*                          HDL Compilation                              *
=========================================================================
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/intc_pkg.vhd in Library intc_core_v1_00_c.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/kind_of_edge.vhd in Library intc_core_v1_00_c.
Entity <kind_of_edge> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/bus_mux_le.vhd in Library intc_core_v1_00_c.
Entity <bus_mux_le> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/edge_det_bit.vhd in Library intc_core_v1_00_c.
Entity <edge_det_bit> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/lvl_det_bit.vhd in Library intc_core_v1_00_c.
Entity <lvl_det_bit> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/or_muxcy.vhd in Library proc_common_v1_00_a.
Entity <or_muxcy> (Architecture <implementation>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/proc_common_pkg.vhd in Library proc_common_v1_00_a.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/wr_reg_decode.vhd in Library intc_core_v1_00_c.
Entity <wr_reg_decode> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/ier_logic.vhd in Library intc_core_v1_00_c.
Entity <ier_logic> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/mer_reg.vhd in Library intc_core_v1_00_c.
Entity <mer_reg> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/opt_regs.vhd in Library intc_core_v1_00_c.
Entity <opt_regs> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/detect_intr.vhd in Library intc_core_v1_00_c.
Entity <detect_intr> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/pulse_gen.vhd in Library intc_core_v1_00_c.
Entity <pulse_gen> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/or_gate.vhd in Library proc_common_v1_00_a.
Entity <or_gate> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/common_types_pkg.vhd in Library proc_common_v1_00_a.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd in Library proc_common_v1_00_a.
Entity <pselect> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/irq_gen.vhd in Library intc_core_v1_00_c.
Entity <irq_gen> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/int_det.vhd in Library intc_core_v1_00_c.
Entity <int_det> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd in Library intc_core_v1_00_c.
Entity <regs> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/intc_core.vhd in Library intc_core_v1_00_c.
Entity <intc_core> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd in Library opb_intc_v1_00_c.
Entity <opb_intfc> (Architecture <imp>) compiled.
Compiling vhdl file C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intc.vhd in Library opb_intc_v1_00_c.
Entity <opb_intc> (Architecture <imp>) compiled.
Compiling vhdl file C:/edk_user_repository/lab1/synthesis/../hdl/opb_intc_0_wrapper.vhd in Library work.
Entity <opb_intc_0_wrapper> (Architecture <STRUCTURE>) compiled.

=========================================================================
*                            HDL Analysis                               *
=========================================================================
Analyzing Entity <opb_intc_0_wrapper> (Architecture <STRUCTURE>).
Instantiating component <opb_intc> from Library <opb_intc_v1_00_c>.
Entity <opb_intc_0_wrapper> analyzed. Unit <opb_intc_0_wrapper> generated.

Analyzing generic Entity <opb_intc> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_OPB_AWIDTH = 32
	C_OPB_DWIDTH = 32
	C_BASEADDR = <u>10000000001000000000000100000000
	C_HIGHADDR = <u>10000000001000000000000111111111
	C_NUM_INTR_INPUTS = 1
	C_KIND_OF_INTR = <u>00000000000000000000000000000001
	C_KIND_OF_EDGE = <u>00000000000000000000000000000001
	C_KIND_OF_LVL = <u>00000000000000000000000000000000
	C_HAS_IPR = 1
	C_HAS_SIE = 1
	C_HAS_CIE = 1
	C_HAS_IVR = 1
	C_IRQ_IS_LEVEL = 1
	C_IRQ_ACTIVE = <u>1
Instantiating component <intc_core> from Library <intc_core_v1_00_c>.
Entity <opb_intc> analyzed. Unit <opb_intc> generated.

Analyzing generic Entity <intc_core> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_DWIDTH = 32
	C_NUM_INTR_INPUTS = 1
	C_KIND_OF_INTR = <u>00000000000000000000000000000001
	C_KIND_OF_EDGE = <u>00000000000000000000000000000001
	C_KIND_OF_LVL = <u>00000000000000000000000000000000
	C_HAS_IPR = <u>1
	C_HAS_SIE = <u>1
	C_HAS_CIE = <u>1
	C_HAS_IVR = <u>1
	C_IRQ_IS_LEVEL = <u>1
	C_IRQ_ACTIVE = <u>1
Entity <intc_core> analyzed. Unit <intc_core> generated.

Analyzing generic Entity <irq_gen> (Architecture <imp>).
	C_INT_ACTIVE = <u>1
	C_ACK_ACTIVE = <u>1
	C_IRQ_ACTIVE = <u>1
	C_IRQ_IS_LEVEL = <u>1
	C_NUM_INTS = 2
Instantiating component <or_gate> from Library <proc_common_v1_00_a>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/irq_gen.vhd line 216: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/irq_gen.vhd line 216: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/irq_gen.vhd line 226: Generating a Black Box for component <fdr>.
Instantiating component <or_gate> from Library <proc_common_v1_00_a>.
Entity <irq_gen> analyzed. Unit <irq_gen> generated.

Analyzing generic Entity <pulse_gen> (Architecture <imp>).
	C_TRIG_ACTIVE = <u>1
	C_ACK_ACTIVE = <u>1
	C_OUT_ACTIVE = <u>1
	C_ACK_ENDS_PLS = <u>1
Entity <pulse_gen> analyzed. Unit <pulse_gen> generated.

Analyzing generic Entity <or_gate> (Architecture <imp>).
	C_OR_WIDTH = 2
	C_BUS_WIDTH = 1
	C_USE_LUT_OR = <u>1
Entity <or_gate> analyzed. Unit <or_gate> generated.

Analyzing generic Entity <int_det> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_NUM_INTS = 2
	C_KIND_OF_INTR = <u>00000000000000000000000000000001
	C_KIND_OF_EDGE = <u>00000000000000000000000000000001
	C_KIND_OF_LVL = <u>00000000000000000000000000000010
Entity <int_det> analyzed. Unit <int_det> generated.

Analyzing generic Entity <detect_intr> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_NUM_INTS = 2
	C_KIND_OF_INTR = <u>00000000000000000000000000000001
	C_KIND_OF_EDGE = <u>00000000000000000000000000000001
	C_KIND_OF_LVL = <u>00000000000000000000000000000010
Entity <detect_intr> analyzed. Unit <detect_intr> generated.

Analyzing generic Entity <edge_det_bit> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_EDGE_POLARITY = <u>1
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/edge_det_bit.vhd line 147: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/edge_det_bit.vhd line 155: Generating a Black Box for component <fdr>.
Entity <edge_det_bit> analyzed. Unit <edge_det_bit> generated.

Analyzing generic Entity <kind_of_edge> (Architecture <imp>).
	C_KIND_OF_EDGE = <u>1
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/kind_of_edge.vhd line 134: Generating a Black Box for component <fdc>.
Entity <kind_of_edge> analyzed. Unit <kind_of_edge> generated.

Analyzing generic Entity <lvl_det_bit> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_LVL_POLARITY = <u>1
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/lvl_det_bit.vhd line 138: Generating a Black Box for component <fdre>.
Entity <lvl_det_bit> analyzed. Unit <lvl_det_bit> generated.

Analyzing generic Entity <regs> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_DWIDTH = 32
	C_HAS_IPR = <u>1
	C_HAS_SIE = <u>1
	C_HAS_CIE = <u>1
	C_HAS_IVR = <u>1
	C_RWIDTH = 2
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd line 285: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd line 285: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd line 299: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd line 299: Generating a Black Box for component <fdre>.
WARNING:Xst:1542 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd line 324: No default binding for component: <wr_reg_decode>. Generic <C_HAS_SIE> is not on the component.
WARNING:Xst:1542 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd line 324: No default binding for component: <wr_reg_decode>. Generic <C_HAS_CIE> is not on the component.
Entity <regs> analyzed. Unit <regs> generated.

Analyzing generic Entity <bus_mux_le> (Architecture <imp>).
	C_W = 2
	C_SW = 3
	C_N = 8
Entity <bus_mux_le> analyzed. Unit <bus_mux_le> generated.

Analyzing generic Entity <wr_reg_decode> (Architecture <imp>).
	C_WIDTH = 2
INFO:Xst:1561 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/wr_reg_decode.vhd line 161: Mux is complete : default of case is discarded
Entity <wr_reg_decode> analyzed. Unit <wr_reg_decode> generated.

Analyzing generic Entity <ier_logic> (Architecture <imp>).
	C_WIDTH = 2
	C_HAS_SIE = <u>1
	C_HAS_CIE = <u>1
	C_SEL_WIDTH = 2
Entity <ier_logic> analyzed. Unit <ier_logic> generated.

Analyzing generic Entity <bus_mux_le> (Architecture <imp>).
	C_W = 2
	C_SW = 2
	C_N = 3
Entity <bus_mux_le> analyzed. Unit <bus_mux_le0> generated.

Analyzing generic Entity <mer_reg> (Architecture <imp>).
	C_WIDTH = 2
WARNING:Xst:1994 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/mer_reg.vhd line 119: Null range in type of signal <upper_bits>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/mer_reg.vhd line 125: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/mer_reg.vhd line 135: Generating a Black Box for component <fdre>.
WARNING:Xst:1995 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/mer_reg.vhd line 145: Use of null array on signal <upper_bits> is not supported.
WARNING:Xst:1995 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/mer_reg.vhd line 147: Use of null array on signal <upper_bits> is not supported.
Entity <mer_reg> analyzed. Unit <mer_reg> generated.

Analyzing generic Entity <opt_regs> (Architecture <imp>).
	C_WIDTH = 2
	C_HAS_IPR = <u>1
	C_HAS_IVR = <u>1
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/opt_regs.vhd line 149: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/opt_regs.vhd line 149: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/opt_regs.vhd line 198: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/opt_regs.vhd line 198: Generating a Black Box for component <fdr>.
Entity <opt_regs> analyzed. Unit <opt_regs> generated.

Analyzing generic Entity <opb_intfc> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_Y = 0
	C_X = 0
	C_U_SET = "intc"
	C_INTC_BASEADDR = <u>10000000001000000000000100000000
	C_BASE_NUM_BITS = 24
	C_OPB_AWIDTH = 32
	C_OPB_DWIDTH = 32
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 210: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 223: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 236: Generating a Black Box for component <fdre>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 247: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 256: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 265: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 277: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 277: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 277: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 277: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 287: Generating a Black Box for component <fdr>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd line 296: Generating a Black Box for component <fdr>.
Instantiating component <pselect> from Library <proc_common_v1_00_a>.
Entity <opb_intfc> analyzed. Unit <opb_intfc> generated.

Analyzing generic Entity <pselect> (Architecture <imp>).
	C_AB = 24
	C_AW = 32
	C_BAR = <u>10000000001000000000000100000000
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd line 225: Generating a Black Box for component <MUXCY>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd line 225: Generating a Black Box for component <MUXCY>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd line 225: Generating a Black Box for component <MUXCY>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd line 225: Generating a Black Box for component <MUXCY>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd line 225: Generating a Black Box for component <MUXCY>.
WARNING:Xst:766 - C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd line 225: Generating a Black Box for component <MUXCY>.
Entity <pselect> analyzed. Unit <pselect> generated.


=========================================================================
*                           HDL Synthesis                               *
=========================================================================

Synthesizing Unit <pselect>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/pselect.vhd.
WARNING:Xst:647 - Input <A<24:31>> is never used.
WARNING:Xst:646 - Signal <bar_4> is assigned but never used.
Unit <pselect> synthesized.


Synthesizing Unit <bus_mux_le0>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/bus_mux_le.vhd.
    Found 2-bit 4-to-1 multiplexer for signal <Bus_out>.
    Summary:
	inferred   2 Multiplexer(s).
Unit <bus_mux_le0> synthesized.


Synthesizing Unit <opt_regs>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/opt_regs.vhd.
Unit <opt_regs> synthesized.


Synthesizing Unit <mer_reg>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/mer_reg.vhd.
WARNING:Xst:1780 - Signal <upper_bits> is never used or assigned.
Unit <mer_reg> synthesized.


Synthesizing Unit <ier_logic>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/ier_logic.vhd.
Unit <ier_logic> synthesized.


Synthesizing Unit <wr_reg_decode>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/wr_reg_decode.vhd.
Unit <wr_reg_decode> synthesized.


Synthesizing Unit <bus_mux_le>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/bus_mux_le.vhd.
    Found 2-bit 8-to-1 multiplexer for signal <Bus_out>.
    Summary:
	inferred   2 Multiplexer(s).
Unit <bus_mux_le> synthesized.


Synthesizing Unit <kind_of_edge>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/kind_of_edge.vhd.
Unit <kind_of_edge> synthesized.


Synthesizing Unit <lvl_det_bit>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/lvl_det_bit.vhd.
Unit <lvl_det_bit> synthesized.


Synthesizing Unit <edge_det_bit>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/edge_det_bit.vhd.
Unit <edge_det_bit> synthesized.


Synthesizing Unit <detect_intr>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/detect_intr.vhd.
Unit <detect_intr> synthesized.


Synthesizing Unit <or_gate>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/proc_common_v1_00_a/hdl/vhdl/or_gate.vhd.
WARNING:Xst:1780 - Signal <test> is never used or assigned.
Unit <or_gate> synthesized.


Synthesizing Unit <pulse_gen>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/pulse_gen.vhd.
    Found 4-bit register for signal <current>.
    Summary:
	inferred   4 D-type flip-flop(s).
Unit <pulse_gen> synthesized.


Synthesizing Unit <regs>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/regs.vhd.
WARNING:Xst:647 - Input <Wr_data<31:2>> is never used.
Unit <regs> synthesized.


Synthesizing Unit <int_det>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/int_det.vhd.
    Found 2 1-bit 2-to-1 multiplexers.
    Summary:
	inferred   2 Multiplexer(s).
Unit <int_det> synthesized.


Synthesizing Unit <irq_gen>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/irq_gen.vhd.
Unit <irq_gen> synthesized.


Synthesizing Unit <opb_intfc>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intfc.vhd.
WARNING:Xst:647 - Input <OPB_seqAddr> is never used.
Unit <opb_intfc> synthesized.


Synthesizing Unit <intc_core>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/intc_core_v1_00_c/hdl/vhdl/intc_core.vhd.
WARNING:Xst:646 - Signal <int_enables<1>> is assigned but never used.
WARNING:Xst:646 - Signal <clr_int> is assigned but never used.
WARNING:Xst:646 - Signal <sw_ints<1>> is assigned but never used.
Unit <intc_core> synthesized.


Synthesizing Unit <opb_intc>.
    Related source file is C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_intc_v1_00_c/hdl/vhdl/opb_intc.vhd.
Unit <opb_intc> synthesized.


Synthesizing Unit <opb_intc_0_wrapper>.
    Related source file is C:/edk_user_repository/lab1/synthesis/../hdl/opb_intc_0_wrapper.vhd.
Unit <opb_intc_0_wrapper> synthesized.


=========================================================================
*                       Advanced HDL Synthesis                          *
=========================================================================

Advanced RAM inference ...
Advanced multiplier inference ...
Advanced Registered AddSub inference ...
Dynamic shift register inference ...

=========================================================================
HDL Synthesis Report

Macro Statistics
# Registers                        : 4
 1-bit register                    : 4
# Multiplexers                     : 3
 2-bit 2-to-1 multiplexer          : 1
 2-bit 8-to-1 multiplexer          : 1
 2-bit 4-to-1 multiplexer          : 1

=========================================================================

=========================================================================
*                         Low Level Synthesis                           *
=========================================================================

Optimizing unit <opb_intc_0_wrapper> ...

Optimizing unit <wr_reg_decode> ...

Optimizing unit <pulse_gen> ...
WARNING:Xst:1710 - FF/Latch  <current_1> (without init value) is constant in block <pulse_gen>.

Optimizing unit <pselect> ...

Optimizing unit <opb_intfc> ...

Optimizing unit <irq_gen> ...

Optimizing unit <regs> ...

Optimizing unit <int_det> ...
Loading device for application Xst from file '3s400.nph' in environment C:/Xilinx.

Mapping all equations...
WARNING:Xst:1710 - FF/Latch  <current_1> (without init value) is constant in block <pulse_gen>.
Building and optimizing final netlist ...
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I0 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I0 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I0 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I25
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I29
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I28
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I27
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I2
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I3
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I4
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I5
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I6
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I7
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I8
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I9
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I10
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I11
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I12
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I13
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I14
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I15
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I16
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I17
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I18
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I19
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I20
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I21
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I22
WARNING:Xst:382 - Register opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I24 is equivalent to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I23
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I1
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IPR_REG_BIT_I0 is equivalent to opb_intc_0/INTC_CORE_I/IRQ_GEN_I/MASKED_INTS_REG_BIT_I0
WARNING:Xst:382 - Register opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I1 is equivalent to opb_intc_0/INTC_CORE_I/REGS_I/OPT_REGS_I/IVR_REG_BIT_I0

=========================================================================
*                            Final Report                               *
=========================================================================
Final Results
RTL Top Level Output File Name     : ../implementation/opb_intc_0_wrapper/opb_intc_0_wrapper.ngr
Top Level Output File Name         : ../implementation/opb_intc_0_wrapper/opb_intc_0_wrapper.ngc
Output Format                      : ngc
Optimization Goal                  : speed
Keep Hierarchy                     : no

Design Statistics
# IOs                              : 111

Macro Statistics :
# Registers                        : 4
#      1-bit register              : 4
# Multiplexers                     : 3
#      2-bit 4-to-1 multiplexer    : 1
#      2-bit 8-to-1 multiplexer    : 1
#      2-to-1 multiplexer          : 1

Cell Usage :
# BELS                             : 89
#      GND                         : 1
#      LUT1                        : 1
#      LUT2                        : 6
#      LUT2_L                      : 1
#      LUT3                        : 14
#      LUT3_D                      : 1
#      LUT3_L                      : 4
#      LUT4                        : 24
#      LUT4_D                      : 6
#      LUT4_L                      : 18
#      MUXCY                       : 6
#      MUXF5                       : 4
#      MUXF6                       : 2
#      VCC                         : 1
# FlipFlops/Latches                : 125
#      FDC                         : 1
#      FDR                         : 86
#      FDRE                        : 37
#      FDS                         : 1
=========================================================================

Device utilization summary:
---------------------------

Selected Device : 3s400ft256-4 

 Number of Slices:                      91  out of   3584     2%  
 Number of Slice Flip Flops:           125  out of   7168     1%  
 Number of 4 input LUTs:                75  out of   7168     1%  


=========================================================================
TIMING REPORT

NOTE: THESE TIMING NUMBERS ARE ONLY A SYNTHESIS ESTIMATE.
      FOR ACCURATE TIMING INFORMATION PLEASE REFER TO THE TRACE REPORT
      GENERATED AFTER PLACE-and-ROUTE.

Clock Information:
------------------
-----------------------------------+------------------------+-------+
Clock Signal                       | Clock buffer(FF name)  | Load  |
-----------------------------------+------------------------+-------+
OPB_Clk                            | NONE                   | 124   |
opb_intc_0/INTC_CORE_I/INTR_DET_I/interrupts<0>(opb_intc_0/INTC_CORE_I/INTR_DET_I/Mmux_interrupts_Result<0>:O)| NONE(*)(opb_intc_0/INTC_CORE_I/INTR_DET_I/DETECT_INTR_I/EDGE_DET_BIT_I0/KIND_OF_EDGE_I/RISING_EDGE_DET_I)| 1     |
-----------------------------------+------------------------+-------+
(*) This 1 clock signal(s) are generated by combinatorial logic,
and XST is not able to identify which are the primary clock signals.
Please use the CLOCK_SIGNAL constraint to specify the clock signal(s) generated by combinatorial logic.

Timing Summary:
---------------
Speed Grade: -4

   Minimum period: 6.209ns (Maximum Frequency: 161.056MHz)
   Minimum input arrival time before clock: 2.900ns
   Maximum output required time after clock: 1.988ns
   Maximum combinational path delay: No path found

Timing Detail:
--------------
All values displayed in nanoseconds (ns)

-------------------------------------------------------------------------
Timing constraint: Default period analysis for Clock 'OPB_Clk'
Delay:               6.209ns (Levels of Logic = 10)
  Source:            opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I0 (FF)
  Destination:       opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I31 (FF)
  Source Clock:      OPB_Clk rising
  Destination Clock: OPB_Clk rising

  Data Path: opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I0 to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I31
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDR:C->Q              1   0.720   0.240  opb_intc_0/OPB_INTFC_I/OPB_ABUS_REG_BIT_I0 (opb_intc_0/OPB_INTFC_I/intc_addr<0>)
     LUT4_L:I0->LO         1   0.551   0.000  opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/_n00231 (opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/lut_out<0>)
     MUXCY:S->O            1   0.500   0.000  opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/MUXCY_I0 (opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/carry_chain<1>)
     MUXCY:CI->O           1   0.064   0.000  opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/MUXCY_I1 (opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/carry_chain<2>)
     MUXCY:CI->O           1   0.064   0.000  opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/MUXCY_I2 (opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/carry_chain<3>)
     MUXCY:CI->O           1   0.064   0.000  opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/MUXCY_I3 (opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/carry_chain<4>)
     MUXCY:CI->O           1   0.064   0.000  opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/MUXCY_I4 (opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/carry_chain<5>)
     MUXCY:CI->O          26   0.281   1.315  opb_intc_0/OPB_INTFC_I/ADDR_DECODE_I/MUXCY_I5 (opb_intc_0/OPB_INTFC_I/intc_select)
     LUT4:I3->O            4   0.551   0.629  opb_intc_0/INTC_CORE_I/REGS_I/rd_reg_sel<1>1 (opb_intc_0/INTC_CORE_I/REGS_I/rd_reg_sel<1>)
     MUXF5:S->O            1   0.621   0.000  opb_intc_0/INTC_CORE_I/REGS_I/RD_REG_MUX_I/Mmux_Bus_out_inst_mux_f5_2 (opb_intc_0/INTC_CORE_I/REGS_I/RD_REG_MUX_I/Mmux_Bus_out__net9)
     MUXF6:I0->O           1   0.342   0.000  opb_intc_0/INTC_CORE_I/REGS_I/RD_REG_MUX_I/Mmux_Bus_out_inst_mux_f6_1 (opb_intc_0/read_data<1>)
     FDRE:D                    0.203          opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I30
    ----------------------------------------
    Total                      6.209ns (4.025ns logic, 2.184ns route)
                                       (64.8% logic, 35.2% route)

-------------------------------------------------------------------------
Timing constraint: Default OFFSET IN BEFORE for Clock 'OPB_Clk'
Offset:              2.900ns (Levels of Logic = 1)
  Source:            OPB_Rst (PAD)
  Destination:       opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26 (FF)
  Destination Clock: OPB_Clk rising

  Data Path: OPB_Rst to opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I26
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     LUT3:I2->O           34   0.551   1.323  opb_intc_0/OPB_INTFC_I/rst_intc_dbus1 (opb_intc_0/OPB_INTFC_I/rst_intc_dbus)
     FDRE:R                    1.026          opb_intc_0/OPB_INTFC_I/INTC_DBUS_BIT_I0
    ----------------------------------------
    Total                      2.900ns (1.577ns logic, 1.323ns route)
                                       (54.4% logic, 45.6% route)

-------------------------------------------------------------------------
Timing constraint: Default OFFSET OUT AFTER for Clock 'OPB_Clk'
Offset:              1.988ns (Levels of Logic = 1)
  Source:            opb_intc_0/INTC_CORE_I/IRQ_GEN_I/IRQ_PUSLE_GEN_I/current_3 (FF)
  Destination:       Irq (PAD)
  Source Clock:      OPB_Clk rising

  Data Path: opb_intc_0/INTC_CORE_I/IRQ_GEN_I/IRQ_PUSLE_GEN_I/current_3 to Irq
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDS:C->Q              7   0.720   0.717  opb_intc_0/INTC_CORE_I/IRQ_GEN_I/IRQ_PUSLE_GEN_I/current_3 (opb_intc_0/INTC_CORE_I/IRQ_GEN_I/IRQ_PUSLE_GEN_I/current_3)
     LUT4:I1->O            0   0.551   0.000  opb_intc_0/INTC_CORE_I/IRQ_GEN_I/Irq1 (Irq)
    ----------------------------------------
    Total                      1.988ns (1.271ns logic, 0.717ns route)
                                       (63.9% logic, 36.1% route)

=========================================================================
CPU : 8.89 / 44.70 s | Elapsed : 9.00 / 10.00 s
 
--> 

Total memory usage is 104816 kilobytes


