Release 6.3i - xst G.35
Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.
--> 
TABLE OF CONTENTS
  1) Synthesis Options Summary
  2) HDL Compilation
  3) HDL Analysis
  4) HDL Synthesis
  5) Advanced HDL Synthesis
     5.1) HDL Synthesis Report
  6) Low Level Synthesis
  7) Final Report
     7.1) Device utilization summary
     7.2) TIMING REPORT


=========================================================================
*                      Synthesis Options Summary                        *
=========================================================================
---- Source Parameters
Input Format                       : MIXED
Input File Name                    : microblaze_0_wrapper_xst.prj

---- Target Parameters
Target Device                      : XC3S200FT256-4
Output File Name                   : ../implementation/microblaze_0_wrapper/microblaze_0_wrapper.ngc

---- Source Options
Top Module Name                    : microblaze_0_wrapper

---- Target Options
Add IO Buffers                     : NO

---- General Options
Optimization Effort                : 2
Optimization Goal                  : speed
RTL Output                         : YES
Hierarchy Separator                : /

=========================================================================


=========================================================================
*                          HDL Compilation                              *
=========================================================================
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/microblaze_types_pkg.vhd in Library microblaze_v3_00_a.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/microblaze_types_pkg_body.vhd in Library microblaze_v3_00_a.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/microblaze_isa_be_pkg.vhd in Library microblaze_v3_00_a.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd in Library microblaze_v3_00_a.
Entity <PC_Bit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd in Library microblaze_v3_00_a.
Entity <MSR_Reg_Bit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd in Library microblaze_v3_00_a.
Entity <Result_Mux_Bit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd in Library microblaze_v3_00_a.
Entity <Shift_Logic_Bit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd in Library microblaze_v3_00_a.
Entity <ALU_Bit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd in Library microblaze_v3_00_a.
Entity <Operand_Select_Bit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd in Library microblaze_v3_00_a.
Entity <Register_File_Bit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/address_hit.vhd in Library microblaze_v3_00_a.
Entity <address_hit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/address_data_hit.vhd in Library microblaze_v3_00_a.
Entity <address_data_hit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mux2_32.vhd in Library microblaze_v3_00_a.
Entity <mux2_32> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/opb_data_mux.vhd in Library microblaze_v3_00_a.
Entity <OPB_Data_Mux> (Architecture <imp>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/data_read_steering.vhd in Library microblaze_v3_00_a.
Entity <Data_Read_Steering> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mux4_8.vhd in Library microblaze_v3_00_a.
Entity <mux4_8> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mux2_8.vhd in Library microblaze_v3_00_a.
Entity <mux2_8> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file.vhd in Library microblaze_v3_00_a.
Entity <Register_File> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select.vhd in Library microblaze_v3_00_a.
Entity <Operand_Select> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu.vhd in Library microblaze_v3_00_a.
Entity <ALU> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic.vhd in Library microblaze_v3_00_a.
Entity <Shift_Logic_Module> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/barrel_shifter.vhd in Library microblaze_v3_00_a.
Entity <barrel_shift> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/div_unit.vhd in Library microblaze_v3_00_a.
Entity <Div_unit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mul_unit.vhd in Library microblaze_v3_00_a.
Entity <MUL_Unit> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux.vhd in Library microblaze_v3_00_a.
Entity <Result_Mux> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/zero_detect.vhd in Library microblaze_v3_00_a.
Entity <Zero_Detect> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg.vhd in Library microblaze_v3_00_a.
Entity <MSR_Reg> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_module.vhd in Library microblaze_v3_00_a.
Entity <PC_Module> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/prefetch_buffer.vhd in Library microblaze_v3_00_a.
Entity <PreFetch_Buffer> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/decode.vhd in Library microblaze_v3_00_a.
Entity <Decode> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/data_flow.vhd in Library microblaze_v3_00_a.
Entity <Data_Flow> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/byte_doublet_handle.vhd in Library microblaze_v3_00_a.
Entity <Byte_Doublet_Handle> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/dopb_interface.vhd in Library microblaze_v3_00_a.
Entity <DOPB_Interface> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/iopb_interface.vhd in Library microblaze_v3_00_a.
Entity <IOPB_Interface> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/debug.vhd in Library microblaze_v3_00_a.
Entity <Debug> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/fsl_module.vhd in Library microblaze_v3_00_a.
Entity <FSL_Module> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/icache.vhd in Library microblaze_v3_00_a.
Entity <ICache> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/dcache.vhd in Library microblaze_v3_00_a.
Entity <DCache> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/exception_registers.vhd in Library microblaze_v3_00_a.
Entity <exception_registers> (Architecture <IMP>) compiled.
Compiling vhdl file //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/microblaze.vhd in Library microblaze_v3_00_a.
Entity <MicroBlaze> (Architecture <IMP>) compiled.
Compiling vhdl file C:/Data/EDKexamples/MB_Spartan3_Tutorial_6_3/synthesis/../hdl/microblaze_0_wrapper.vhd in Library work.
Entity <microblaze_0_wrapper> (Architecture <STRUCTURE>) compiled.

=========================================================================
*                            HDL Analysis                               *
=========================================================================
Analyzing Entity <microblaze_0_wrapper> (Architecture <STRUCTURE>).
Instantiating component <microblaze> from Library <microblaze_v3_00_a>.
WARNING:Xst:1542 - C:/Data/EDKexamples/MB_Spartan3_Tutorial_6_3/synthesis/../hdl/microblaze_0_wrapper.vhd line 425: No default binding for component: <microblaze>. Generic <C_DATA_SIZE> is not on the component.
WARNING:Xst:1542 - C:/Data/EDKexamples/MB_Spartan3_Tutorial_6_3/synthesis/../hdl/microblaze_0_wrapper.vhd line 425: No default binding for component: <microblaze>. Generic <C_DYNAMIC_BUS_SIZING> is not on the component.
Entity <microblaze_0_wrapper> analyzed. Unit <microblaze_0_wrapper> generated.

Analyzing generic Entity <microblaze> (Architecture <imp>).
	C_FAMILY = "spartan3"
	C_INSTANCE = "microblaze_0"
	C_D_OPB = 1
	C_D_LMB = 1
	C_I_OPB = 1
	C_I_LMB = 1
	C_USE_BARREL = 0
	C_USE_DIV = 0
	C_USE_MSR_INSTR = 0
	C_UNALIGNED_EXCEPTIONS = 0
	C_ILL_OPCODE_EXCEPTION = 0
	C_IOPB_BUS_EXCEPTION = 0
	C_DOPB_BUS_EXCEPTION = 0
	C_DIV_ZERO_EXCEPTION = 0
	C_DEBUG_ENABLED = 1
	C_NUMBER_OF_PC_BRK = 2
	C_NUMBER_OF_RD_ADDR_BRK = 1
	C_NUMBER_OF_WR_ADDR_BRK = 1
	C_INTERRUPT_IS_EDGE = 0
	C_EDGE_IS_POSITIVE = 1
	C_FSL_LINKS = 0
	C_FSL_DATA_SIZE = 32
	C_ICACHE_BASEADDR = <u>00000000000000000000000000000000
	C_ICACHE_HIGHADDR = <u>00111111111111111111111111111111
	C_USE_ICACHE = 0
	C_ALLOW_ICACHE_WR = 1
	C_ADDR_TAG_BITS = 7
	C_CACHE_BYTE_SIZE = 8192
	C_ICACHE_USE_FSL = 0
	C_DCACHE_BASEADDR = <u>00000000000000000000000000000000
	C_DCACHE_HIGHADDR = <u>00111111111111111111111111111111
	C_USE_DCACHE = 0
	C_ALLOW_DCACHE_WR = 1
	C_DCACHE_ADDR_TAG = 7
	C_DCACHE_BYTE_SIZE = 8192
	C_DCACHE_USE_FSL = 0
    Set user-defined property "KEEP =  TRUE" for signal <alu_Op>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Flow_I> in unit <microblaze>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Dopb_Interface_I> in unit <microblaze>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Iopb_Interface_I> in unit <microblaze>.
Entity <microblaze> analyzed. Unit <microblaze> generated.

Analyzing generic Entity <Decode> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_USE_ICACHE = 0
	C_USE_DCACHE = 0
	C_USE_BARREL = 0
	C_USE_MSR_INSTR = 0
	C_USE_DIV = 0
	C_FSL_LINKS = 0
	C_UNALIGNED_EXCEPTIONS = 0
	C_ILL_OPCODE_EXCEPTION = 0
	C_IOPB_BUS_EXCEPTION = 0
	C_DOPB_BUS_EXCEPTION = 0
	C_DIV_ZERO_EXCEPTION = 0
	C_USE_HW_MUL = <u>1
    Set user-defined property "KEEP =  true" for signal <of_PipeRun_s_I>.
    Set user-defined property "KEEP =  true" for signal <of_PipeRun_s_II>.
    Set user-defined property "KEEP =  true" for signal <of_PipeRun_s_III>.
    Set user-defined property "U_SET =  microblaze_0" for instance <clean_iReady_MuxCY> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y5" for instance <clean_iReady_MuxCY> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <iFetch_MuxCY_1> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y15" for instance <iFetch_MuxCY_1> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <iFetch_MuxCY_2> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y15" for instance <iFetch_MuxCY_2> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <iFetch_MuxCY_3> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y16" for instance <iFetch_MuxCY_3> in unit <Decode>.
    Set user-defined property "INIT =  0040" for instance <of_PipeRun_Select_LUT4> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <of_PipeRun_Select_LUT4> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y7" for instance <of_PipeRun_Select_LUT4> in unit <Decode>.
    Set user-defined property "INIT =  0004" for instance <of_PipeRun_without_dready_LUT4> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <of_PipeRun_without_dready_LUT4> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <of_PipeRun_MuxCY_1> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y7" for instance <of_PipeRun_MuxCY_1> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <OpSel1_SPR_Select_LUT_1> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y11" for instance <OpSel1_SPR_Select_LUT_1> in unit <Decode>.
    Set user-defined property "INIT =  2000" for instance <OpSel1_SPR_Select_LUT_1> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <OpSel1_SPR_Select_LUT_2> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y11" for instance <OpSel1_SPR_Select_LUT_2> in unit <Decode>.
    Set user-defined property "INIT =  0200" for instance <OpSel1_SPR_Select_LUT_2> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <OpSel1_SPR_Select_LUT_3> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y10" for instance <OpSel1_SPR_Select_LUT_3> in unit <Decode>.
    Set user-defined property "INIT =  04" for instance <OpSel1_SPR_Select_LUT_3> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <OpSel1_SPR_Select_LUT_4> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y10" for instance <OpSel1_SPR_Select_LUT_4> in unit <Decode>.
    Set user-defined property "INIT =  15" for instance <OpSel1_SPR_Select_LUT_4> in unit <Decode>.
    Set user-defined property "RLOC =  X20Y16" for instance <New_Carry_MUXCY> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <New_Carry_MUXCY> in unit <Decode>.
    Set user-defined property "RLOC =  X20Y17" for instance <Correct_Carry_MUXCY> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Correct_Carry_MUXCY> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <force_jump1_LUT3> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y13" for instance <force_jump1_LUT3> in unit <Decode>.
    Set user-defined property "INIT =  B4" for instance <force_jump1_LUT3> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <force_di1_LUT3> in unit <Decode>.
    Set user-defined property "INIT =  B4" for instance <force_di1_LUT3> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXCY_JUMP_CARRY> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y13" for instance <MUXCY_JUMP_CARRY> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <force_jump2_LUT4> in unit <Decode>.
    Set user-defined property "INIT =  0200" for instance <force_jump2_LUT4> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <force_di2_LUT4> in unit <Decode>.
    Set user-defined property "INIT =  AABA" for instance <force_di2_LUT4> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXCY_JUMP_CARRY2> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y14" for instance <MUXCY_JUMP_CARRY2> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXCY_JUMP_CARRY3> in unit <Decode>.
    Set user-defined property "RLOC =  X23Y14" for instance <MUXCY_JUMP_CARRY3> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Take_Intr_MUXCY_1> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y8" for instance <Take_Intr_MUXCY_1> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Take_Intr_MUXCY_2> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y8" for instance <Take_Intr_MUXCY_2> in unit <Decode>.
    Set user-defined property "U_SET =  microblaze_0" for instance <OpSel1_SPR_MUXCY_1> in unit <Decode>.
    Set user-defined property "RLOC =  X25Y9" for instance <OpSel1_SPR_MUXCY_1> in unit <Decode>.
INFO:Xst:1304 - Contents of register <take_Exc> in unit <Decode> never changes during circuit operation. The register is replaced by logic.
Entity <Decode> analyzed. Unit <Decode> generated.

Analyzing generic Entity <PreFetch_Buffer> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_X = 0
	C_Y = 0
	C_IOPB_BUS_EXCEPTION = 0
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I0> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y0" for instance <SRL16E_I0> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I1> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y0" for instance <SRL16E_I1> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I2> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y1" for instance <SRL16E_I2> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I3> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y1" for instance <SRL16E_I3> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I4> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y2" for instance <SRL16E_I4> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I5> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y2" for instance <SRL16E_I5> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I6> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y3" for instance <SRL16E_I6> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I7> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y3" for instance <SRL16E_I7> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I8> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y4" for instance <SRL16E_I8> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I9> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y4" for instance <SRL16E_I9> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I10> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y5" for instance <SRL16E_I10> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I11> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y5" for instance <SRL16E_I11> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I12> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y6" for instance <SRL16E_I12> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I13> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y6" for instance <SRL16E_I13> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I14> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y7" for instance <SRL16E_I14> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I15> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y7" for instance <SRL16E_I15> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I16> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y8" for instance <SRL16E_I16> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I17> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y8" for instance <SRL16E_I17> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I18> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y9" for instance <SRL16E_I18> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I19> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y9" for instance <SRL16E_I19> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I20> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y10" for instance <SRL16E_I20> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I21> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y10" for instance <SRL16E_I21> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I22> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y11" for instance <SRL16E_I22> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I23> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y11" for instance <SRL16E_I23> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I24> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y12" for instance <SRL16E_I24> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I25> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y12" for instance <SRL16E_I25> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I26> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y13" for instance <SRL16E_I26> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I27> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y13" for instance <SRL16E_I27> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I28> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y14" for instance <SRL16E_I28> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I29> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y14" for instance <SRL16E_I29> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I30> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y15" for instance <SRL16E_I30> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <SRL16E_I31> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X24Y15" for instance <SRL16E_I31> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <buffer_Addr_MUXCY_L1> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X23Y7" for instance <buffer_Addr_MUXCY_L1> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <buffer_Addr_XORCY_I1> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X23Y7" for instance <buffer_Addr_XORCY_I1> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <buffer_Addr_MUXCY_L2> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X23Y6" for instance <buffer_Addr_MUXCY_L2> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <buffer_Addr_XORCY_I2> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X23Y6" for instance <buffer_Addr_XORCY_I2> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <buffer_Addr_MUXCY_L3> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X23Y6" for instance <buffer_Addr_MUXCY_L3> in unit <PreFetch_Buffer>.
    Set user-defined property "U_SET =  microblaze_0" for instance <buffer_Addr_XORCY_I3> in unit <PreFetch_Buffer>.
    Set user-defined property "RLOC =  X23Y6" for instance <buffer_Addr_XORCY_I3> in unit <PreFetch_Buffer>.
Entity <PreFetch_Buffer> analyzed. Unit <PreFetch_Buffer> generated.

Analyzing generic Entity <Data_Flow> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR = "00000020"
	C_INTERRUPT_ADDR = "00000010"
	C_EXT_BRK_ADDR = "00000018"
	C_USE_EXCEPTIONS = <u>0
	C_USE_BARREL = 0
	C_USE_DIV = 0
	C_USE_MSR_INSTR = 0
	C_BUFFER_SIZE = 16
	C_PC_START_ADDR = "00000000"
	C_DEBUG_ENABLED = 1
	C_FSL_LINKS = 0
    Set user-defined property "KEEP =  TRUE" for signal <op2_i>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Module_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUL_Unit_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Zero_Detect_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_I> in unit <Data_Flow>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Module_I> in unit <Data_Flow>.
Entity <Data_Flow> analyzed. Unit <Data_Flow> generated.

Analyzing generic Entity <Register_File> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I31> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I30> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I29> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I28> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I27> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I26> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I25> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I24> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I23> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I22> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I21> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I20> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I19> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I18> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I17> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I16> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I15> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I14> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I13> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I12> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I11> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I10> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I9> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I8> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I7> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I6> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I5> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I4> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I3> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I2> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I1> in unit <Register_File>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Register_File_Bit_I0> in unit <Register_File>.
Entity <Register_File> analyzed. Unit <Register_File> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit>.
    Set user-defined property "RLOC =  X2Y0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit>.
    Set user-defined property "RLOC =  X1Y0" for instance <Data_Write_Mux> in unit <Register_File_Bit>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit>.
    Set user-defined property "RLOC =  X1Y0" for instance <Reg1_Mux> in unit <Register_File_Bit>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit>.
    Set user-defined property "RLOC =  X4Y0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit>.
    Set user-defined property "RLOC =  X6Y0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit>.
    Set user-defined property "RLOC =  X3Y0" for instance <Reg2_Mux> in unit <Register_File_Bit>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit0_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit0_>.
    Set user-defined property "RLOC =  X10Y0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit0_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit0_>.
    Set user-defined property "RLOC =  X9Y0" for instance <Data_Write_Mux> in unit <Register_File_Bit0_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit0_>.
    Set user-defined property "RLOC =  X9Y0" for instance <Reg1_Mux> in unit <Register_File_Bit0_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit0_>.
    Set user-defined property "RLOC =  X12Y0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit0_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit0_>.
    Set user-defined property "RLOC =  X14Y0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit0_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit0_>.
    Set user-defined property "RLOC =  X11Y0" for instance <Reg2_Mux> in unit <Register_File_Bit0_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit0_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit0> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y1" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit1_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit1_>.
    Set user-defined property "RLOC =  X2Y1" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit1_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit1_>.
    Set user-defined property "RLOC =  X1Y1" for instance <Data_Write_Mux> in unit <Register_File_Bit1_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit1_>.
    Set user-defined property "RLOC =  X1Y1" for instance <Reg1_Mux> in unit <Register_File_Bit1_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit1_>.
    Set user-defined property "RLOC =  X4Y1" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit1_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit1_>.
    Set user-defined property "RLOC =  X6Y1" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit1_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit1_>.
    Set user-defined property "RLOC =  X3Y1" for instance <Reg2_Mux> in unit <Register_File_Bit1_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit1_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit1> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y1" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit2_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit2_>.
    Set user-defined property "RLOC =  X10Y1" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit2_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit2_>.
    Set user-defined property "RLOC =  X9Y1" for instance <Data_Write_Mux> in unit <Register_File_Bit2_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit2_>.
    Set user-defined property "RLOC =  X9Y1" for instance <Reg1_Mux> in unit <Register_File_Bit2_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit2_>.
    Set user-defined property "RLOC =  X12Y1" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit2_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit2_>.
    Set user-defined property "RLOC =  X14Y1" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit2_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit2_>.
    Set user-defined property "RLOC =  X11Y1" for instance <Reg2_Mux> in unit <Register_File_Bit2_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit2_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit2> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y2" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit3_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit3_>.
    Set user-defined property "RLOC =  X2Y2" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit3_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit3_>.
    Set user-defined property "RLOC =  X1Y2" for instance <Data_Write_Mux> in unit <Register_File_Bit3_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit3_>.
    Set user-defined property "RLOC =  X1Y2" for instance <Reg1_Mux> in unit <Register_File_Bit3_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit3_>.
    Set user-defined property "RLOC =  X4Y2" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit3_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit3_>.
    Set user-defined property "RLOC =  X6Y2" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit3_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit3_>.
    Set user-defined property "RLOC =  X3Y2" for instance <Reg2_Mux> in unit <Register_File_Bit3_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit3_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit3> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y2" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit4_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit4_>.
    Set user-defined property "RLOC =  X10Y2" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit4_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit4_>.
    Set user-defined property "RLOC =  X9Y2" for instance <Data_Write_Mux> in unit <Register_File_Bit4_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit4_>.
    Set user-defined property "RLOC =  X9Y2" for instance <Reg1_Mux> in unit <Register_File_Bit4_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit4_>.
    Set user-defined property "RLOC =  X12Y2" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit4_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit4_>.
    Set user-defined property "RLOC =  X14Y2" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit4_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit4_>.
    Set user-defined property "RLOC =  X11Y2" for instance <Reg2_Mux> in unit <Register_File_Bit4_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit4_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit4> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y3" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit5_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit5_>.
    Set user-defined property "RLOC =  X2Y3" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit5_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit5_>.
    Set user-defined property "RLOC =  X1Y3" for instance <Data_Write_Mux> in unit <Register_File_Bit5_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit5_>.
    Set user-defined property "RLOC =  X1Y3" for instance <Reg1_Mux> in unit <Register_File_Bit5_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit5_>.
    Set user-defined property "RLOC =  X4Y3" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit5_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit5_>.
    Set user-defined property "RLOC =  X6Y3" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit5_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit5_>.
    Set user-defined property "RLOC =  X3Y3" for instance <Reg2_Mux> in unit <Register_File_Bit5_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit5_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit5> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y3" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit6_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit6_>.
    Set user-defined property "RLOC =  X10Y3" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit6_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit6_>.
    Set user-defined property "RLOC =  X9Y3" for instance <Data_Write_Mux> in unit <Register_File_Bit6_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit6_>.
    Set user-defined property "RLOC =  X9Y3" for instance <Reg1_Mux> in unit <Register_File_Bit6_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit6_>.
    Set user-defined property "RLOC =  X12Y3" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit6_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit6_>.
    Set user-defined property "RLOC =  X14Y3" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit6_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit6_>.
    Set user-defined property "RLOC =  X11Y3" for instance <Reg2_Mux> in unit <Register_File_Bit6_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit6_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit6> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y4" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit7_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit7_>.
    Set user-defined property "RLOC =  X2Y4" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit7_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit7_>.
    Set user-defined property "RLOC =  X1Y4" for instance <Data_Write_Mux> in unit <Register_File_Bit7_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit7_>.
    Set user-defined property "RLOC =  X1Y4" for instance <Reg1_Mux> in unit <Register_File_Bit7_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit7_>.
    Set user-defined property "RLOC =  X4Y4" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit7_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit7_>.
    Set user-defined property "RLOC =  X6Y4" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit7_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit7_>.
    Set user-defined property "RLOC =  X3Y4" for instance <Reg2_Mux> in unit <Register_File_Bit7_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit7_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit7> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y4" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit8_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit8_>.
    Set user-defined property "RLOC =  X10Y4" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit8_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit8_>.
    Set user-defined property "RLOC =  X9Y4" for instance <Data_Write_Mux> in unit <Register_File_Bit8_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit8_>.
    Set user-defined property "RLOC =  X9Y4" for instance <Reg1_Mux> in unit <Register_File_Bit8_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit8_>.
    Set user-defined property "RLOC =  X12Y4" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit8_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit8_>.
    Set user-defined property "RLOC =  X14Y4" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit8_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit8_>.
    Set user-defined property "RLOC =  X11Y4" for instance <Reg2_Mux> in unit <Register_File_Bit8_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit8_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit8> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y5" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit9_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit9_>.
    Set user-defined property "RLOC =  X2Y5" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit9_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit9_>.
    Set user-defined property "RLOC =  X1Y5" for instance <Data_Write_Mux> in unit <Register_File_Bit9_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit9_>.
    Set user-defined property "RLOC =  X1Y5" for instance <Reg1_Mux> in unit <Register_File_Bit9_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit9_>.
    Set user-defined property "RLOC =  X4Y5" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit9_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit9_>.
    Set user-defined property "RLOC =  X6Y5" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit9_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit9_>.
    Set user-defined property "RLOC =  X3Y5" for instance <Reg2_Mux> in unit <Register_File_Bit9_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit9_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit9> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y5" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit10_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit10_>.
    Set user-defined property "RLOC =  X10Y5" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit10_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit10_>.
    Set user-defined property "RLOC =  X9Y5" for instance <Data_Write_Mux> in unit <Register_File_Bit10_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit10_>.
    Set user-defined property "RLOC =  X9Y5" for instance <Reg1_Mux> in unit <Register_File_Bit10_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit10_>.
    Set user-defined property "RLOC =  X12Y5" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit10_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit10_>.
    Set user-defined property "RLOC =  X14Y5" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit10_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit10_>.
    Set user-defined property "RLOC =  X11Y5" for instance <Reg2_Mux> in unit <Register_File_Bit10_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit10_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit10> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y6" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit11_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit11_>.
    Set user-defined property "RLOC =  X2Y6" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit11_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit11_>.
    Set user-defined property "RLOC =  X1Y6" for instance <Data_Write_Mux> in unit <Register_File_Bit11_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit11_>.
    Set user-defined property "RLOC =  X1Y6" for instance <Reg1_Mux> in unit <Register_File_Bit11_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit11_>.
    Set user-defined property "RLOC =  X4Y6" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit11_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit11_>.
    Set user-defined property "RLOC =  X6Y6" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit11_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit11_>.
    Set user-defined property "RLOC =  X3Y6" for instance <Reg2_Mux> in unit <Register_File_Bit11_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit11_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit11> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y6" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit12_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit12_>.
    Set user-defined property "RLOC =  X10Y6" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit12_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit12_>.
    Set user-defined property "RLOC =  X9Y6" for instance <Data_Write_Mux> in unit <Register_File_Bit12_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit12_>.
    Set user-defined property "RLOC =  X9Y6" for instance <Reg1_Mux> in unit <Register_File_Bit12_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit12_>.
    Set user-defined property "RLOC =  X12Y6" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit12_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit12_>.
    Set user-defined property "RLOC =  X14Y6" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit12_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit12_>.
    Set user-defined property "RLOC =  X11Y6" for instance <Reg2_Mux> in unit <Register_File_Bit12_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit12_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit12> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y7" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit13_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit13_>.
    Set user-defined property "RLOC =  X2Y7" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit13_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit13_>.
    Set user-defined property "RLOC =  X1Y7" for instance <Data_Write_Mux> in unit <Register_File_Bit13_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit13_>.
    Set user-defined property "RLOC =  X1Y7" for instance <Reg1_Mux> in unit <Register_File_Bit13_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit13_>.
    Set user-defined property "RLOC =  X4Y7" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit13_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit13_>.
    Set user-defined property "RLOC =  X6Y7" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit13_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit13_>.
    Set user-defined property "RLOC =  X3Y7" for instance <Reg2_Mux> in unit <Register_File_Bit13_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit13_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit13> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y7" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit14_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit14_>.
    Set user-defined property "RLOC =  X10Y7" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit14_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit14_>.
    Set user-defined property "RLOC =  X9Y7" for instance <Data_Write_Mux> in unit <Register_File_Bit14_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit14_>.
    Set user-defined property "RLOC =  X9Y7" for instance <Reg1_Mux> in unit <Register_File_Bit14_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit14_>.
    Set user-defined property "RLOC =  X12Y7" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit14_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit14_>.
    Set user-defined property "RLOC =  X14Y7" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit14_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit14_>.
    Set user-defined property "RLOC =  X11Y7" for instance <Reg2_Mux> in unit <Register_File_Bit14_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit14_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit14> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y8" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit15_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit15_>.
    Set user-defined property "RLOC =  X2Y8" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit15_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit15_>.
    Set user-defined property "RLOC =  X1Y8" for instance <Data_Write_Mux> in unit <Register_File_Bit15_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit15_>.
    Set user-defined property "RLOC =  X1Y8" for instance <Reg1_Mux> in unit <Register_File_Bit15_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit15_>.
    Set user-defined property "RLOC =  X4Y8" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit15_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit15_>.
    Set user-defined property "RLOC =  X6Y8" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit15_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit15_>.
    Set user-defined property "RLOC =  X3Y8" for instance <Reg2_Mux> in unit <Register_File_Bit15_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit15_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit15> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y8" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit16_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit16_>.
    Set user-defined property "RLOC =  X10Y8" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit16_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit16_>.
    Set user-defined property "RLOC =  X9Y8" for instance <Data_Write_Mux> in unit <Register_File_Bit16_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit16_>.
    Set user-defined property "RLOC =  X9Y8" for instance <Reg1_Mux> in unit <Register_File_Bit16_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit16_>.
    Set user-defined property "RLOC =  X12Y8" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit16_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit16_>.
    Set user-defined property "RLOC =  X14Y8" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit16_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit16_>.
    Set user-defined property "RLOC =  X11Y8" for instance <Reg2_Mux> in unit <Register_File_Bit16_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit16_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit16> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y9" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit17_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit17_>.
    Set user-defined property "RLOC =  X2Y9" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit17_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit17_>.
    Set user-defined property "RLOC =  X1Y9" for instance <Data_Write_Mux> in unit <Register_File_Bit17_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit17_>.
    Set user-defined property "RLOC =  X1Y9" for instance <Reg1_Mux> in unit <Register_File_Bit17_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit17_>.
    Set user-defined property "RLOC =  X4Y9" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit17_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit17_>.
    Set user-defined property "RLOC =  X6Y9" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit17_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit17_>.
    Set user-defined property "RLOC =  X3Y9" for instance <Reg2_Mux> in unit <Register_File_Bit17_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit17_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit17> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y9" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit18_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit18_>.
    Set user-defined property "RLOC =  X10Y9" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit18_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit18_>.
    Set user-defined property "RLOC =  X9Y9" for instance <Data_Write_Mux> in unit <Register_File_Bit18_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit18_>.
    Set user-defined property "RLOC =  X9Y9" for instance <Reg1_Mux> in unit <Register_File_Bit18_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit18_>.
    Set user-defined property "RLOC =  X12Y9" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit18_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit18_>.
    Set user-defined property "RLOC =  X14Y9" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit18_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit18_>.
    Set user-defined property "RLOC =  X11Y9" for instance <Reg2_Mux> in unit <Register_File_Bit18_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit18_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit18> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y10" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit19_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit19_>.
    Set user-defined property "RLOC =  X2Y10" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit19_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit19_>.
    Set user-defined property "RLOC =  X1Y10" for instance <Data_Write_Mux> in unit <Register_File_Bit19_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit19_>.
    Set user-defined property "RLOC =  X1Y10" for instance <Reg1_Mux> in unit <Register_File_Bit19_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit19_>.
    Set user-defined property "RLOC =  X4Y10" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit19_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit19_>.
    Set user-defined property "RLOC =  X6Y10" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit19_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit19_>.
    Set user-defined property "RLOC =  X3Y10" for instance <Reg2_Mux> in unit <Register_File_Bit19_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit19_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit19> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y10" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit20_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit20_>.
    Set user-defined property "RLOC =  X10Y10" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit20_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit20_>.
    Set user-defined property "RLOC =  X9Y10" for instance <Data_Write_Mux> in unit <Register_File_Bit20_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit20_>.
    Set user-defined property "RLOC =  X9Y10" for instance <Reg1_Mux> in unit <Register_File_Bit20_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit20_>.
    Set user-defined property "RLOC =  X12Y10" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit20_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit20_>.
    Set user-defined property "RLOC =  X14Y10" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit20_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit20_>.
    Set user-defined property "RLOC =  X11Y10" for instance <Reg2_Mux> in unit <Register_File_Bit20_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit20_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit20> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y11" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit21_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit21_>.
    Set user-defined property "RLOC =  X2Y11" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit21_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit21_>.
    Set user-defined property "RLOC =  X1Y11" for instance <Data_Write_Mux> in unit <Register_File_Bit21_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit21_>.
    Set user-defined property "RLOC =  X1Y11" for instance <Reg1_Mux> in unit <Register_File_Bit21_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit21_>.
    Set user-defined property "RLOC =  X4Y11" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit21_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit21_>.
    Set user-defined property "RLOC =  X6Y11" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit21_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit21_>.
    Set user-defined property "RLOC =  X3Y11" for instance <Reg2_Mux> in unit <Register_File_Bit21_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit21_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit21> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y11" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit22_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit22_>.
    Set user-defined property "RLOC =  X10Y11" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit22_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit22_>.
    Set user-defined property "RLOC =  X9Y11" for instance <Data_Write_Mux> in unit <Register_File_Bit22_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit22_>.
    Set user-defined property "RLOC =  X9Y11" for instance <Reg1_Mux> in unit <Register_File_Bit22_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit22_>.
    Set user-defined property "RLOC =  X12Y11" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit22_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit22_>.
    Set user-defined property "RLOC =  X14Y11" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit22_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit22_>.
    Set user-defined property "RLOC =  X11Y11" for instance <Reg2_Mux> in unit <Register_File_Bit22_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit22_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit22> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y12" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit23_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit23_>.
    Set user-defined property "RLOC =  X2Y12" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit23_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit23_>.
    Set user-defined property "RLOC =  X1Y12" for instance <Data_Write_Mux> in unit <Register_File_Bit23_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit23_>.
    Set user-defined property "RLOC =  X1Y12" for instance <Reg1_Mux> in unit <Register_File_Bit23_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit23_>.
    Set user-defined property "RLOC =  X4Y12" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit23_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit23_>.
    Set user-defined property "RLOC =  X6Y12" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit23_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit23_>.
    Set user-defined property "RLOC =  X3Y12" for instance <Reg2_Mux> in unit <Register_File_Bit23_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit23_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit23> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y12" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit24_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit24_>.
    Set user-defined property "RLOC =  X10Y12" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit24_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit24_>.
    Set user-defined property "RLOC =  X9Y12" for instance <Data_Write_Mux> in unit <Register_File_Bit24_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit24_>.
    Set user-defined property "RLOC =  X9Y12" for instance <Reg1_Mux> in unit <Register_File_Bit24_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit24_>.
    Set user-defined property "RLOC =  X12Y12" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit24_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit24_>.
    Set user-defined property "RLOC =  X14Y12" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit24_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit24_>.
    Set user-defined property "RLOC =  X11Y12" for instance <Reg2_Mux> in unit <Register_File_Bit24_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit24_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit24> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y13" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit25_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit25_>.
    Set user-defined property "RLOC =  X2Y13" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit25_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit25_>.
    Set user-defined property "RLOC =  X1Y13" for instance <Data_Write_Mux> in unit <Register_File_Bit25_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit25_>.
    Set user-defined property "RLOC =  X1Y13" for instance <Reg1_Mux> in unit <Register_File_Bit25_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit25_>.
    Set user-defined property "RLOC =  X4Y13" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit25_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit25_>.
    Set user-defined property "RLOC =  X6Y13" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit25_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit25_>.
    Set user-defined property "RLOC =  X3Y13" for instance <Reg2_Mux> in unit <Register_File_Bit25_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit25_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit25> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y13" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit26_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit26_>.
    Set user-defined property "RLOC =  X10Y13" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit26_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit26_>.
    Set user-defined property "RLOC =  X9Y13" for instance <Data_Write_Mux> in unit <Register_File_Bit26_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit26_>.
    Set user-defined property "RLOC =  X9Y13" for instance <Reg1_Mux> in unit <Register_File_Bit26_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit26_>.
    Set user-defined property "RLOC =  X12Y13" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit26_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit26_>.
    Set user-defined property "RLOC =  X14Y13" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit26_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit26_>.
    Set user-defined property "RLOC =  X11Y13" for instance <Reg2_Mux> in unit <Register_File_Bit26_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit26_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit26> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y14" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit27_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit27_>.
    Set user-defined property "RLOC =  X2Y14" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit27_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit27_>.
    Set user-defined property "RLOC =  X1Y14" for instance <Data_Write_Mux> in unit <Register_File_Bit27_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit27_>.
    Set user-defined property "RLOC =  X1Y14" for instance <Reg1_Mux> in unit <Register_File_Bit27_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit27_>.
    Set user-defined property "RLOC =  X4Y14" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit27_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit27_>.
    Set user-defined property "RLOC =  X6Y14" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit27_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit27_>.
    Set user-defined property "RLOC =  X3Y14" for instance <Reg2_Mux> in unit <Register_File_Bit27_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit27_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit27> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y14" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit28_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit28_>.
    Set user-defined property "RLOC =  X10Y14" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit28_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit28_>.
    Set user-defined property "RLOC =  X9Y14" for instance <Data_Write_Mux> in unit <Register_File_Bit28_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit28_>.
    Set user-defined property "RLOC =  X9Y14" for instance <Reg1_Mux> in unit <Register_File_Bit28_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit28_>.
    Set user-defined property "RLOC =  X12Y14" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit28_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit28_>.
    Set user-defined property "RLOC =  X14Y14" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit28_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit28_>.
    Set user-defined property "RLOC =  X11Y14" for instance <Reg2_Mux> in unit <Register_File_Bit28_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit28_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit28> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 0
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X0Y15" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit29_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit29_>.
    Set user-defined property "RLOC =  X2Y15" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit29_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit29_>.
    Set user-defined property "RLOC =  X1Y15" for instance <Data_Write_Mux> in unit <Register_File_Bit29_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit29_>.
    Set user-defined property "RLOC =  X1Y15" for instance <Reg1_Mux> in unit <Register_File_Bit29_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit29_>.
    Set user-defined property "RLOC =  X4Y15" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit29_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit29_>.
    Set user-defined property "RLOC =  X6Y15" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit29_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit29_>.
    Set user-defined property "RLOC =  X3Y15" for instance <Reg2_Mux> in unit <Register_File_Bit29_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit29_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit29> generated.

Analyzing generic Entity <Register_File_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 8
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X8Y15" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit30_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_Low> in unit <Register_File_Bit30_>.
    Set user-defined property "RLOC =  X10Y15" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit30_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg1_High> in unit <Register_File_Bit30_>.
    Set user-defined property "RLOC =  X9Y15" for instance <Data_Write_Mux> in unit <Register_File_Bit30_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Data_Write_Mux> in unit <Register_File_Bit30_>.
    Set user-defined property "RLOC =  X9Y15" for instance <Reg1_Mux> in unit <Register_File_Bit30_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg1_Mux> in unit <Register_File_Bit30_>.
    Set user-defined property "RLOC =  X12Y15" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit30_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_Low> in unit <Register_File_Bit30_>.
    Set user-defined property "RLOC =  X14Y15" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit30_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <RAM16x1D_Reg2_High> in unit <Register_File_Bit30_>.
    Set user-defined property "RLOC =  X11Y15" for instance <Reg2_Mux> in unit <Register_File_Bit30_>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Reg2_Mux> in unit <Register_File_Bit30_>.
Entity <Register_File_Bit> analyzed. Unit <Register_File_Bit30> generated.

Analyzing generic Entity <Operand_Select> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_DEBUG_ENABLED = 1
	C_USE_EXCEPTIONS = <u>0
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_INTERRUPT_ADDR = "00000010"
	C_EXT_BRK_ADDR = "00000018"
	C_EXCEPTION_ADDR = "00000020"
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I31> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I30> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I29> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I28> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I27> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I26> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I25> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I24> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I23> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I22> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I21> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I20> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I19> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I18> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I17> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I16> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I15> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I14> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I13> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I12> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I11> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I10> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I9> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I8> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I7> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I6> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I5> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I4> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I3> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I2> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I1> in unit <Operand_Select>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Operand_Select_Bit_I0> in unit <Operand_Select>.
Entity <Operand_Select> analyzed. Unit <Operand_Select> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X5Y0" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X5Y0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X5Y0" for instance <Op1_MUXF5> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X5Y0" for instance <Op1_DFF> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X5Y0" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X7Y0" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X7Y0" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X7Y0" for instance <Op2_MUXF5> in unit <Operand_Select_Bit>.
    Set user-defined property "RLOC =  X7Y0" for instance <Op2_DFF> in unit <Operand_Select_Bit>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X13Y0" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit31_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X13Y0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X13Y0" for instance <Op1_MUXF5> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X13Y0" for instance <Op1_DFF> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X13Y0" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit31_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X15Y0" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit31_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X15Y0" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X15Y0" for instance <Op2_MUXF5> in unit <Operand_Select_Bit31_>.
    Set user-defined property "RLOC =  X15Y0" for instance <Op2_DFF> in unit <Operand_Select_Bit31_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit31> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X5Y1" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit32_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X5Y1" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X5Y1" for instance <Op1_MUXF5> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X5Y1" for instance <Op1_DFF> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X5Y1" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit32_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X7Y1" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit32_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X7Y1" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X7Y1" for instance <Op2_MUXF5> in unit <Operand_Select_Bit32_>.
    Set user-defined property "RLOC =  X7Y1" for instance <Op2_DFF> in unit <Operand_Select_Bit32_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit32> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>1
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X13Y1" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit33_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X13Y1" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X13Y1" for instance <Op1_MUXF5> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X13Y1" for instance <Op1_DFF> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X13Y1" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit33_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X15Y1" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit33_>.
    Set user-defined property "INIT =  54" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X15Y1" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X15Y1" for instance <Op2_MUXF5> in unit <Operand_Select_Bit33_>.
    Set user-defined property "RLOC =  X15Y1" for instance <Op2_DFF> in unit <Operand_Select_Bit33_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit33> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>1
	C_EXT_BRK_ADDR_BIT = <u>1
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X5Y2" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit34_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X5Y2" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X5Y2" for instance <Op1_MUXF5> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X5Y2" for instance <Op1_DFF> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X5Y2" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit34_>.
    Set user-defined property "INIT =  FFCA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X7Y2" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit34_>.
    Set user-defined property "INIT =  54" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X7Y2" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X7Y2" for instance <Op2_MUXF5> in unit <Operand_Select_Bit34_>.
    Set user-defined property "RLOC =  X7Y2" for instance <Op2_DFF> in unit <Operand_Select_Bit34_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit34> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>1
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X13Y2" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit35_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X13Y2" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X13Y2" for instance <Op1_MUXF5> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X13Y2" for instance <Op1_DFF> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X13Y2" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit35_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X15Y2" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit35_>.
    Set user-defined property "INIT =  BA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X15Y2" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X15Y2" for instance <Op2_MUXF5> in unit <Operand_Select_Bit35_>.
    Set user-defined property "RLOC =  X15Y2" for instance <Op2_DFF> in unit <Operand_Select_Bit35_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit35> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X5Y3" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit36_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X5Y3" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X5Y3" for instance <Op1_MUXF5> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X5Y3" for instance <Op1_DFF> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X5Y3" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit36_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X7Y3" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit36_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X7Y3" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X7Y3" for instance <Op2_MUXF5> in unit <Operand_Select_Bit36_>.
    Set user-defined property "RLOC =  X7Y3" for instance <Op2_DFF> in unit <Operand_Select_Bit36_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit36> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X13Y3" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit37_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X13Y3" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X13Y3" for instance <Op1_MUXF5> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X13Y3" for instance <Op1_DFF> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X13Y3" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit37_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X15Y3" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit37_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X15Y3" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X15Y3" for instance <Op2_MUXF5> in unit <Operand_Select_Bit37_>.
    Set user-defined property "RLOC =  X15Y3" for instance <Op2_DFF> in unit <Operand_Select_Bit37_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit37> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X5Y4" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit38_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X5Y4" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X5Y4" for instance <Op1_MUXF5> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X5Y4" for instance <Op1_DFF> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X5Y4" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit38_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X7Y4" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit38_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X7Y4" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X7Y4" for instance <Op2_MUXF5> in unit <Operand_Select_Bit38_>.
    Set user-defined property "RLOC =  X7Y4" for instance <Op2_DFF> in unit <Operand_Select_Bit38_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit38> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X13Y4" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit39_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X13Y4" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X13Y4" for instance <Op1_MUXF5> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X13Y4" for instance <Op1_DFF> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X13Y4" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit39_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X15Y4" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit39_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X15Y4" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X15Y4" for instance <Op2_MUXF5> in unit <Operand_Select_Bit39_>.
    Set user-defined property "RLOC =  X15Y4" for instance <Op2_DFF> in unit <Operand_Select_Bit39_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit39> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X5Y5" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit40_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X5Y5" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X5Y5" for instance <Op1_MUXF5> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X5Y5" for instance <Op1_DFF> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X5Y5" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit40_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X7Y5" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit40_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X7Y5" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X7Y5" for instance <Op2_MUXF5> in unit <Operand_Select_Bit40_>.
    Set user-defined property "RLOC =  X7Y5" for instance <Op2_DFF> in unit <Operand_Select_Bit40_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit40> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X13Y5" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit41_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X13Y5" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X13Y5" for instance <Op1_MUXF5> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X13Y5" for instance <Op1_DFF> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X13Y5" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit41_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X15Y5" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit41_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X15Y5" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X15Y5" for instance <Op2_MUXF5> in unit <Operand_Select_Bit41_>.
    Set user-defined property "RLOC =  X15Y5" for instance <Op2_DFF> in unit <Operand_Select_Bit41_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit41> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X5Y6" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit42_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X5Y6" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X5Y6" for instance <Op1_MUXF5> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X5Y6" for instance <Op1_DFF> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X5Y6" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit42_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X7Y6" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit42_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X7Y6" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X7Y6" for instance <Op2_MUXF5> in unit <Operand_Select_Bit42_>.
    Set user-defined property "RLOC =  X7Y6" for instance <Op2_DFF> in unit <Operand_Select_Bit42_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit42> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X13Y6" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit43_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X13Y6" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X13Y6" for instance <Op1_MUXF5> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X13Y6" for instance <Op1_DFF> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X13Y6" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit43_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X15Y6" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit43_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X15Y6" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X15Y6" for instance <Op2_MUXF5> in unit <Operand_Select_Bit43_>.
    Set user-defined property "RLOC =  X15Y6" for instance <Op2_DFF> in unit <Operand_Select_Bit43_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit43> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X5Y7" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit44_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X5Y7" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X5Y7" for instance <Op1_MUXF5> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X5Y7" for instance <Op1_DFF> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X5Y7" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit44_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X7Y7" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit44_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X7Y7" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X7Y7" for instance <Op2_MUXF5> in unit <Operand_Select_Bit44_>.
    Set user-defined property "RLOC =  X7Y7" for instance <Op2_DFF> in unit <Operand_Select_Bit44_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit44> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>1
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X13Y7" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit45_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X13Y7" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X13Y7" for instance <Op1_MUXF5> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X13Y7" for instance <Op1_DFF> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X13Y7" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit45_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X15Y7" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit45_>.
    Set user-defined property "INIT =  10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X15Y7" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X15Y7" for instance <Op2_MUXF5> in unit <Operand_Select_Bit45_>.
    Set user-defined property "RLOC =  X15Y7" for instance <Op2_DFF> in unit <Operand_Select_Bit45_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit45> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X5Y8" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit46_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X5Y8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X5Y8" for instance <Op1_MUXF5> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X5Y8" for instance <Op1_DFF> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X5Y8" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit46_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X7Y8" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit46_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X7Y8" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X7Y8" for instance <Op2_MUXF5> in unit <Operand_Select_Bit46_>.
    Set user-defined property "RLOC =  X7Y8" for instance <Op2_DFF> in unit <Operand_Select_Bit46_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit46> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X13Y8" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit47_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X13Y8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X13Y8" for instance <Op1_MUXF5> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X13Y8" for instance <Op1_DFF> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X13Y8" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit47_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X15Y8" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit47_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X15Y8" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X15Y8" for instance <Op2_MUXF5> in unit <Operand_Select_Bit47_>.
    Set user-defined property "RLOC =  X15Y8" for instance <Op2_DFF> in unit <Operand_Select_Bit47_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit47> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X5Y9" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit48_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X5Y9" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X5Y9" for instance <Op1_MUXF5> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X5Y9" for instance <Op1_DFF> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X5Y9" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit48_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X7Y9" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit48_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X7Y9" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X7Y9" for instance <Op2_MUXF5> in unit <Operand_Select_Bit48_>.
    Set user-defined property "RLOC =  X7Y9" for instance <Op2_DFF> in unit <Operand_Select_Bit48_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit48> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X13Y9" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit49_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X13Y9" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X13Y9" for instance <Op1_MUXF5> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X13Y9" for instance <Op1_DFF> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X13Y9" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit49_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X15Y9" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit49_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X15Y9" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X15Y9" for instance <Op2_MUXF5> in unit <Operand_Select_Bit49_>.
    Set user-defined property "RLOC =  X15Y9" for instance <Op2_DFF> in unit <Operand_Select_Bit49_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit49> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X5Y10" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit50_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X5Y10" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X5Y10" for instance <Op1_MUXF5> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X5Y10" for instance <Op1_DFF> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X5Y10" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit50_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X7Y10" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit50_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X7Y10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X7Y10" for instance <Op2_MUXF5> in unit <Operand_Select_Bit50_>.
    Set user-defined property "RLOC =  X7Y10" for instance <Op2_DFF> in unit <Operand_Select_Bit50_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit50> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X13Y10" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit51_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X13Y10" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X13Y10" for instance <Op1_MUXF5> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X13Y10" for instance <Op1_DFF> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X13Y10" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit51_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X15Y10" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit51_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X15Y10" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X15Y10" for instance <Op2_MUXF5> in unit <Operand_Select_Bit51_>.
    Set user-defined property "RLOC =  X15Y10" for instance <Op2_DFF> in unit <Operand_Select_Bit51_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit51> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X5Y11" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit52_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X5Y11" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X5Y11" for instance <Op1_MUXF5> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X5Y11" for instance <Op1_DFF> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X5Y11" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit52_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X7Y11" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit52_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X7Y11" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X7Y11" for instance <Op2_MUXF5> in unit <Operand_Select_Bit52_>.
    Set user-defined property "RLOC =  X7Y11" for instance <Op2_DFF> in unit <Operand_Select_Bit52_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit52> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X13Y11" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit53_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X13Y11" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X13Y11" for instance <Op1_MUXF5> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X13Y11" for instance <Op1_DFF> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X13Y11" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit53_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X15Y11" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit53_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X15Y11" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X15Y11" for instance <Op2_MUXF5> in unit <Operand_Select_Bit53_>.
    Set user-defined property "RLOC =  X15Y11" for instance <Op2_DFF> in unit <Operand_Select_Bit53_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit53> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X5Y12" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit54_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X5Y12" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X5Y12" for instance <Op1_MUXF5> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X5Y12" for instance <Op1_DFF> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X5Y12" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit54_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X7Y12" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit54_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X7Y12" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X7Y12" for instance <Op2_MUXF5> in unit <Operand_Select_Bit54_>.
    Set user-defined property "RLOC =  X7Y12" for instance <Op2_DFF> in unit <Operand_Select_Bit54_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit54> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X13Y12" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit55_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X13Y12" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X13Y12" for instance <Op1_MUXF5> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X13Y12" for instance <Op1_DFF> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X13Y12" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit55_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X15Y12" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit55_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X15Y12" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X15Y12" for instance <Op2_MUXF5> in unit <Operand_Select_Bit55_>.
    Set user-defined property "RLOC =  X15Y12" for instance <Op2_DFF> in unit <Operand_Select_Bit55_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit55> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X5Y13" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit56_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X5Y13" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X5Y13" for instance <Op1_MUXF5> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X5Y13" for instance <Op1_DFF> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X5Y13" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit56_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X7Y13" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit56_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X7Y13" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X7Y13" for instance <Op2_MUXF5> in unit <Operand_Select_Bit56_>.
    Set user-defined property "RLOC =  X7Y13" for instance <Op2_DFF> in unit <Operand_Select_Bit56_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit56> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X13Y13" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit57_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X13Y13" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X13Y13" for instance <Op1_MUXF5> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X13Y13" for instance <Op1_DFF> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X13Y13" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit57_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X15Y13" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit57_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X15Y13" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X15Y13" for instance <Op2_MUXF5> in unit <Operand_Select_Bit57_>.
    Set user-defined property "RLOC =  X15Y13" for instance <Op2_DFF> in unit <Operand_Select_Bit57_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit57> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X5Y14" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit58_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X5Y14" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X5Y14" for instance <Op1_MUXF5> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X5Y14" for instance <Op1_DFF> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X5Y14" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit58_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X7Y14" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit58_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X7Y14" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X7Y14" for instance <Op2_MUXF5> in unit <Operand_Select_Bit58_>.
    Set user-defined property "RLOC =  X7Y14" for instance <Op2_DFF> in unit <Operand_Select_Bit58_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit58> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X13Y14" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit59_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X13Y14" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X13Y14" for instance <Op1_MUXF5> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X13Y14" for instance <Op1_DFF> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X13Y14" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit59_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X15Y14" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit59_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X15Y14" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X15Y14" for instance <Op2_MUXF5> in unit <Operand_Select_Bit59_>.
    Set user-defined property "RLOC =  X15Y14" for instance <Op2_DFF> in unit <Operand_Select_Bit59_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit59> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 5
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>1
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X5Y15" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit60_>.
    Set user-defined property "INIT =  8" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X5Y15" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X5Y15" for instance <Op1_MUXF5> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X5Y15" for instance <Op1_DFF> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X5Y15" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit60_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X7Y15" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit60_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X7Y15" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X7Y15" for instance <Op2_MUXF5> in unit <Operand_Select_Bit60_>.
    Set user-defined property "RLOC =  X7Y15" for instance <Op2_DFF> in unit <Operand_Select_Bit60_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit60> generated.

Analyzing generic Entity <Operand_Select_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 13
	C_U_SET = "microblaze_0"
	C_EXCEPTION_ADDR_BIT = <u>0
	C_INTERRUPT_ADDR_BIT = <u>0
	C_EXT_BRK_ADDR_BIT = <u>0
	C_ONLY_PC = <u>0
	C_DEBUG_ENABLED = 1
	C_LOWER_HALFWORD = <u>0
    Set user-defined property "INIT =  00CA" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X13Y15" for instance <Op1_Mux2_1> in unit <Operand_Select_Bit61_>.
    Set user-defined property "INIT =  CAC0" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X13Y15" for instance <Op1_Mux2_2> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X13Y15" for instance <Op1_MUXF5> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X13Y15" for instance <Op1_DFF> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X13Y15" for instance <Op1_Reg_DFF> in unit <Operand_Select_Bit61_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X15Y15" for instance <Op2_Mux2_1> in unit <Operand_Select_Bit61_>.
    Set user-defined property "INIT =  00CA" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X15Y15" for instance <Op2_Mux2_2> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X15Y15" for instance <Op2_MUXF5> in unit <Operand_Select_Bit61_>.
    Set user-defined property "RLOC =  X15Y15" for instance <Op2_DFF> in unit <Operand_Select_Bit61_>.
Entity <Operand_Select_Bit> analyzed. Unit <Operand_Select_Bit61> generated.

Analyzing generic Entity <ALU> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I31> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I30> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I29> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I28> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I27> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I26> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I25> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I24> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I23> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I22> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I21> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I20> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I19> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I18> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I17> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I16> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I15> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I14> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I13> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I12> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I11> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I10> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I9> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I8> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I7> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I6> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I5> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I4> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I3> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I2> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I1> in unit <ALU>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ALU_Bit_I0> in unit <ALU>.
Entity <ALU> analyzed. Unit <ALU> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit>.
    Set user-defined property "RLOC =  X20Y0" for instance <I_ALU_LUT> in unit <ALU_Bit>.
    Set user-defined property "RLOC =  X20Y0" for instance <MULT_AND_I> in unit <ALU_Bit>.
    Set user-defined property "RLOC =  X20Y0" for instance <MUXCY_I> in unit <ALU_Bit>.
    Set user-defined property "RLOC =  X20Y0" for instance <XOR_I> in unit <ALU_Bit>.
    Set user-defined property "RLOC =  X20Y0" for instance <I_ABus_DFF> in unit <ALU_Bit>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit62_>.
    Set user-defined property "RLOC =  X20Y1" for instance <I_ALU_LUT> in unit <ALU_Bit62_>.
    Set user-defined property "RLOC =  X20Y1" for instance <MULT_AND_I> in unit <ALU_Bit62_>.
    Set user-defined property "RLOC =  X20Y1" for instance <MUXCY_I> in unit <ALU_Bit62_>.
    Set user-defined property "RLOC =  X20Y1" for instance <XOR_I> in unit <ALU_Bit62_>.
    Set user-defined property "RLOC =  X20Y1" for instance <I_ABus_DFF> in unit <ALU_Bit62_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit62> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit63_>.
    Set user-defined property "RLOC =  X20Y2" for instance <I_ALU_LUT> in unit <ALU_Bit63_>.
    Set user-defined property "RLOC =  X20Y2" for instance <MULT_AND_I> in unit <ALU_Bit63_>.
    Set user-defined property "RLOC =  X20Y2" for instance <MUXCY_I> in unit <ALU_Bit63_>.
    Set user-defined property "RLOC =  X20Y2" for instance <XOR_I> in unit <ALU_Bit63_>.
    Set user-defined property "RLOC =  X20Y2" for instance <I_ABus_DFF> in unit <ALU_Bit63_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit63> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit64_>.
    Set user-defined property "RLOC =  X20Y3" for instance <I_ALU_LUT> in unit <ALU_Bit64_>.
    Set user-defined property "RLOC =  X20Y3" for instance <MULT_AND_I> in unit <ALU_Bit64_>.
    Set user-defined property "RLOC =  X20Y3" for instance <MUXCY_I> in unit <ALU_Bit64_>.
    Set user-defined property "RLOC =  X20Y3" for instance <XOR_I> in unit <ALU_Bit64_>.
    Set user-defined property "RLOC =  X20Y3" for instance <I_ABus_DFF> in unit <ALU_Bit64_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit64> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit65_>.
    Set user-defined property "RLOC =  X20Y4" for instance <I_ALU_LUT> in unit <ALU_Bit65_>.
    Set user-defined property "RLOC =  X20Y4" for instance <MULT_AND_I> in unit <ALU_Bit65_>.
    Set user-defined property "RLOC =  X20Y4" for instance <MUXCY_I> in unit <ALU_Bit65_>.
    Set user-defined property "RLOC =  X20Y4" for instance <XOR_I> in unit <ALU_Bit65_>.
    Set user-defined property "RLOC =  X20Y4" for instance <I_ABus_DFF> in unit <ALU_Bit65_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit65> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit66_>.
    Set user-defined property "RLOC =  X20Y5" for instance <I_ALU_LUT> in unit <ALU_Bit66_>.
    Set user-defined property "RLOC =  X20Y5" for instance <MULT_AND_I> in unit <ALU_Bit66_>.
    Set user-defined property "RLOC =  X20Y5" for instance <MUXCY_I> in unit <ALU_Bit66_>.
    Set user-defined property "RLOC =  X20Y5" for instance <XOR_I> in unit <ALU_Bit66_>.
    Set user-defined property "RLOC =  X20Y5" for instance <I_ABus_DFF> in unit <ALU_Bit66_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit66> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit67_>.
    Set user-defined property "RLOC =  X20Y6" for instance <I_ALU_LUT> in unit <ALU_Bit67_>.
    Set user-defined property "RLOC =  X20Y6" for instance <MULT_AND_I> in unit <ALU_Bit67_>.
    Set user-defined property "RLOC =  X20Y6" for instance <MUXCY_I> in unit <ALU_Bit67_>.
    Set user-defined property "RLOC =  X20Y6" for instance <XOR_I> in unit <ALU_Bit67_>.
    Set user-defined property "RLOC =  X20Y6" for instance <I_ABus_DFF> in unit <ALU_Bit67_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit67> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit68_>.
    Set user-defined property "RLOC =  X20Y7" for instance <I_ALU_LUT> in unit <ALU_Bit68_>.
    Set user-defined property "RLOC =  X20Y7" for instance <MULT_AND_I> in unit <ALU_Bit68_>.
    Set user-defined property "RLOC =  X20Y7" for instance <MUXCY_I> in unit <ALU_Bit68_>.
    Set user-defined property "RLOC =  X20Y7" for instance <XOR_I> in unit <ALU_Bit68_>.
    Set user-defined property "RLOC =  X20Y7" for instance <I_ABus_DFF> in unit <ALU_Bit68_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit68> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit69_>.
    Set user-defined property "RLOC =  X20Y8" for instance <I_ALU_LUT> in unit <ALU_Bit69_>.
    Set user-defined property "RLOC =  X20Y8" for instance <MULT_AND_I> in unit <ALU_Bit69_>.
    Set user-defined property "RLOC =  X20Y8" for instance <MUXCY_I> in unit <ALU_Bit69_>.
    Set user-defined property "RLOC =  X20Y8" for instance <XOR_I> in unit <ALU_Bit69_>.
    Set user-defined property "RLOC =  X20Y8" for instance <I_ABus_DFF> in unit <ALU_Bit69_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit69> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit70_>.
    Set user-defined property "RLOC =  X20Y9" for instance <I_ALU_LUT> in unit <ALU_Bit70_>.
    Set user-defined property "RLOC =  X20Y9" for instance <MULT_AND_I> in unit <ALU_Bit70_>.
    Set user-defined property "RLOC =  X20Y9" for instance <MUXCY_I> in unit <ALU_Bit70_>.
    Set user-defined property "RLOC =  X20Y9" for instance <XOR_I> in unit <ALU_Bit70_>.
    Set user-defined property "RLOC =  X20Y9" for instance <I_ABus_DFF> in unit <ALU_Bit70_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit70> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit71_>.
    Set user-defined property "RLOC =  X20Y10" for instance <I_ALU_LUT> in unit <ALU_Bit71_>.
    Set user-defined property "RLOC =  X20Y10" for instance <MULT_AND_I> in unit <ALU_Bit71_>.
    Set user-defined property "RLOC =  X20Y10" for instance <MUXCY_I> in unit <ALU_Bit71_>.
    Set user-defined property "RLOC =  X20Y10" for instance <XOR_I> in unit <ALU_Bit71_>.
    Set user-defined property "RLOC =  X20Y10" for instance <I_ABus_DFF> in unit <ALU_Bit71_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit71> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit72_>.
    Set user-defined property "RLOC =  X20Y11" for instance <I_ALU_LUT> in unit <ALU_Bit72_>.
    Set user-defined property "RLOC =  X20Y11" for instance <MULT_AND_I> in unit <ALU_Bit72_>.
    Set user-defined property "RLOC =  X20Y11" for instance <MUXCY_I> in unit <ALU_Bit72_>.
    Set user-defined property "RLOC =  X20Y11" for instance <XOR_I> in unit <ALU_Bit72_>.
    Set user-defined property "RLOC =  X20Y11" for instance <I_ABus_DFF> in unit <ALU_Bit72_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit72> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit73_>.
    Set user-defined property "RLOC =  X20Y12" for instance <I_ALU_LUT> in unit <ALU_Bit73_>.
    Set user-defined property "RLOC =  X20Y12" for instance <MULT_AND_I> in unit <ALU_Bit73_>.
    Set user-defined property "RLOC =  X20Y12" for instance <MUXCY_I> in unit <ALU_Bit73_>.
    Set user-defined property "RLOC =  X20Y12" for instance <XOR_I> in unit <ALU_Bit73_>.
    Set user-defined property "RLOC =  X20Y12" for instance <I_ABus_DFF> in unit <ALU_Bit73_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit73> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit74_>.
    Set user-defined property "RLOC =  X20Y13" for instance <I_ALU_LUT> in unit <ALU_Bit74_>.
    Set user-defined property "RLOC =  X20Y13" for instance <MULT_AND_I> in unit <ALU_Bit74_>.
    Set user-defined property "RLOC =  X20Y13" for instance <MUXCY_I> in unit <ALU_Bit74_>.
    Set user-defined property "RLOC =  X20Y13" for instance <XOR_I> in unit <ALU_Bit74_>.
    Set user-defined property "RLOC =  X20Y13" for instance <I_ABus_DFF> in unit <ALU_Bit74_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit74> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit75_>.
    Set user-defined property "RLOC =  X20Y14" for instance <I_ALU_LUT> in unit <ALU_Bit75_>.
    Set user-defined property "RLOC =  X20Y14" for instance <MULT_AND_I> in unit <ALU_Bit75_>.
    Set user-defined property "RLOC =  X20Y14" for instance <MUXCY_I> in unit <ALU_Bit75_>.
    Set user-defined property "RLOC =  X20Y14" for instance <XOR_I> in unit <ALU_Bit75_>.
    Set user-defined property "RLOC =  X20Y14" for instance <I_ABus_DFF> in unit <ALU_Bit75_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit75> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>0
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT> in unit <ALU_Bit76_>.
    Set user-defined property "RLOC =  X20Y15" for instance <I_ALU_LUT> in unit <ALU_Bit76_>.
    Set user-defined property "RLOC =  X20Y15" for instance <MULT_AND_I> in unit <ALU_Bit76_>.
    Set user-defined property "RLOC =  X20Y15" for instance <MUXCY_I> in unit <ALU_Bit76_>.
    Set user-defined property "RLOC =  X20Y15" for instance <XOR_I> in unit <ALU_Bit76_>.
    Set user-defined property "RLOC =  X20Y15" for instance <I_ABus_DFF> in unit <ALU_Bit76_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit76> generated.

Analyzing generic Entity <ALU_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 20
	C_U_SET = "microblaze_0"
	C_LAST_BIT = <u>1
    Set user-defined property "RLOC =  X20Y15" for instance <Pre_MUXCY_I> in unit <ALU_Bit77_>.
    Set user-defined property "INIT =  A678" for instance <I_ALU_LUT_1> in unit <ALU_Bit77_>.
    Set user-defined property "INIT =  FA0A" for instance <I_ALU_LUT_2> in unit <ALU_Bit77_>.
    Set user-defined property "RLOC =  X20Y16" for instance <I_ALU_LUT_2> in unit <ALU_Bit77_>.
    Set user-defined property "RLOC =  X20Y16" for instance <MULT_AND_I> in unit <ALU_Bit77_>.
    Set user-defined property "RLOC =  X20Y16" for instance <MUXCY_I> in unit <ALU_Bit77_>.
    Set user-defined property "RLOC =  X20Y16" for instance <XOR_I> in unit <ALU_Bit77_>.
    Set user-defined property "RLOC =  X20Y16" for instance <I_ABus_DFF> in unit <ALU_Bit77_>.
Entity <ALU_Bit> analyzed. Unit <ALU_Bit77> generated.

Analyzing generic Entity <Shift_Logic_Module> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I31> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I30> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I29> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I28> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I27> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I26> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I25> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I24> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I23> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I22> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I21> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I20> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I19> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I18> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I17> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I16> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I15> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I14> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I13> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I12> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I11> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I10> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I9> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I8> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I7> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I6> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I5> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I4> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I3> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I2> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I1> in unit <Shift_Logic_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Shift_Logic_Bit_I0> in unit <Shift_Logic_Module>.
Entity <Shift_Logic_Module> analyzed. Unit <Shift_Logic_Module> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit>.
    Set user-defined property "RLOC =  X21Y0" for instance <Shift_LUT> in unit <Shift_Logic_Bit>.
    Set user-defined property "RLOC =  X21Y0" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit78_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit78_>.
    Set user-defined property "RLOC =  X22Y0" for instance <Shift_LUT> in unit <Shift_Logic_Bit78_>.
    Set user-defined property "RLOC =  X22Y0" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit78_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit78> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit79_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit79_>.
    Set user-defined property "RLOC =  X21Y1" for instance <Shift_LUT> in unit <Shift_Logic_Bit79_>.
    Set user-defined property "RLOC =  X21Y1" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit79_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit79> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit80_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit80_>.
    Set user-defined property "RLOC =  X22Y1" for instance <Shift_LUT> in unit <Shift_Logic_Bit80_>.
    Set user-defined property "RLOC =  X22Y1" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit80_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit80> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit81_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit81_>.
    Set user-defined property "RLOC =  X21Y2" for instance <Shift_LUT> in unit <Shift_Logic_Bit81_>.
    Set user-defined property "RLOC =  X21Y2" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit81_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit81> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit82_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit82_>.
    Set user-defined property "RLOC =  X22Y2" for instance <Shift_LUT> in unit <Shift_Logic_Bit82_>.
    Set user-defined property "RLOC =  X22Y2" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit82_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit82> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit83_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit83_>.
    Set user-defined property "RLOC =  X21Y3" for instance <Shift_LUT> in unit <Shift_Logic_Bit83_>.
    Set user-defined property "RLOC =  X21Y3" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit83_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit83> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit84_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit84_>.
    Set user-defined property "RLOC =  X22Y3" for instance <Shift_LUT> in unit <Shift_Logic_Bit84_>.
    Set user-defined property "RLOC =  X22Y3" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit84_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit84> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit85_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit85_>.
    Set user-defined property "RLOC =  X21Y4" for instance <Shift_LUT> in unit <Shift_Logic_Bit85_>.
    Set user-defined property "RLOC =  X21Y4" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit85_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit85> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit86_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit86_>.
    Set user-defined property "RLOC =  X22Y4" for instance <Shift_LUT> in unit <Shift_Logic_Bit86_>.
    Set user-defined property "RLOC =  X22Y4" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit86_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit86> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit87_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit87_>.
    Set user-defined property "RLOC =  X21Y5" for instance <Shift_LUT> in unit <Shift_Logic_Bit87_>.
    Set user-defined property "RLOC =  X21Y5" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit87_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit87> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit88_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit88_>.
    Set user-defined property "RLOC =  X22Y5" for instance <Shift_LUT> in unit <Shift_Logic_Bit88_>.
    Set user-defined property "RLOC =  X22Y5" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit88_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit88> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit89_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit89_>.
    Set user-defined property "RLOC =  X21Y6" for instance <Shift_LUT> in unit <Shift_Logic_Bit89_>.
    Set user-defined property "RLOC =  X21Y6" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit89_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit89> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit90_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit90_>.
    Set user-defined property "RLOC =  X22Y6" for instance <Shift_LUT> in unit <Shift_Logic_Bit90_>.
    Set user-defined property "RLOC =  X22Y6" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit90_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit90> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit91_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit91_>.
    Set user-defined property "RLOC =  X21Y7" for instance <Shift_LUT> in unit <Shift_Logic_Bit91_>.
    Set user-defined property "RLOC =  X21Y7" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit91_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit91> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit92_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit92_>.
    Set user-defined property "RLOC =  X22Y7" for instance <Shift_LUT> in unit <Shift_Logic_Bit92_>.
    Set user-defined property "RLOC =  X22Y7" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit92_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit92> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit93_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit93_>.
    Set user-defined property "RLOC =  X21Y8" for instance <Shift_LUT> in unit <Shift_Logic_Bit93_>.
    Set user-defined property "RLOC =  X21Y8" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit93_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit93> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit94_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit94_>.
    Set user-defined property "RLOC =  X22Y8" for instance <Shift_LUT> in unit <Shift_Logic_Bit94_>.
    Set user-defined property "RLOC =  X22Y8" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit94_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit94> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit95_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit95_>.
    Set user-defined property "RLOC =  X21Y9" for instance <Shift_LUT> in unit <Shift_Logic_Bit95_>.
    Set user-defined property "RLOC =  X21Y9" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit95_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit95> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit96_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit96_>.
    Set user-defined property "RLOC =  X22Y9" for instance <Shift_LUT> in unit <Shift_Logic_Bit96_>.
    Set user-defined property "RLOC =  X22Y9" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit96_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit96> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit97_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit97_>.
    Set user-defined property "RLOC =  X21Y10" for instance <Shift_LUT> in unit <Shift_Logic_Bit97_>.
    Set user-defined property "RLOC =  X21Y10" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit97_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit97> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit98_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit98_>.
    Set user-defined property "RLOC =  X22Y10" for instance <Shift_LUT> in unit <Shift_Logic_Bit98_>.
    Set user-defined property "RLOC =  X22Y10" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit98_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit98> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit99_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit99_>.
    Set user-defined property "RLOC =  X21Y11" for instance <Shift_LUT> in unit <Shift_Logic_Bit99_>.
    Set user-defined property "RLOC =  X21Y11" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit99_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit99> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit100_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit100_>.
    Set user-defined property "RLOC =  X22Y11" for instance <Shift_LUT> in unit <Shift_Logic_Bit100_>.
    Set user-defined property "RLOC =  X22Y11" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit100_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit100> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit101_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit101_>.
    Set user-defined property "RLOC =  X21Y12" for instance <Shift_LUT> in unit <Shift_Logic_Bit101_>.
    Set user-defined property "RLOC =  X21Y12" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit101_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit101> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit102_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit102_>.
    Set user-defined property "RLOC =  X22Y12" for instance <Shift_LUT> in unit <Shift_Logic_Bit102_>.
    Set user-defined property "RLOC =  X22Y12" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit102_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit102> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit103_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit103_>.
    Set user-defined property "RLOC =  X21Y13" for instance <Shift_LUT> in unit <Shift_Logic_Bit103_>.
    Set user-defined property "RLOC =  X21Y13" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit103_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit103> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit104_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit104_>.
    Set user-defined property "RLOC =  X22Y13" for instance <Shift_LUT> in unit <Shift_Logic_Bit104_>.
    Set user-defined property "RLOC =  X22Y13" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit104_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit104> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit105_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit105_>.
    Set user-defined property "RLOC =  X21Y14" for instance <Shift_LUT> in unit <Shift_Logic_Bit105_>.
    Set user-defined property "RLOC =  X21Y14" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit105_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit105> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit106_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit106_>.
    Set user-defined property "RLOC =  X22Y14" for instance <Shift_LUT> in unit <Shift_Logic_Bit106_>.
    Set user-defined property "RLOC =  X22Y14" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit106_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit106> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 21
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit107_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit107_>.
    Set user-defined property "RLOC =  X21Y15" for instance <Shift_LUT> in unit <Shift_Logic_Bit107_>.
    Set user-defined property "RLOC =  X21Y15" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit107_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit107> generated.

Analyzing generic Entity <Shift_Logic_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 22
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  468E" for instance <Logic_LUT> in unit <Shift_Logic_Bit108_>.
    Set user-defined property "INIT =  FCAA" for instance <Shift_LUT> in unit <Shift_Logic_Bit108_>.
    Set user-defined property "RLOC =  X22Y15" for instance <Shift_LUT> in unit <Shift_Logic_Bit108_>.
    Set user-defined property "RLOC =  X22Y15" for instance <Shift_Logic_Mux> in unit <Shift_Logic_Bit108_>.
Entity <Shift_Logic_Bit> analyzed. Unit <Shift_Logic_Bit108> generated.

Analyzing generic Entity <MUL_Unit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_DATA_SIZE = 32
Entity <MUL_Unit> analyzed. Unit <MUL_Unit> generated.

Analyzing generic Entity <Result_Mux> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I31> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I30> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I29> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I28> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I27> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I26> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I25> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I24> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I23> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I22> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I21> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I20> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I19> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I18> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I17> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I16> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I15> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I14> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I13> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I12> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I11> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I10> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I9> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I8> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I7> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I6> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I5> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I4> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I3> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I2> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I1> in unit <Result_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Result_Mux_Bit_I0> in unit <Result_Mux>.
Entity <Result_Mux> analyzed. Unit <Result_Mux> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit>.
    Set user-defined property "RLOC =  X18Y0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit>.
    Set user-defined property "RLOC =  X18Y0" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit>.
    Set user-defined property "RLOC =  X18Y0" for instance <Result_MUXF5> in unit <Result_Mux_Bit>.
    Set user-defined property "RLOC =  X18Y0" for instance <EX_Result_DFF> in unit <Result_Mux_Bit>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit109_>.
    Set user-defined property "RLOC =  X19Y0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit109_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit109_>.
    Set user-defined property "RLOC =  X19Y0" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit109_>.
    Set user-defined property "RLOC =  X19Y0" for instance <Result_MUXF5> in unit <Result_Mux_Bit109_>.
    Set user-defined property "RLOC =  X19Y0" for instance <EX_Result_DFF> in unit <Result_Mux_Bit109_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit109> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit110_>.
    Set user-defined property "RLOC =  X18Y1" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit110_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit110_>.
    Set user-defined property "RLOC =  X18Y1" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit110_>.
    Set user-defined property "RLOC =  X18Y1" for instance <Result_MUXF5> in unit <Result_Mux_Bit110_>.
    Set user-defined property "RLOC =  X18Y1" for instance <EX_Result_DFF> in unit <Result_Mux_Bit110_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit110> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit111_>.
    Set user-defined property "RLOC =  X19Y1" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit111_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit111_>.
    Set user-defined property "RLOC =  X19Y1" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit111_>.
    Set user-defined property "RLOC =  X19Y1" for instance <Result_MUXF5> in unit <Result_Mux_Bit111_>.
    Set user-defined property "RLOC =  X19Y1" for instance <EX_Result_DFF> in unit <Result_Mux_Bit111_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit111> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit112_>.
    Set user-defined property "RLOC =  X18Y2" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit112_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit112_>.
    Set user-defined property "RLOC =  X18Y2" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit112_>.
    Set user-defined property "RLOC =  X18Y2" for instance <Result_MUXF5> in unit <Result_Mux_Bit112_>.
    Set user-defined property "RLOC =  X18Y2" for instance <EX_Result_DFF> in unit <Result_Mux_Bit112_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit112> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit113_>.
    Set user-defined property "RLOC =  X19Y2" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit113_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit113_>.
    Set user-defined property "RLOC =  X19Y2" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit113_>.
    Set user-defined property "RLOC =  X19Y2" for instance <Result_MUXF5> in unit <Result_Mux_Bit113_>.
    Set user-defined property "RLOC =  X19Y2" for instance <EX_Result_DFF> in unit <Result_Mux_Bit113_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit113> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit114_>.
    Set user-defined property "RLOC =  X18Y3" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit114_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit114_>.
    Set user-defined property "RLOC =  X18Y3" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit114_>.
    Set user-defined property "RLOC =  X18Y3" for instance <Result_MUXF5> in unit <Result_Mux_Bit114_>.
    Set user-defined property "RLOC =  X18Y3" for instance <EX_Result_DFF> in unit <Result_Mux_Bit114_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit114> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit115_>.
    Set user-defined property "RLOC =  X19Y3" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit115_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit115_>.
    Set user-defined property "RLOC =  X19Y3" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit115_>.
    Set user-defined property "RLOC =  X19Y3" for instance <Result_MUXF5> in unit <Result_Mux_Bit115_>.
    Set user-defined property "RLOC =  X19Y3" for instance <EX_Result_DFF> in unit <Result_Mux_Bit115_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit115> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit116_>.
    Set user-defined property "RLOC =  X18Y4" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit116_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit116_>.
    Set user-defined property "RLOC =  X18Y4" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit116_>.
    Set user-defined property "RLOC =  X18Y4" for instance <Result_MUXF5> in unit <Result_Mux_Bit116_>.
    Set user-defined property "RLOC =  X18Y4" for instance <EX_Result_DFF> in unit <Result_Mux_Bit116_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit116> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit117_>.
    Set user-defined property "RLOC =  X19Y4" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit117_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit117_>.
    Set user-defined property "RLOC =  X19Y4" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit117_>.
    Set user-defined property "RLOC =  X19Y4" for instance <Result_MUXF5> in unit <Result_Mux_Bit117_>.
    Set user-defined property "RLOC =  X19Y4" for instance <EX_Result_DFF> in unit <Result_Mux_Bit117_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit117> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit118_>.
    Set user-defined property "RLOC =  X18Y5" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit118_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit118_>.
    Set user-defined property "RLOC =  X18Y5" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit118_>.
    Set user-defined property "RLOC =  X18Y5" for instance <Result_MUXF5> in unit <Result_Mux_Bit118_>.
    Set user-defined property "RLOC =  X18Y5" for instance <EX_Result_DFF> in unit <Result_Mux_Bit118_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit118> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit119_>.
    Set user-defined property "RLOC =  X19Y5" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit119_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit119_>.
    Set user-defined property "RLOC =  X19Y5" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit119_>.
    Set user-defined property "RLOC =  X19Y5" for instance <Result_MUXF5> in unit <Result_Mux_Bit119_>.
    Set user-defined property "RLOC =  X19Y5" for instance <EX_Result_DFF> in unit <Result_Mux_Bit119_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit119> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit120_>.
    Set user-defined property "RLOC =  X18Y6" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit120_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit120_>.
    Set user-defined property "RLOC =  X18Y6" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit120_>.
    Set user-defined property "RLOC =  X18Y6" for instance <Result_MUXF5> in unit <Result_Mux_Bit120_>.
    Set user-defined property "RLOC =  X18Y6" for instance <EX_Result_DFF> in unit <Result_Mux_Bit120_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit120> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit121_>.
    Set user-defined property "RLOC =  X19Y6" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit121_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit121_>.
    Set user-defined property "RLOC =  X19Y6" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit121_>.
    Set user-defined property "RLOC =  X19Y6" for instance <Result_MUXF5> in unit <Result_Mux_Bit121_>.
    Set user-defined property "RLOC =  X19Y6" for instance <EX_Result_DFF> in unit <Result_Mux_Bit121_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit121> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit122_>.
    Set user-defined property "RLOC =  X18Y7" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit122_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit122_>.
    Set user-defined property "RLOC =  X18Y7" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit122_>.
    Set user-defined property "RLOC =  X18Y7" for instance <Result_MUXF5> in unit <Result_Mux_Bit122_>.
    Set user-defined property "RLOC =  X18Y7" for instance <EX_Result_DFF> in unit <Result_Mux_Bit122_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit122> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit123_>.
    Set user-defined property "RLOC =  X19Y7" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit123_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit123_>.
    Set user-defined property "RLOC =  X19Y7" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit123_>.
    Set user-defined property "RLOC =  X19Y7" for instance <Result_MUXF5> in unit <Result_Mux_Bit123_>.
    Set user-defined property "RLOC =  X19Y7" for instance <EX_Result_DFF> in unit <Result_Mux_Bit123_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit123> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit124_>.
    Set user-defined property "RLOC =  X18Y8" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit124_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit124_>.
    Set user-defined property "RLOC =  X18Y8" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit124_>.
    Set user-defined property "RLOC =  X18Y8" for instance <Result_MUXF5> in unit <Result_Mux_Bit124_>.
    Set user-defined property "RLOC =  X18Y8" for instance <EX_Result_DFF> in unit <Result_Mux_Bit124_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit124> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit125_>.
    Set user-defined property "RLOC =  X19Y8" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit125_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit125_>.
    Set user-defined property "RLOC =  X19Y8" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit125_>.
    Set user-defined property "RLOC =  X19Y8" for instance <Result_MUXF5> in unit <Result_Mux_Bit125_>.
    Set user-defined property "RLOC =  X19Y8" for instance <EX_Result_DFF> in unit <Result_Mux_Bit125_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit125> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit126_>.
    Set user-defined property "RLOC =  X18Y9" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit126_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit126_>.
    Set user-defined property "RLOC =  X18Y9" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit126_>.
    Set user-defined property "RLOC =  X18Y9" for instance <Result_MUXF5> in unit <Result_Mux_Bit126_>.
    Set user-defined property "RLOC =  X18Y9" for instance <EX_Result_DFF> in unit <Result_Mux_Bit126_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit126> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit127_>.
    Set user-defined property "RLOC =  X19Y9" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit127_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit127_>.
    Set user-defined property "RLOC =  X19Y9" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit127_>.
    Set user-defined property "RLOC =  X19Y9" for instance <Result_MUXF5> in unit <Result_Mux_Bit127_>.
    Set user-defined property "RLOC =  X19Y9" for instance <EX_Result_DFF> in unit <Result_Mux_Bit127_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit127> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit128_>.
    Set user-defined property "RLOC =  X18Y10" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit128_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit128_>.
    Set user-defined property "RLOC =  X18Y10" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit128_>.
    Set user-defined property "RLOC =  X18Y10" for instance <Result_MUXF5> in unit <Result_Mux_Bit128_>.
    Set user-defined property "RLOC =  X18Y10" for instance <EX_Result_DFF> in unit <Result_Mux_Bit128_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit128> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit129_>.
    Set user-defined property "RLOC =  X19Y10" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit129_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit129_>.
    Set user-defined property "RLOC =  X19Y10" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit129_>.
    Set user-defined property "RLOC =  X19Y10" for instance <Result_MUXF5> in unit <Result_Mux_Bit129_>.
    Set user-defined property "RLOC =  X19Y10" for instance <EX_Result_DFF> in unit <Result_Mux_Bit129_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit129> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit130_>.
    Set user-defined property "RLOC =  X18Y11" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit130_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit130_>.
    Set user-defined property "RLOC =  X18Y11" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit130_>.
    Set user-defined property "RLOC =  X18Y11" for instance <Result_MUXF5> in unit <Result_Mux_Bit130_>.
    Set user-defined property "RLOC =  X18Y11" for instance <EX_Result_DFF> in unit <Result_Mux_Bit130_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit130> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit131_>.
    Set user-defined property "RLOC =  X19Y11" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit131_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit131_>.
    Set user-defined property "RLOC =  X19Y11" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit131_>.
    Set user-defined property "RLOC =  X19Y11" for instance <Result_MUXF5> in unit <Result_Mux_Bit131_>.
    Set user-defined property "RLOC =  X19Y11" for instance <EX_Result_DFF> in unit <Result_Mux_Bit131_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit131> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit132_>.
    Set user-defined property "RLOC =  X18Y12" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit132_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit132_>.
    Set user-defined property "RLOC =  X18Y12" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit132_>.
    Set user-defined property "RLOC =  X18Y12" for instance <Result_MUXF5> in unit <Result_Mux_Bit132_>.
    Set user-defined property "RLOC =  X18Y12" for instance <EX_Result_DFF> in unit <Result_Mux_Bit132_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit132> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit133_>.
    Set user-defined property "RLOC =  X19Y12" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit133_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit133_>.
    Set user-defined property "RLOC =  X19Y12" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit133_>.
    Set user-defined property "RLOC =  X19Y12" for instance <Result_MUXF5> in unit <Result_Mux_Bit133_>.
    Set user-defined property "RLOC =  X19Y12" for instance <EX_Result_DFF> in unit <Result_Mux_Bit133_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit133> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit134_>.
    Set user-defined property "RLOC =  X18Y13" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit134_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit134_>.
    Set user-defined property "RLOC =  X18Y13" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit134_>.
    Set user-defined property "RLOC =  X18Y13" for instance <Result_MUXF5> in unit <Result_Mux_Bit134_>.
    Set user-defined property "RLOC =  X18Y13" for instance <EX_Result_DFF> in unit <Result_Mux_Bit134_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit134> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit135_>.
    Set user-defined property "RLOC =  X19Y13" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit135_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit135_>.
    Set user-defined property "RLOC =  X19Y13" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit135_>.
    Set user-defined property "RLOC =  X19Y13" for instance <Result_MUXF5> in unit <Result_Mux_Bit135_>.
    Set user-defined property "RLOC =  X19Y13" for instance <EX_Result_DFF> in unit <Result_Mux_Bit135_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit135> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit136_>.
    Set user-defined property "RLOC =  X18Y14" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit136_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit136_>.
    Set user-defined property "RLOC =  X18Y14" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit136_>.
    Set user-defined property "RLOC =  X18Y14" for instance <Result_MUXF5> in unit <Result_Mux_Bit136_>.
    Set user-defined property "RLOC =  X18Y14" for instance <EX_Result_DFF> in unit <Result_Mux_Bit136_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit136> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit137_>.
    Set user-defined property "RLOC =  X19Y14" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit137_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit137_>.
    Set user-defined property "RLOC =  X19Y14" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit137_>.
    Set user-defined property "RLOC =  X19Y14" for instance <Result_MUXF5> in unit <Result_Mux_Bit137_>.
    Set user-defined property "RLOC =  X19Y14" for instance <EX_Result_DFF> in unit <Result_Mux_Bit137_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit137> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 18
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit138_>.
    Set user-defined property "RLOC =  X18Y15" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit138_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit138_>.
    Set user-defined property "RLOC =  X18Y15" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit138_>.
    Set user-defined property "RLOC =  X18Y15" for instance <Result_MUXF5> in unit <Result_Mux_Bit138_>.
    Set user-defined property "RLOC =  X18Y15" for instance <EX_Result_DFF> in unit <Result_Mux_Bit138_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit138> generated.

Analyzing generic Entity <Result_Mux_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 19
	C_U_SET = "microblaze_0"
    Set user-defined property "INIT =  EFE0" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit139_>.
    Set user-defined property "RLOC =  X19Y15" for instance <Mul_ALU_Mux> in unit <Result_Mux_Bit139_>.
    Set user-defined property "INIT =  E040" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit139_>.
    Set user-defined property "RLOC =  X19Y15" for instance <Data_Shift_Mux> in unit <Result_Mux_Bit139_>.
    Set user-defined property "RLOC =  X19Y15" for instance <Result_MUXF5> in unit <Result_Mux_Bit139_>.
    Set user-defined property "RLOC =  X19Y15" for instance <EX_Result_DFF> in unit <Result_Mux_Bit139_>.
Entity <Result_Mux_Bit> analyzed. Unit <Result_Mux_Bit139> generated.

Analyzing generic Entity <Zero_Detect> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "U_SET =  microblaze_0" for instance <Part_Of_Zero_Carry_Start> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y8" for instance <Part_Of_Zero_Carry_Start> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect0> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y8" for instance <I_Part_Of_Zero_Detect0> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect1> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y9" for instance <I_Part_Of_Zero_Detect1> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect2> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y9" for instance <I_Part_Of_Zero_Detect2> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect3> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y10" for instance <I_Part_Of_Zero_Detect3> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect4> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y10" for instance <I_Part_Of_Zero_Detect4> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect5> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y11" for instance <I_Part_Of_Zero_Detect5> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect6> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y11" for instance <I_Part_Of_Zero_Detect6> in unit <Zero_Detect>.
    Set user-defined property "U_SET =  microblaze_0" for instance <I_Part_Of_Zero_Detect7> in unit <Zero_Detect>.
    Set user-defined property "RLOC =  X23Y12" for instance <I_Part_Of_Zero_Detect7> in unit <Zero_Detect>.
Entity <Zero_Detect> analyzed. Unit <Zero_Detect> generated.

Analyzing generic Entity <MSR_Reg> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_USE_MSR_INSTR = 0
	C_USE_EXCEPTIONS = <u>0
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I9> in unit <MSR_Reg>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I8> in unit <MSR_Reg>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I7> in unit <MSR_Reg>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I6> in unit <MSR_Reg>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I5> in unit <MSR_Reg>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I4> in unit <MSR_Reg>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I3> in unit <MSR_Reg>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MSR_Reg_Bit_I2> in unit <MSR_Reg>.
Entity <MSR_Reg> analyzed. Unit <MSR_Reg> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 10
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 11
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit140> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 12
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit141> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 13
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit142> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 14
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit143> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 15
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit144> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 16
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit145> generated.

Analyzing generic Entity <MSR_Reg_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 16
	C_X = 17
	C_U_SET = "microblaze_0"
Entity <MSR_Reg_Bit> analyzed. Unit <MSR_Reg_Bit146> generated.

Analyzing generic Entity <PC_Module> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_PC_START_ADDR = "00000000"
    Set user-defined property "USELOWSKEWLINES =  yes" for signal <pc_write_I>.
    Set property "MAX_FANOUT = 1000" for signal <pc_write_I>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I31> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I30> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I29> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I28> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I27> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I26> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I25> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I24> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I23> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I22> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I21> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I20> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I19> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I18> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I17> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I16> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I15> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I14> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I13> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I12> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I11> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I10> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I9> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I8> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I7> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I6> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I5> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I4> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I3> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I2> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I1> in unit <PC_Module>.
    Set user-defined property "U_SET =  microblaze_0" for instance <PC_Bit_I0> in unit <PC_Module>.
Entity <PC_Module> analyzed. Unit <PC_Module> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>0
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit>.
    Set user-defined property "RLOC =  X26Y0" for instance <Sum_I> in unit <PC_Bit>.
    Set user-defined property "RLOC =  X26Y0" for instance <MUXCY_X> in unit <PC_Bit>.
    Set user-defined property "RLOC =  X26Y0" for instance <XOR_X> in unit <PC_Bit>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit>.
    Set user-defined property "RLOC =  X27Y0" for instance <NewPC_Mux> in unit <PC_Bit>.
    Set user-defined property "RLOC =  X27Y0" for instance <PC_IF_DFF> in unit <PC_Bit>.
    Set user-defined property "RLOC =  X28Y0" for instance <PC_OF_Buffer> in unit <PC_Bit>.
    Set user-defined property "RLOC =  X28Y0" for instance <PC_EX_DFF> in unit <PC_Bit>.
Entity <PC_Bit> analyzed. Unit <PC_Bit> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 1
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit147_>.
    Set user-defined property "RLOC =  X26Y1" for instance <Sum_I> in unit <PC_Bit147_>.
    Set user-defined property "RLOC =  X26Y1" for instance <MUXCY_X> in unit <PC_Bit147_>.
    Set user-defined property "RLOC =  X26Y1" for instance <XOR_X> in unit <PC_Bit147_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit147_>.
    Set user-defined property "RLOC =  X27Y1" for instance <NewPC_Mux> in unit <PC_Bit147_>.
    Set user-defined property "RLOC =  X27Y1" for instance <PC_IF_DFF> in unit <PC_Bit147_>.
    Set user-defined property "RLOC =  X28Y1" for instance <PC_OF_Buffer> in unit <PC_Bit147_>.
    Set user-defined property "RLOC =  X28Y1" for instance <PC_EX_DFF> in unit <PC_Bit147_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit147> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 2
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit148_>.
    Set user-defined property "RLOC =  X26Y2" for instance <Sum_I> in unit <PC_Bit148_>.
    Set user-defined property "RLOC =  X26Y2" for instance <MUXCY_X> in unit <PC_Bit148_>.
    Set user-defined property "RLOC =  X26Y2" for instance <XOR_X> in unit <PC_Bit148_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit148_>.
    Set user-defined property "RLOC =  X27Y2" for instance <NewPC_Mux> in unit <PC_Bit148_>.
    Set user-defined property "RLOC =  X27Y2" for instance <PC_IF_DFF> in unit <PC_Bit148_>.
    Set user-defined property "RLOC =  X28Y2" for instance <PC_OF_Buffer> in unit <PC_Bit148_>.
    Set user-defined property "RLOC =  X28Y2" for instance <PC_EX_DFF> in unit <PC_Bit148_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit148> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 3
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit149_>.
    Set user-defined property "RLOC =  X26Y3" for instance <Sum_I> in unit <PC_Bit149_>.
    Set user-defined property "RLOC =  X26Y3" for instance <MUXCY_X> in unit <PC_Bit149_>.
    Set user-defined property "RLOC =  X26Y3" for instance <XOR_X> in unit <PC_Bit149_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit149_>.
    Set user-defined property "RLOC =  X27Y3" for instance <NewPC_Mux> in unit <PC_Bit149_>.
    Set user-defined property "RLOC =  X27Y3" for instance <PC_IF_DFF> in unit <PC_Bit149_>.
    Set user-defined property "RLOC =  X28Y3" for instance <PC_OF_Buffer> in unit <PC_Bit149_>.
    Set user-defined property "RLOC =  X28Y3" for instance <PC_EX_DFF> in unit <PC_Bit149_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit149> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit150_>.
    Set user-defined property "RLOC =  X26Y4" for instance <Sum_I> in unit <PC_Bit150_>.
    Set user-defined property "RLOC =  X26Y4" for instance <MUXCY_X> in unit <PC_Bit150_>.
    Set user-defined property "RLOC =  X26Y4" for instance <XOR_X> in unit <PC_Bit150_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit150_>.
    Set user-defined property "RLOC =  X27Y4" for instance <NewPC_Mux> in unit <PC_Bit150_>.
    Set user-defined property "RLOC =  X27Y4" for instance <PC_IF_DFF> in unit <PC_Bit150_>.
    Set user-defined property "RLOC =  X28Y4" for instance <PC_OF_Buffer> in unit <PC_Bit150_>.
    Set user-defined property "RLOC =  X28Y4" for instance <PC_EX_DFF> in unit <PC_Bit150_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit150> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 5
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit151_>.
    Set user-defined property "RLOC =  X26Y5" for instance <Sum_I> in unit <PC_Bit151_>.
    Set user-defined property "RLOC =  X26Y5" for instance <MUXCY_X> in unit <PC_Bit151_>.
    Set user-defined property "RLOC =  X26Y5" for instance <XOR_X> in unit <PC_Bit151_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit151_>.
    Set user-defined property "RLOC =  X27Y5" for instance <NewPC_Mux> in unit <PC_Bit151_>.
    Set user-defined property "RLOC =  X27Y5" for instance <PC_IF_DFF> in unit <PC_Bit151_>.
    Set user-defined property "RLOC =  X28Y5" for instance <PC_OF_Buffer> in unit <PC_Bit151_>.
    Set user-defined property "RLOC =  X28Y5" for instance <PC_EX_DFF> in unit <PC_Bit151_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit151> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 6
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit152_>.
    Set user-defined property "RLOC =  X26Y6" for instance <Sum_I> in unit <PC_Bit152_>.
    Set user-defined property "RLOC =  X26Y6" for instance <MUXCY_X> in unit <PC_Bit152_>.
    Set user-defined property "RLOC =  X26Y6" for instance <XOR_X> in unit <PC_Bit152_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit152_>.
    Set user-defined property "RLOC =  X27Y6" for instance <NewPC_Mux> in unit <PC_Bit152_>.
    Set user-defined property "RLOC =  X27Y6" for instance <PC_IF_DFF> in unit <PC_Bit152_>.
    Set user-defined property "RLOC =  X28Y6" for instance <PC_OF_Buffer> in unit <PC_Bit152_>.
    Set user-defined property "RLOC =  X28Y6" for instance <PC_EX_DFF> in unit <PC_Bit152_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit152> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 7
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit153_>.
    Set user-defined property "RLOC =  X26Y7" for instance <Sum_I> in unit <PC_Bit153_>.
    Set user-defined property "RLOC =  X26Y7" for instance <MUXCY_X> in unit <PC_Bit153_>.
    Set user-defined property "RLOC =  X26Y7" for instance <XOR_X> in unit <PC_Bit153_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit153_>.
    Set user-defined property "RLOC =  X27Y7" for instance <NewPC_Mux> in unit <PC_Bit153_>.
    Set user-defined property "RLOC =  X27Y7" for instance <PC_IF_DFF> in unit <PC_Bit153_>.
    Set user-defined property "RLOC =  X28Y7" for instance <PC_OF_Buffer> in unit <PC_Bit153_>.
    Set user-defined property "RLOC =  X28Y7" for instance <PC_EX_DFF> in unit <PC_Bit153_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit153> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 8
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit154_>.
    Set user-defined property "RLOC =  X26Y8" for instance <Sum_I> in unit <PC_Bit154_>.
    Set user-defined property "RLOC =  X26Y8" for instance <MUXCY_X> in unit <PC_Bit154_>.
    Set user-defined property "RLOC =  X26Y8" for instance <XOR_X> in unit <PC_Bit154_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit154_>.
    Set user-defined property "RLOC =  X27Y8" for instance <NewPC_Mux> in unit <PC_Bit154_>.
    Set user-defined property "RLOC =  X27Y8" for instance <PC_IF_DFF> in unit <PC_Bit154_>.
    Set user-defined property "RLOC =  X28Y8" for instance <PC_OF_Buffer> in unit <PC_Bit154_>.
    Set user-defined property "RLOC =  X28Y8" for instance <PC_EX_DFF> in unit <PC_Bit154_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit154> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 9
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit155_>.
    Set user-defined property "RLOC =  X26Y9" for instance <Sum_I> in unit <PC_Bit155_>.
    Set user-defined property "RLOC =  X26Y9" for instance <MUXCY_X> in unit <PC_Bit155_>.
    Set user-defined property "RLOC =  X26Y9" for instance <XOR_X> in unit <PC_Bit155_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit155_>.
    Set user-defined property "RLOC =  X27Y9" for instance <NewPC_Mux> in unit <PC_Bit155_>.
    Set user-defined property "RLOC =  X27Y9" for instance <PC_IF_DFF> in unit <PC_Bit155_>.
    Set user-defined property "RLOC =  X28Y9" for instance <PC_OF_Buffer> in unit <PC_Bit155_>.
    Set user-defined property "RLOC =  X28Y9" for instance <PC_EX_DFF> in unit <PC_Bit155_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit155> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 10
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit156_>.
    Set user-defined property "RLOC =  X26Y10" for instance <Sum_I> in unit <PC_Bit156_>.
    Set user-defined property "RLOC =  X26Y10" for instance <MUXCY_X> in unit <PC_Bit156_>.
    Set user-defined property "RLOC =  X26Y10" for instance <XOR_X> in unit <PC_Bit156_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit156_>.
    Set user-defined property "RLOC =  X27Y10" for instance <NewPC_Mux> in unit <PC_Bit156_>.
    Set user-defined property "RLOC =  X27Y10" for instance <PC_IF_DFF> in unit <PC_Bit156_>.
    Set user-defined property "RLOC =  X28Y10" for instance <PC_OF_Buffer> in unit <PC_Bit156_>.
    Set user-defined property "RLOC =  X28Y10" for instance <PC_EX_DFF> in unit <PC_Bit156_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit156> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 11
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit157_>.
    Set user-defined property "RLOC =  X26Y11" for instance <Sum_I> in unit <PC_Bit157_>.
    Set user-defined property "RLOC =  X26Y11" for instance <MUXCY_X> in unit <PC_Bit157_>.
    Set user-defined property "RLOC =  X26Y11" for instance <XOR_X> in unit <PC_Bit157_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit157_>.
    Set user-defined property "RLOC =  X27Y11" for instance <NewPC_Mux> in unit <PC_Bit157_>.
    Set user-defined property "RLOC =  X27Y11" for instance <PC_IF_DFF> in unit <PC_Bit157_>.
    Set user-defined property "RLOC =  X28Y11" for instance <PC_OF_Buffer> in unit <PC_Bit157_>.
    Set user-defined property "RLOC =  X28Y11" for instance <PC_EX_DFF> in unit <PC_Bit157_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit157> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit158_>.
    Set user-defined property "RLOC =  X26Y12" for instance <Sum_I> in unit <PC_Bit158_>.
    Set user-defined property "RLOC =  X26Y12" for instance <MUXCY_X> in unit <PC_Bit158_>.
    Set user-defined property "RLOC =  X26Y12" for instance <XOR_X> in unit <PC_Bit158_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit158_>.
    Set user-defined property "RLOC =  X27Y12" for instance <NewPC_Mux> in unit <PC_Bit158_>.
    Set user-defined property "RLOC =  X27Y12" for instance <PC_IF_DFF> in unit <PC_Bit158_>.
    Set user-defined property "RLOC =  X28Y12" for instance <PC_OF_Buffer> in unit <PC_Bit158_>.
    Set user-defined property "RLOC =  X28Y12" for instance <PC_EX_DFF> in unit <PC_Bit158_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit158> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 13
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit159_>.
    Set user-defined property "RLOC =  X26Y13" for instance <Sum_I> in unit <PC_Bit159_>.
    Set user-defined property "RLOC =  X26Y13" for instance <MUXCY_X> in unit <PC_Bit159_>.
    Set user-defined property "RLOC =  X26Y13" for instance <XOR_X> in unit <PC_Bit159_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit159_>.
    Set user-defined property "RLOC =  X27Y13" for instance <NewPC_Mux> in unit <PC_Bit159_>.
    Set user-defined property "RLOC =  X27Y13" for instance <PC_IF_DFF> in unit <PC_Bit159_>.
    Set user-defined property "RLOC =  X28Y13" for instance <PC_OF_Buffer> in unit <PC_Bit159_>.
    Set user-defined property "RLOC =  X28Y13" for instance <PC_EX_DFF> in unit <PC_Bit159_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit159> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 14
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit160_>.
    Set user-defined property "RLOC =  X26Y14" for instance <Sum_I> in unit <PC_Bit160_>.
    Set user-defined property "RLOC =  X26Y14" for instance <MUXCY_X> in unit <PC_Bit160_>.
    Set user-defined property "RLOC =  X26Y14" for instance <XOR_X> in unit <PC_Bit160_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit160_>.
    Set user-defined property "RLOC =  X27Y14" for instance <NewPC_Mux> in unit <PC_Bit160_>.
    Set user-defined property "RLOC =  X27Y14" for instance <PC_IF_DFF> in unit <PC_Bit160_>.
    Set user-defined property "RLOC =  X28Y14" for instance <PC_OF_Buffer> in unit <PC_Bit160_>.
    Set user-defined property "RLOC =  X28Y14" for instance <PC_EX_DFF> in unit <PC_Bit160_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit160> generated.

Analyzing generic Entity <PC_Bit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 15
	C_X = 26
	C_U_SET = "microblaze_0"
	C_RESET_VALUE = <u>1
    Set user-defined property "INIT =  F066" for instance <Sum_I> in unit <PC_Bit161_>.
    Set user-defined property "RLOC =  X26Y15" for instance <Sum_I> in unit <PC_Bit161_>.
    Set user-defined property "RLOC =  X26Y15" for instance <MUXCY_X> in unit <PC_Bit161_>.
    Set user-defined property "RLOC =  X26Y15" for instance <XOR_X> in unit <PC_Bit161_>.
    Set user-defined property "INIT =  AACA" for instance <NewPC_Mux> in unit <PC_Bit161_>.
    Set user-defined property "RLOC =  X27Y15" for instance <NewPC_Mux> in unit <PC_Bit161_>.
    Set user-defined property "RLOC =  X27Y15" for instance <PC_IF_DFF> in unit <PC_Bit161_>.
    Set user-defined property "RLOC =  X28Y15" for instance <PC_OF_Buffer> in unit <PC_Bit161_>.
    Set user-defined property "RLOC =  X28Y15" for instance <PC_EX_DFF> in unit <PC_Bit161_>.
Entity <PC_Bit> analyzed. Unit <PC_Bit161> generated.

Analyzing generic Entity <Byte_Doublet_Handle> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_DYNAMIC_BUS_SIZING = <u>1
	C_D_OPB = 1
	C_OPB_WIDTH = 32
	C_DATA_SIZE = 32
    Set user-defined property "U_SET =  microblaze_0" for instance <BYTE_0_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <BYTE_1_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <BYTE_2_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <BYTE_3_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "RLOC =  X29Y0" for instance <READ_SEL_LEFT_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <READ_SEL_LEFT_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "RLOC =  X29Y1" for instance <READ_SEL_RIGHT_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <READ_SEL_RIGHT_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "RLOC =  X29Y2" for instance <WRITE_MSB_SEL_LEFT_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <WRITE_MSB_SEL_LEFT_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LOW_ADDR_OUT_LEFT_I> in unit <Byte_Doublet_Handle>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LOW_ADDR_OUT_RIGHT_I> in unit <Byte_Doublet_Handle>.
Entity <Byte_Doublet_Handle> analyzed. Unit <Byte_Doublet_Handle> generated.

Analyzing generic Entity <Data_Read_Steering> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X17Y0" for instance <LUT30_I0> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I0> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y0" for instance <LUT31_I0> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I0> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y0" for instance <MUXF5_I0> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I0> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y1" for instance <LUT30_I1> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I1> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y1" for instance <LUT31_I1> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I1> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y1" for instance <MUXF5_I1> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I1> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y2" for instance <LUT30_I2> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I2> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y2" for instance <LUT31_I2> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I2> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y2" for instance <MUXF5_I2> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I2> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y3" for instance <LUT30_I3> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I3> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y3" for instance <LUT31_I3> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I3> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y3" for instance <MUXF5_I3> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I3> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y4" for instance <LUT30_I4> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I4> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y4" for instance <LUT31_I4> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I4> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y4" for instance <MUXF5_I4> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I4> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y5" for instance <LUT30_I5> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I5> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y5" for instance <LUT31_I5> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I5> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y5" for instance <MUXF5_I5> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I5> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y6" for instance <LUT30_I6> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I6> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y6" for instance <LUT31_I6> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I6> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y6" for instance <MUXF5_I6> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I6> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y7" for instance <LUT30_I7> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I7> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y7" for instance <LUT31_I7> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I7> in unit <Data_Read_Steering>.
    Set user-defined property "RLOC =  X17Y7" for instance <MUXF5_I7> in unit <Data_Read_Steering>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I7> in unit <Data_Read_Steering>.
Entity <Data_Read_Steering> analyzed. Unit <Data_Read_Steering> generated.

Analyzing generic Entity <mux4_8> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 4
	C_X = 29
	C_U_SET = "microblaze_0"
	C_BE = <u>1
    Set user-defined property "RLOC =  X29Y11" for instance <LUT30_I0> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I0> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y11" for instance <LUT31_I0> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I0> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y11" for instance <MUXF5_I0> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I0> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y10" for instance <LUT30_I1> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I1> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y10" for instance <LUT31_I1> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I1> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y10" for instance <MUXF5_I1> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I1> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y9" for instance <LUT30_I2> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I2> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y9" for instance <LUT31_I2> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I2> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y9" for instance <MUXF5_I2> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I2> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y8" for instance <LUT30_I3> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I3> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y8" for instance <LUT31_I3> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I3> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y8" for instance <MUXF5_I3> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I3> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y7" for instance <LUT30_I4> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I4> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y7" for instance <LUT31_I4> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I4> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y7" for instance <MUXF5_I4> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I4> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y6" for instance <LUT30_I5> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I5> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y6" for instance <LUT31_I5> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I5> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y6" for instance <MUXF5_I5> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I5> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y5" for instance <LUT30_I6> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I6> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y5" for instance <LUT31_I6> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I6> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y5" for instance <MUXF5_I6> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I6> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y4" for instance <LUT30_I7> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT30_I7> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y4" for instance <LUT31_I7> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT31_I7> in unit <mux4_8>.
    Set user-defined property "RLOC =  X29Y4" for instance <MUXF5_I7> in unit <mux4_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUXF5_I7> in unit <mux4_8>.
Entity <mux4_8> analyzed. Unit <mux4_8> generated.

Analyzing generic Entity <mux2_8> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 12
	C_X = 29
	C_U_SET = "microblaze_0"
	C_BE = <u>1
    Set user-defined property "RLOC =  X29Y15" for instance <LUT3_I0> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I0> in unit <mux2_8>.
    Set user-defined property "RLOC =  X29Y15" for instance <LUT3_I1> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I1> in unit <mux2_8>.
    Set user-defined property "RLOC =  X29Y14" for instance <LUT3_I2> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I2> in unit <mux2_8>.
    Set user-defined property "RLOC =  X29Y14" for instance <LUT3_I3> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I3> in unit <mux2_8>.
    Set user-defined property "RLOC =  X29Y13" for instance <LUT3_I4> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I4> in unit <mux2_8>.
    Set user-defined property "RLOC =  X29Y13" for instance <LUT3_I5> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I5> in unit <mux2_8>.
    Set user-defined property "RLOC =  X29Y12" for instance <LUT3_I6> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I6> in unit <mux2_8>.
    Set user-defined property "RLOC =  X29Y12" for instance <LUT3_I7> in unit <mux2_8>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I7> in unit <mux2_8>.
Entity <mux2_8> analyzed. Unit <mux2_8> generated.

Analyzing generic Entity <DOPB_Interface> (Architecture <imp>).
	C_D_OPB = 1
	C_D_LMB = 1
	C_DATA_SIZE = 32
	C_OPB_WIDTH = 32
	C_USE_DCACHE = 0
	C_DOPB_BUS_EXCEPTION = 0
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X32Y0" for instance <DM_request_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <DM_request_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y1" for instance <Request_Drop_In_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Request_Drop_In_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y8" for instance <Request_Drop_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Request_Drop_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y2" for instance <OPB_RESPONSE_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <OPB_RESPONSE_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y1" for instance <dOPB_MGrant_Rst_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <dOPB_MGrant_Rst_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y8" for instance <dOPB_MGrant_d_In_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <dOPB_MGrant_d_In_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y2" for instance <dOPB_MGrant_d_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <dOPB_MGrant_d_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y1" for instance <DM_select_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <DM_select_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X25Y7" for instance <dopb_DReady_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <dopb_DReady_I> in unit <DOPB_Interface>.
    Set user-defined property "INIT =  7577" for instance <dopb_DReady_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X25Y7" for instance <Mux_DReady_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Mux_DReady_I> in unit <DOPB_Interface>.
    Set user-defined property "RLOC =  X32Y3" for instance <DOPB_Interrupt_I> in unit <DOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <DOPB_Interrupt_I> in unit <DOPB_Interface>.
Entity <DOPB_Interface> analyzed. Unit <DOPB_Interface> generated.

Analyzing generic Entity <OPB_Data_Mux> (Architecture <imp>).
	C_DATA_SIZE = 32
	C_OPB_WIDTH = 32
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "RLOC =  X16Y0" for instance <MUX_LUT31> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT31> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT31> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y0" for instance <MUX_LUT30> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT30> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT30> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y1" for instance <MUX_LUT29> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT29> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT29> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y1" for instance <MUX_LUT28> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT28> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT28> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y2" for instance <MUX_LUT27> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT27> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT27> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y2" for instance <MUX_LUT26> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT26> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT26> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y3" for instance <MUX_LUT25> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT25> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT25> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y3" for instance <MUX_LUT24> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT24> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT24> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y4" for instance <MUX_LUT23> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT23> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT23> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y4" for instance <MUX_LUT22> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT22> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT22> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y5" for instance <MUX_LUT21> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT21> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT21> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y5" for instance <MUX_LUT20> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT20> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT20> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y6" for instance <MUX_LUT19> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT19> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT19> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y6" for instance <MUX_LUT18> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT18> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT18> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y7" for instance <MUX_LUT17> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT17> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT17> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y7" for instance <MUX_LUT16> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT16> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT16> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y8" for instance <MUX_LUT15> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT15> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT15> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y8" for instance <MUX_LUT14> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT14> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT14> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y9" for instance <MUX_LUT13> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT13> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT13> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y9" for instance <MUX_LUT12> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT12> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT12> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y10" for instance <MUX_LUT11> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT11> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT11> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y10" for instance <MUX_LUT10> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT10> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT10> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y11" for instance <MUX_LUT9> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT9> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT9> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y11" for instance <MUX_LUT8> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT8> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT8> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y12" for instance <MUX_LUT7> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT7> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT7> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y12" for instance <MUX_LUT6> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT6> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT6> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y13" for instance <MUX_LUT5> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT5> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT5> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y13" for instance <MUX_LUT4> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT4> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT4> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y14" for instance <MUX_LUT3> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT3> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT3> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y14" for instance <MUX_LUT2> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT2> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT2> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y15" for instance <MUX_LUT1> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT1> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT1> in unit <OPB_Data_Mux>.
    Set user-defined property "RLOC =  X16Y15" for instance <MUX_LUT0> in unit <OPB_Data_Mux>.
    Set user-defined property "U_SET =  microblaze_0" for instance <MUX_LUT0> in unit <OPB_Data_Mux>.
    Set user-defined property "INIT =  00CA" for instance <MUX_LUT0> in unit <OPB_Data_Mux>.
Entity <OPB_Data_Mux> analyzed. Unit <OPB_Data_Mux> generated.

Analyzing generic Entity <IOPB_Interface> (Architecture <imp>).
	C_I_OPB = 1
	C_I_LMB = 1
	C_DATA_SIZE = 32
	C_OPB_WIDTH = 32
	C_USE_NEW_LMB = 0
	C_ICACHE_USE_FSL = 0
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I31> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y0" for instance <ABus_FF_I31> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I31> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y0" for instance <IM_ABus_I31> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I30> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y0" for instance <ABus_FF_I30> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I30> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y0" for instance <IM_ABus_I30> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I29> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y1" for instance <ABus_FF_I29> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I29> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y1" for instance <IM_ABus_I29> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I28> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y1" for instance <ABus_FF_I28> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I28> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y1" for instance <IM_ABus_I28> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I27> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y2" for instance <ABus_FF_I27> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I27> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y2" for instance <IM_ABus_I27> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I26> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y2" for instance <ABus_FF_I26> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I26> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y2" for instance <IM_ABus_I26> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I25> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y3" for instance <ABus_FF_I25> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I25> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y3" for instance <IM_ABus_I25> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I24> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y3" for instance <ABus_FF_I24> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I24> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y3" for instance <IM_ABus_I24> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I23> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y4" for instance <ABus_FF_I23> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I23> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y4" for instance <IM_ABus_I23> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I22> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y4" for instance <ABus_FF_I22> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I22> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y4" for instance <IM_ABus_I22> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I21> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y5" for instance <ABus_FF_I21> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I21> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y5" for instance <IM_ABus_I21> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I20> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y5" for instance <ABus_FF_I20> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I20> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y5" for instance <IM_ABus_I20> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I19> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y6" for instance <ABus_FF_I19> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I19> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y6" for instance <IM_ABus_I19> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I18> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y6" for instance <ABus_FF_I18> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I18> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y6" for instance <IM_ABus_I18> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I17> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y7" for instance <ABus_FF_I17> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I17> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y7" for instance <IM_ABus_I17> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I16> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y7" for instance <ABus_FF_I16> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I16> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y7" for instance <IM_ABus_I16> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I15> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y8" for instance <ABus_FF_I15> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I15> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y8" for instance <IM_ABus_I15> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I14> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y8" for instance <ABus_FF_I14> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I14> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y8" for instance <IM_ABus_I14> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I13> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y9" for instance <ABus_FF_I13> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I13> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y9" for instance <IM_ABus_I13> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I12> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y9" for instance <ABus_FF_I12> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I12> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y9" for instance <IM_ABus_I12> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I11> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y10" for instance <ABus_FF_I11> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I11> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y10" for instance <IM_ABus_I11> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I10> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y10" for instance <ABus_FF_I10> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I10> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y10" for instance <IM_ABus_I10> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I9> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y11" for instance <ABus_FF_I9> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I9> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y11" for instance <IM_ABus_I9> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I8> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y11" for instance <ABus_FF_I8> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I8> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y11" for instance <IM_ABus_I8> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I7> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y12" for instance <ABus_FF_I7> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I7> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y12" for instance <IM_ABus_I7> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I6> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y12" for instance <ABus_FF_I6> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I6> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y12" for instance <IM_ABus_I6> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I5> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y13" for instance <ABus_FF_I5> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I5> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y13" for instance <IM_ABus_I5> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I4> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y13" for instance <ABus_FF_I4> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I4> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y13" for instance <IM_ABus_I4> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I3> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y14" for instance <ABus_FF_I3> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I3> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y14" for instance <IM_ABus_I3> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I2> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y14" for instance <ABus_FF_I2> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I2> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y14" for instance <IM_ABus_I2> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I1> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y15" for instance <ABus_FF_I1> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I1> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y15" for instance <IM_ABus_I1> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <ABus_FF_I0> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y15" for instance <ABus_FF_I0> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_ABus_I0> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X31Y15" for instance <IM_ABus_I0> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X23Y16" for instance <IM_request_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_request_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y7" for instance <Request_Drop_In_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Request_Drop_In_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y7" for instance <Request_Drop_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Request_Drop_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y6" for instance <OPB_RESPONSE_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <OPB_RESPONSE_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y5" for instance <IOPB_MGrant_Rst_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IOPB_MGrant_Rst_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y6" for instance <iOPB_MGrant_d_In_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <iOPB_MGrant_d_In_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y6" for instance <iOPB_MGrant_d_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <iOPB_MGrant_d_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y6" for instance <IM_select_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IM_select_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X23Y5" for instance <Mux_IReady_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Mux_IReady_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <Mux_Instr_Read_I> in unit <IOPB_Interface>.
    Set user-defined property "RLOC =  X32Y5" for instance <IOPB_Interrupt_I> in unit <IOPB_Interface>.
    Set user-defined property "U_SET =  microblaze_0" for instance <IOPB_Interrupt_I> in unit <IOPB_Interface>.
Entity <IOPB_Interface> analyzed. Unit <IOPB_Interface> generated.

Analyzing generic Entity <mux2_32> (Architecture <imp>).
	C_TARGET = <u>0110
	C_Y = 0
	C_X = 30
	C_U_SET = "microblaze_0"
	C_BE = <u>1
    Set user-defined property "RLOC =  X30Y15" for instance <LUT3_I0> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I0> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y15" for instance <LUT3_I1> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I1> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y14" for instance <LUT3_I2> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I2> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y14" for instance <LUT3_I3> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I3> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y13" for instance <LUT3_I4> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I4> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y13" for instance <LUT3_I5> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I5> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y12" for instance <LUT3_I6> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I6> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y12" for instance <LUT3_I7> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I7> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y11" for instance <LUT3_I8> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I8> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y11" for instance <LUT3_I9> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I9> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y10" for instance <LUT3_I10> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I10> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y10" for instance <LUT3_I11> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I11> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y9" for instance <LUT3_I12> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I12> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y9" for instance <LUT3_I13> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I13> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y8" for instance <LUT3_I14> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I14> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y8" for instance <LUT3_I15> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I15> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y7" for instance <LUT3_I16> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I16> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y7" for instance <LUT3_I17> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I17> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y6" for instance <LUT3_I18> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I18> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y6" for instance <LUT3_I19> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I19> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y5" for instance <LUT3_I20> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I20> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y5" for instance <LUT3_I21> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I21> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y4" for instance <LUT3_I22> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I22> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y4" for instance <LUT3_I23> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I23> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y3" for instance <LUT3_I24> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I24> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y3" for instance <LUT3_I25> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I25> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y2" for instance <LUT3_I26> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I26> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y2" for instance <LUT3_I27> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I27> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y1" for instance <LUT3_I28> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I28> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y1" for instance <LUT3_I29> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I29> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y0" for instance <LUT3_I30> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I30> in unit <mux2_32>.
    Set user-defined property "RLOC =  X30Y0" for instance <LUT3_I31> in unit <mux2_32>.
    Set user-defined property "U_SET =  microblaze_0" for instance <LUT3_I31> in unit <mux2_32>.
Entity <mux2_32> analyzed. Unit <mux2_32> generated.

Analyzing generic Entity <Debug> (Architecture <imp>).
	C_USE_ICACHE = 0
	C_ICACHE_BASEADDR = <u>00000000000000000000000000000000
	C_ICACHE_HIGHADDR = <u>00111111111111111111111111111111
	C_USE_DCACHE = 0
	C_DCACHE_BASEADDR = <u>00000000000000000000000000000000
	C_DCACHE_HIGHADDR = <u>00111111111111111111111111111111
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0"
	C_DATA_SIZE = 32
	C_NUMBER_OF_PC_BRK = 2
	C_NUMBER_OF_RD_ADDR_BRK = 1
	C_NUMBER_OF_WR_ADDR_BRK = 1
    Set user-defined property "INIT =  1123" for instance <SRL16E_I> in unit <Debug>.
    Set user-defined property "INIT =  FFFF" for instance <SRL16E_Cache_I1> in unit <Debug>.
    Set user-defined property "INIT =  3FFF" for instance <SRL16E_Cache_I2> in unit <Debug>.
    Set user-defined property "INIT =  0000" for instance <SRL16E_Cache_I3> in unit <Debug>.
    Set user-defined property "INIT =  0000" for instance <SRL16E_Cache_I4> in unit <Debug>.
    Set user-defined property "INIT =  FFFF" for instance <SRL16E_Cache_I5> in unit <Debug>.
    Set user-defined property "INIT =  3FFF" for instance <SRL16E_Cache_I6> in unit <Debug>.
    Set user-defined property "INIT =  0000" for instance <SRL16E_Cache_I7> in unit <Debug>.
    Set user-defined property "INIT =  0000" for instance <SRL16E_Cache_I8> in unit <Debug>.
    Set user-defined property "INIT =  0" for instance <Stop_CPU_FDRSE> in unit <Debug>.
INFO:Xst:1304 - Contents of register <pc_hit<4>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<5>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<6>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<7>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<8>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<9>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<10>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<11>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<12>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<13>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<14>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
INFO:Xst:1304 - Contents of register <pc_hit<15>> in unit <Debug> never changes during circuit operation. The register is replaced by logic.
Entity <Debug> analyzed. Unit <Debug> generated.

Analyzing generic Entity <address_hit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0_address_hit01100000110000"
	C_FIRST = <u>1
	No_Bits = 32
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_Pre> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y0" for instance <MUXCY_Pre> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_23> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_23> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_13> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_13> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_13> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_13> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_23> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_23> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_22> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_22> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_12> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_12> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_12> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_12> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_22> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_22> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_21> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_21> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_11> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_11> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_11> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_11> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_21> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_21> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_20> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_20> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_10> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <SRL16E_10> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_10> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_10> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_20> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_20> in unit <address_hit>.
    Set user-defined property "U_SET =  microblaze_0_address_hit00" for instance <MUXCY_Post> in unit <address_hit>.
    Set user-defined property "RLOC =  X0Y5" for instance <MUXCY_Post> in unit <address_hit>.
Entity <address_hit> analyzed. Unit <address_hit> generated.

Analyzing generic Entity <address_hit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0_address_hit01100000110001"
	C_FIRST = <u>0
	No_Bits = 32
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_Pre> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y0" for instance <MUXCY_Pre> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_23> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_23> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_13> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_13> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_13> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_13> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_23> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_23> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_22> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_22> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_12> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_12> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_12> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_12> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_22> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_22> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_21> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_21> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_11> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_11> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_11> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_11> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_21> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_21> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_20> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_20> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_10> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <SRL16E_10> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_10> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_10> in unit <address_hit162_>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_20> in unit <address_hit162_>.
    Set user-defined property "U_SET =  microblaze_0_address_hit01" for instance <MUXCY_20> in unit <address_hit162_>.
Entity <address_hit> analyzed. Unit <address_hit162> generated.

Analyzing generic Entity <address_data_hit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0_read_address_hit01100000110000"
	No_Bits = 32
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_Pre> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y0" for instance <MUXCY_Pre> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y5" for instance <SRL16E_addr_23> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_23> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y5" for instance <SRL16E_addr_13> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_13> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y5" for instance <MUXCY_addr_13> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_13> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y5" for instance <MUXCY_addr_23> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_23> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_data_23> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_23> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_data_13> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_13> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_data_13> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_13> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_data_23> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_23> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y6" for instance <SRL16E_addr_22> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_22> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y6" for instance <SRL16E_addr_12> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_12> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y6" for instance <MUXCY_addr_12> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_12> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y6" for instance <MUXCY_addr_22> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_22> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_data_22> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_22> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_data_12> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_12> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_data_12> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_12> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_data_22> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_22> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y7" for instance <SRL16E_addr_21> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_21> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y7" for instance <SRL16E_addr_11> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_11> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y7" for instance <MUXCY_addr_11> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_11> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y7" for instance <MUXCY_addr_21> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_21> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_data_21> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_21> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_data_11> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_11> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_data_11> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_11> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_data_21> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_21> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y8" for instance <SRL16E_addr_20> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_20> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y8" for instance <SRL16E_addr_10> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_addr_10> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y8" for instance <MUXCY_addr_10> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_10> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y8" for instance <MUXCY_addr_20> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_addr_20> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_data_20> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_20> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_data_10> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <SRL16E_data_10> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_data_10> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_10> in unit <address_data_hit>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_data_20> in unit <address_data_hit>.
    Set user-defined property "U_SET =  microblaze_0_read_address_hit00" for instance <MUXCY_data_20> in unit <address_data_hit>.
Entity <address_data_hit> analyzed. Unit <address_data_hit> generated.

Analyzing generic Entity <address_data_hit> (Architecture <imp>).
	C_TARGET = <u>0110
	C_U_SET = "microblaze_0_write_address_hit01100000110000"
	No_Bits = 32
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_Pre> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y0" for instance <MUXCY_Pre> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y5" for instance <SRL16E_addr_23> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_23> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y5" for instance <SRL16E_addr_13> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_13> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y5" for instance <MUXCY_addr_13> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_13> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y5" for instance <MUXCY_addr_23> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_23> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_data_23> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_23> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y1" for instance <SRL16E_data_13> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_13> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_data_13> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_13> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y1" for instance <MUXCY_data_23> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_23> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y6" for instance <SRL16E_addr_22> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_22> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y6" for instance <SRL16E_addr_12> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_12> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y6" for instance <MUXCY_addr_12> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_12> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y6" for instance <MUXCY_addr_22> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_22> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_data_22> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_22> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y2" for instance <SRL16E_data_12> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_12> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_data_12> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_12> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y2" for instance <MUXCY_data_22> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_22> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y7" for instance <SRL16E_addr_21> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_21> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y7" for instance <SRL16E_addr_11> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_11> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y7" for instance <MUXCY_addr_11> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_11> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y7" for instance <MUXCY_addr_21> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_21> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_data_21> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_21> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y3" for instance <SRL16E_data_11> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_11> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_data_11> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_11> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y3" for instance <MUXCY_data_21> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_21> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y8" for instance <SRL16E_addr_20> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_20> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y8" for instance <SRL16E_addr_10> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_addr_10> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y8" for instance <MUXCY_addr_10> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_10> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y8" for instance <MUXCY_addr_20> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_addr_20> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_data_20> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_20> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y4" for instance <SRL16E_data_10> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <SRL16E_data_10> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_data_10> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_10> in unit <address_data_hit163_>.
    Set user-defined property "RLOC =  X0Y4" for instance <MUXCY_data_20> in unit <address_data_hit163_>.
    Set user-defined property "U_SET =  microblaze_0_write_address_hit00" for instance <MUXCY_data_20> in unit <address_data_hit163_>.
Entity <address_data_hit> analyzed. Unit <address_data_hit163> generated.


=========================================================================
*                           HDL Synthesis                               *
=========================================================================

Synthesizing Unit <address_data_hit163>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/address_data_hit.vhd.
WARNING:Xst:1780 - Signal <srl16_Array_addr> is never used or assigned.
WARNING:Xst:1780 - Signal <srl16_Array_data> is never used or assigned.
Unit <address_data_hit163> synthesized.


Synthesizing Unit <address_data_hit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/address_data_hit.vhd.
WARNING:Xst:1780 - Signal <srl16_Array_addr> is never used or assigned.
WARNING:Xst:1780 - Signal <srl16_Array_data> is never used or assigned.
Unit <address_data_hit> synthesized.


Synthesizing Unit <address_hit162>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/address_hit.vhd.
WARNING:Xst:647 - Input <Single_Step_N> is never used.
WARNING:Xst:1780 - Signal <srl16_Array> is never used or assigned.
Unit <address_hit162> synthesized.


Synthesizing Unit <address_hit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/address_hit.vhd.
WARNING:Xst:1780 - Signal <srl16_Array> is never used or assigned.
Unit <address_hit> synthesized.


Synthesizing Unit <mux2_32>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mux2_32.vhd.
Unit <mux2_32> synthesized.


Synthesizing Unit <OPB_Data_Mux>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/opb_data_mux.vhd.
Unit <OPB_Data_Mux> synthesized.


Synthesizing Unit <mux2_8>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mux2_8.vhd.
Unit <mux2_8> synthesized.


Synthesizing Unit <mux4_8>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mux4_8.vhd.
Unit <mux4_8> synthesized.


Synthesizing Unit <Data_Read_Steering>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/data_read_steering.vhd.
Unit <Data_Read_Steering> synthesized.


Synthesizing Unit <PC_Bit161>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit161> synthesized.


Synthesizing Unit <PC_Bit160>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit160> synthesized.


Synthesizing Unit <PC_Bit159>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit159> synthesized.


Synthesizing Unit <PC_Bit158>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit158> synthesized.


Synthesizing Unit <PC_Bit157>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit157> synthesized.


Synthesizing Unit <PC_Bit156>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit156> synthesized.


Synthesizing Unit <PC_Bit155>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit155> synthesized.


Synthesizing Unit <PC_Bit154>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit154> synthesized.


Synthesizing Unit <PC_Bit153>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit153> synthesized.


Synthesizing Unit <PC_Bit152>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit152> synthesized.


Synthesizing Unit <PC_Bit151>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit151> synthesized.


Synthesizing Unit <PC_Bit150>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit150> synthesized.


Synthesizing Unit <PC_Bit149>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit149> synthesized.


Synthesizing Unit <PC_Bit148>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit148> synthesized.


Synthesizing Unit <PC_Bit147>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit147> synthesized.


Synthesizing Unit <PC_Bit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_bit.vhd.
Unit <PC_Bit> synthesized.


Synthesizing Unit <MSR_Reg_Bit146>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit146> synthesized.


Synthesizing Unit <MSR_Reg_Bit145>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit145> synthesized.


Synthesizing Unit <MSR_Reg_Bit144>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit144> synthesized.


Synthesizing Unit <MSR_Reg_Bit143>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit143> synthesized.


Synthesizing Unit <MSR_Reg_Bit142>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit142> synthesized.


Synthesizing Unit <MSR_Reg_Bit141>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit141> synthesized.


Synthesizing Unit <MSR_Reg_Bit140>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit140> synthesized.


Synthesizing Unit <MSR_Reg_Bit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <MSR_Reg_Bit> synthesized.


Synthesizing Unit <Result_Mux_Bit139>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit139> synthesized.


Synthesizing Unit <Result_Mux_Bit138>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit138> synthesized.


Synthesizing Unit <Result_Mux_Bit137>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit137> synthesized.


Synthesizing Unit <Result_Mux_Bit136>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit136> synthesized.


Synthesizing Unit <Result_Mux_Bit135>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit135> synthesized.


Synthesizing Unit <Result_Mux_Bit134>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit134> synthesized.


Synthesizing Unit <Result_Mux_Bit133>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit133> synthesized.


Synthesizing Unit <Result_Mux_Bit132>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit132> synthesized.


Synthesizing Unit <Result_Mux_Bit131>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit131> synthesized.


Synthesizing Unit <Result_Mux_Bit130>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit130> synthesized.


Synthesizing Unit <Result_Mux_Bit129>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit129> synthesized.


Synthesizing Unit <Result_Mux_Bit128>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit128> synthesized.


Synthesizing Unit <Result_Mux_Bit127>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit127> synthesized.


Synthesizing Unit <Result_Mux_Bit126>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit126> synthesized.


Synthesizing Unit <Result_Mux_Bit125>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit125> synthesized.


Synthesizing Unit <Result_Mux_Bit124>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit124> synthesized.


Synthesizing Unit <Result_Mux_Bit123>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit123> synthesized.


Synthesizing Unit <Result_Mux_Bit122>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit122> synthesized.


Synthesizing Unit <Result_Mux_Bit121>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit121> synthesized.


Synthesizing Unit <Result_Mux_Bit120>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit120> synthesized.


Synthesizing Unit <Result_Mux_Bit119>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit119> synthesized.


Synthesizing Unit <Result_Mux_Bit118>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit118> synthesized.


Synthesizing Unit <Result_Mux_Bit117>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit117> synthesized.


Synthesizing Unit <Result_Mux_Bit116>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit116> synthesized.


Synthesizing Unit <Result_Mux_Bit115>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit115> synthesized.


Synthesizing Unit <Result_Mux_Bit114>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit114> synthesized.


Synthesizing Unit <Result_Mux_Bit113>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit113> synthesized.


Synthesizing Unit <Result_Mux_Bit112>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit112> synthesized.


Synthesizing Unit <Result_Mux_Bit111>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit111> synthesized.


Synthesizing Unit <Result_Mux_Bit110>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit110> synthesized.


Synthesizing Unit <Result_Mux_Bit109>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit109> synthesized.


Synthesizing Unit <Result_Mux_Bit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
Unit <Result_Mux_Bit> synthesized.


Synthesizing Unit <Shift_Logic_Bit108>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit108> synthesized.


Synthesizing Unit <Shift_Logic_Bit107>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit107> synthesized.


Synthesizing Unit <Shift_Logic_Bit106>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit106> synthesized.


Synthesizing Unit <Shift_Logic_Bit105>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit105> synthesized.


Synthesizing Unit <Shift_Logic_Bit104>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit104> synthesized.


Synthesizing Unit <Shift_Logic_Bit103>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit103> synthesized.


Synthesizing Unit <Shift_Logic_Bit102>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit102> synthesized.


Synthesizing Unit <Shift_Logic_Bit101>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit101> synthesized.


Synthesizing Unit <Shift_Logic_Bit100>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit100> synthesized.


Synthesizing Unit <Shift_Logic_Bit99>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit99> synthesized.


Synthesizing Unit <Shift_Logic_Bit98>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit98> synthesized.


Synthesizing Unit <Shift_Logic_Bit97>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit97> synthesized.


Synthesizing Unit <Shift_Logic_Bit96>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit96> synthesized.


Synthesizing Unit <Shift_Logic_Bit95>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit95> synthesized.


Synthesizing Unit <Shift_Logic_Bit94>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit94> synthesized.


Synthesizing Unit <Shift_Logic_Bit93>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit93> synthesized.


Synthesizing Unit <Shift_Logic_Bit92>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit92> synthesized.


Synthesizing Unit <Shift_Logic_Bit91>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit91> synthesized.


Synthesizing Unit <Shift_Logic_Bit90>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit90> synthesized.


Synthesizing Unit <Shift_Logic_Bit89>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit89> synthesized.


Synthesizing Unit <Shift_Logic_Bit88>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit88> synthesized.


Synthesizing Unit <Shift_Logic_Bit87>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit87> synthesized.


Synthesizing Unit <Shift_Logic_Bit86>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit86> synthesized.


Synthesizing Unit <Shift_Logic_Bit85>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit85> synthesized.


Synthesizing Unit <Shift_Logic_Bit84>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit84> synthesized.


Synthesizing Unit <Shift_Logic_Bit83>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit83> synthesized.


Synthesizing Unit <Shift_Logic_Bit82>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit82> synthesized.


Synthesizing Unit <Shift_Logic_Bit81>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit81> synthesized.


Synthesizing Unit <Shift_Logic_Bit80>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit80> synthesized.


Synthesizing Unit <Shift_Logic_Bit79>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit79> synthesized.


Synthesizing Unit <Shift_Logic_Bit78>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit78> synthesized.


Synthesizing Unit <Shift_Logic_Bit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic_bit.vhd.
Unit <Shift_Logic_Bit> synthesized.


Synthesizing Unit <ALU_Bit77>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
    Found 1-bit xor2 for signal <$n0001> created at line 290.
Unit <ALU_Bit77> synthesized.


Synthesizing Unit <ALU_Bit76>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit76> synthesized.


Synthesizing Unit <ALU_Bit75>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit75> synthesized.


Synthesizing Unit <ALU_Bit74>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit74> synthesized.


Synthesizing Unit <ALU_Bit73>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit73> synthesized.


Synthesizing Unit <ALU_Bit72>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit72> synthesized.


Synthesizing Unit <ALU_Bit71>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit71> synthesized.


Synthesizing Unit <ALU_Bit70>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit70> synthesized.


Synthesizing Unit <ALU_Bit69>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit69> synthesized.


Synthesizing Unit <ALU_Bit68>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit68> synthesized.


Synthesizing Unit <ALU_Bit67>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit67> synthesized.


Synthesizing Unit <ALU_Bit66>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit66> synthesized.


Synthesizing Unit <ALU_Bit65>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit65> synthesized.


Synthesizing Unit <ALU_Bit64>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit64> synthesized.


Synthesizing Unit <ALU_Bit63>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit63> synthesized.


Synthesizing Unit <ALU_Bit62>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit62> synthesized.


Synthesizing Unit <ALU_Bit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu_bit.vhd.
WARNING:Xst:647 - Input <Compare_Instr> is never used.
WARNING:Xst:647 - Input <Unsigned_Op> is never used.
Unit <ALU_Bit> synthesized.


Synthesizing Unit <Operand_Select_Bit61>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit61> synthesized.


Synthesizing Unit <Operand_Select_Bit60>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit60> synthesized.


Synthesizing Unit <Operand_Select_Bit59>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit59> synthesized.


Synthesizing Unit <Operand_Select_Bit58>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit58> synthesized.


Synthesizing Unit <Operand_Select_Bit57>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit57> synthesized.


Synthesizing Unit <Operand_Select_Bit56>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit56> synthesized.


Synthesizing Unit <Operand_Select_Bit55>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit55> synthesized.


Synthesizing Unit <Operand_Select_Bit54>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit54> synthesized.


Synthesizing Unit <Operand_Select_Bit53>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit53> synthesized.


Synthesizing Unit <Operand_Select_Bit52>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit52> synthesized.


Synthesizing Unit <Operand_Select_Bit51>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit51> synthesized.


Synthesizing Unit <Operand_Select_Bit50>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit50> synthesized.


Synthesizing Unit <Operand_Select_Bit49>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit49> synthesized.


Synthesizing Unit <Operand_Select_Bit48>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit48> synthesized.


Synthesizing Unit <Operand_Select_Bit47>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit47> synthesized.


Synthesizing Unit <Operand_Select_Bit46>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <take_Ext_Brk_I> is assigned but never used.
Unit <Operand_Select_Bit46> synthesized.


Synthesizing Unit <Operand_Select_Bit45>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit45> synthesized.


Synthesizing Unit <Operand_Select_Bit44>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit44> synthesized.


Synthesizing Unit <Operand_Select_Bit43>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit43> synthesized.


Synthesizing Unit <Operand_Select_Bit42>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit42> synthesized.


Synthesizing Unit <Operand_Select_Bit41>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit41> synthesized.


Synthesizing Unit <Operand_Select_Bit40>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit40> synthesized.


Synthesizing Unit <Operand_Select_Bit39>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit39> synthesized.


Synthesizing Unit <Operand_Select_Bit38>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:647 - Input <Enable_MSR> is never used.
WARNING:Xst:647 - Input <MSR> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit38> synthesized.


Synthesizing Unit <Operand_Select_Bit37>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit37> synthesized.


Synthesizing Unit <Operand_Select_Bit36>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit36> synthesized.


Synthesizing Unit <Operand_Select_Bit35>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit35> synthesized.


Synthesizing Unit <Operand_Select_Bit34>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit34> synthesized.


Synthesizing Unit <Operand_Select_Bit33>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit33> synthesized.


Synthesizing Unit <Operand_Select_Bit32>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit32> synthesized.


Synthesizing Unit <Operand_Select_Bit31>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit31> synthesized.


Synthesizing Unit <Operand_Select_Bit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select_bit.vhd.
WARNING:Xst:647 - Input <Sign_Imm> is never used.
WARNING:Xst:646 - Signal <rst> is assigned but never used.
WARNING:Xst:646 - Signal <use_Imm_Reg_I> is assigned but never used.
Unit <Operand_Select_Bit> synthesized.


Synthesizing Unit <Register_File_Bit30>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit30> synthesized.


Synthesizing Unit <Register_File_Bit29>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit29> synthesized.


Synthesizing Unit <Register_File_Bit28>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit28> synthesized.


Synthesizing Unit <Register_File_Bit27>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit27> synthesized.


Synthesizing Unit <Register_File_Bit26>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit26> synthesized.


Synthesizing Unit <Register_File_Bit25>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit25> synthesized.


Synthesizing Unit <Register_File_Bit24>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit24> synthesized.


Synthesizing Unit <Register_File_Bit23>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit23> synthesized.


Synthesizing Unit <Register_File_Bit22>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit22> synthesized.


Synthesizing Unit <Register_File_Bit21>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit21> synthesized.


Synthesizing Unit <Register_File_Bit20>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit20> synthesized.


Synthesizing Unit <Register_File_Bit19>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit19> synthesized.


Synthesizing Unit <Register_File_Bit18>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit18> synthesized.


Synthesizing Unit <Register_File_Bit17>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit17> synthesized.


Synthesizing Unit <Register_File_Bit16>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit16> synthesized.


Synthesizing Unit <Register_File_Bit15>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit15> synthesized.


Synthesizing Unit <Register_File_Bit14>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit14> synthesized.


Synthesizing Unit <Register_File_Bit13>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit13> synthesized.


Synthesizing Unit <Register_File_Bit12>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit12> synthesized.


Synthesizing Unit <Register_File_Bit11>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit11> synthesized.


Synthesizing Unit <Register_File_Bit10>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit10> synthesized.


Synthesizing Unit <Register_File_Bit9>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit9> synthesized.


Synthesizing Unit <Register_File_Bit8>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit8> synthesized.


Synthesizing Unit <Register_File_Bit7>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit7> synthesized.


Synthesizing Unit <Register_File_Bit6>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit6> synthesized.


Synthesizing Unit <Register_File_Bit5>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit5> synthesized.


Synthesizing Unit <Register_File_Bit4>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit4> synthesized.


Synthesizing Unit <Register_File_Bit3>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit3> synthesized.


Synthesizing Unit <Register_File_Bit2>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit2> synthesized.


Synthesizing Unit <Register_File_Bit1>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit1> synthesized.


Synthesizing Unit <Register_File_Bit0>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit0> synthesized.


Synthesizing Unit <Register_File_Bit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file_bit.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:1780 - Signal <reg_WE> is never used or assigned.
Unit <Register_File_Bit> synthesized.


Synthesizing Unit <PC_Module>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/pc_module.vhd.
WARNING:Xst:646 - Signal <Carry<0>> is assigned but never used.
WARNING:Xst:1780 - Signal <pc_I> is never used or assigned.
WARNING:Xst:1780 - Signal <PC_EX_i> is never used or assigned.
WARNING:Xst:1780 - Signal <pc_OF_I> is never used or assigned.
WARNING:Xst:1780 - Signal <new_PC> is never used or assigned.
WARNING:Xst:1780 - Signal <PC_Buffer> is never used or assigned.
Unit <PC_Module> synthesized.


Synthesizing Unit <MSR_Reg>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/msr_reg.vhd.
WARNING:Xst:647 - Input <Enable_Exceptions<0>> is never used.
WARNING:Xst:647 - Input <MSRclr_Instr<0>> is never used.
WARNING:Xst:647 - Input <Logic_Result> is never used.
WARNING:Xst:647 - Input <Reset_EIP<0>> is never used.
WARNING:Xst:647 - Input <Disable_Exceptions<0>> is never used.
WARNING:Xst:647 - Input <Set_EIP<0>> is never used.
WARNING:Xst:647 - Input <MSRxxx_Instr<0>> is never used.
WARNING:Xst:646 - Signal <we_Bits<0:1>> is assigned but never used.
WARNING:Xst:1780 - Signal <rst_Values<0:1>> is never used or assigned.
WARNING:Xst:1780 - Signal <rst_Values_I> is never used or assigned.
WARNING:Xst:1780 - Signal <set_Values_I> is never used or assigned.
WARNING:Xst:1780 - Signal <set_Values<0:1>> is never used or assigned.
WARNING:Xst:646 - Signal <new_Value_I<0:1>> is assigned but never used.
    Found 1 1-bit 2-to-1 multiplexers.
    Summary:
	inferred   1 Multiplexer(s).
Unit <MSR_Reg> synthesized.


Synthesizing Unit <Zero_Detect>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/zero_detect.vhd.
Unit <Zero_Detect> synthesized.


Synthesizing Unit <Result_Mux>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/result_mux.vhd.
WARNING:Xst:647 - Input <Hexlet_Read<0>> is never used.
WARNING:Xst:647 - Input <Op1<0:15>> is never used.
WARNING:Xst:647 - Input <Op1<17:23>> is never used.
WARNING:Xst:647 - Input <Op1<25:31>> is never used.
WARNING:Xst:647 - Input <Sext32<0>> is never used.
WARNING:Xst:1780 - Signal <ex_Result_i> is never used or assigned.
    Found 8 1-bit 2-to-1 multiplexers.
    Summary:
	inferred   8 Multiplexer(s).
Unit <Result_Mux> synthesized.


Synthesizing Unit <MUL_Unit>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/mul_unit.vhd.
WARNING:Xst:1780 - Signal <Prod_AD_Plus_BC> is never used or assigned.
WARNING:Xst:1780 - Signal <Prod_AD_Plus_BC_I> is never used or assigned.
WARNING:Xst:646 - Signal <prod_AD<0:19>> is assigned but never used.
WARNING:Xst:646 - Signal <prod_BC<0:19>> is assigned but never used.
WARNING:Xst:646 - Signal <prod_BD<0:3>> is assigned but never used.
WARNING:Xst:1780 - Signal <prod_BD_1> is never used or assigned.
    Found 16-bit adder for signal <$n0000> created at line 371.
    Found 16-bit adder for signal <Prod_AD_Plus_BC_I0>.
    Summary:
	inferred   2 Adder/Subtracter(s).
Unit <MUL_Unit> synthesized.


Synthesizing Unit <Shift_Logic_Module>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/shift_logic.vhd.
WARNING:Xst:647 - Input <Sext32<0>> is never used.
WARNING:Xst:1780 - Signal <or_Oper> is never used or assigned.
    Found 16 1-bit 2-to-1 multiplexers.
    Summary:
	inferred  16 Multiplexer(s).
Unit <Shift_Logic_Module> synthesized.


Synthesizing Unit <ALU>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/alu.vhd.
WARNING:Xst:1780 - Signal <alu_Result_i> is never used or assigned.
WARNING:Xst:1780 - Signal <M_ABus_i> is never used or assigned.
Unit <ALU> synthesized.


Synthesizing Unit <Operand_Select>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/operand_select.vhd.
WARNING:Xst:647 - Input <MFS_Reg_Sel> is never used.
WARNING:Xst:647 - Input <EAR> is never used.
WARNING:Xst:647 - Input <ESR> is never used.
WARNING:Xst:1780 - Signal <Op1_I> is never used or assigned.
WARNING:Xst:1780 - Signal <Op2_I> is never used or assigned.
WARNING:Xst:1780 - Signal <Op2_C_I> is never used or assigned.
WARNING:Xst:1780 - Signal <Reg1_I> is never used or assigned.
    Found 16-bit register for signal <imm_Reg>.
    Summary:
	inferred  16 D-type flip-flop(s).
Unit <Operand_Select> synthesized.


Synthesizing Unit <Register_File>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/register_file.vhd.
WARNING:Xst:1780 - Signal <Reg_File> is never used or assigned.
Unit <Register_File> synthesized.


Synthesizing Unit <PreFetch_Buffer>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/prefetch_buffer.vhd.
WARNING:Xst:1780 - Signal <buffer_Addr_Carry<0>> is never used or assigned.
WARNING:Xst:646 - Signal <buffer_Addr_Carry<1>> is assigned but never used.
WARNING:Xst:1780 - Signal <buffer_Addr_Calc> is never used or assigned.
WARNING:Xst:1780 - Signal <buffer_Addr_Sum<0>> is never used or assigned.
WARNING:Xst:1780 - Signal <PC_Buffer> is never used or assigned.
WARNING:Xst:1780 - Signal <buffer_Addr_S_I<0>> is never used or assigned.
WARNING:Xst:1780 - Signal <buffer_Addr_DI> is never used or assigned.
WARNING:Xst:646 - Signal <One> is assigned but never used.
WARNING:Xst:646 - Signal <Zero> is assigned but never used.
WARNING:Xst:1780 - Signal <iReady_I> is never used or assigned.
WARNING:Xst:1780 - Signal <buffer_Addr_Incr> is never used or assigned.
WARNING:Xst:1780 - Signal <buffer_Addr_I<0>> is never used or assigned.
    Found 3-bit xor2 for signal <buffer_Addr_Sum<1:3>>.
Unit <PreFetch_Buffer> synthesized.


Synthesizing Unit <Debug>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/debug.vhd.
WARNING:Xst:647 - Input <OF_PipeRun<0>> is never used.
WARNING:Xst:647 - Input <Reg_Read> is never used.
WARNING:Xst:1780 - Signal <pc_hit_i<4:15>> is never used or assigned.
WARNING:Xst:646 - Signal <write_register_1> is assigned but never used.
WARNING:Xst:646 - Signal <which_pc<4:15>> is assigned but never used.
WARNING:Xst:1780 - Signal <temp8<0>> is never used or assigned.
WARNING:Xst:646 - Signal <hold_Stop_CPU> is assigned but never used.
WARNING:Xst:1780 - Signal <temp9<0>> is never used or assigned.
WARNING:Xst:646 - Signal <prev_11<6:7>> is assigned but never used.
    Found finite state machine <FSM_0> for signal <dbg_pipe_state>.
    -----------------------------------------------------------------------
    | States             | 6                                              |
    | Transitions        | 10                                             |
    | Inputs             | 3                                              |
    | Outputs            | 6                                              |
    | Clock              | Clk (rising_edge)                              |
    | Reset              | Reset<0> (positive)                            |
    | Reset type         | asynchronous                                   |
    | Reset State        | idle                                           |
    | Power Up State     | idle                                           |
    | Encoding           | automatic                                      |
    | Implementation     | automatic                                      |
    -----------------------------------------------------------------------
    Found 1-bit register for signal <Dbg_Set_Op1>.
    Found 1-bit register for signal <Dbg_Set_Op2>.
    Found 2-bit register for signal <Dbg_Result_Sel>.
    Found 1-bit register for signal <MB_Halted>.
    Found 1-bit register for signal <Dbg_Write_Reg<0>>.
    Found 1-bit register for signal <Dbg_Force_Logic>.
    Found 1-bit register for signal <Dbg_AS_Strobe>.
    Found 1-bit register for signal <Dbg_Restore_Logic>.
    Found 1-bit register for signal <Dbg_Reg_Access>.
    Found 1-bit register for signal <Dbg_Write_PC<0>>.
    Found 1-bit register for signal <Dbg_Write_Strobe>.
    Found 32-bit register for signal <Dbg_Rst_Op1>.
    Found 32-bit register for signal <Dbg_Rst_Op2>.
    Found 1-bit register for signal <Dbg_Write_MSR<0>>.
    Found 1-bit register for signal <Dbg_Read_Strobe>.
    Found 37-bit register for signal <addr_reg>.
    Found 1-bit register for signal <change_op1>.
    Found 1-bit register for signal <change_op2>.
    Found 8-bit register for signal <command_reg>.
    Found 1-bit register for signal <continue_from_brk>.
    Found 1-bit register for signal <continue_from_brk_TClk>.
    Found 3-bit register for signal <control_reg>.
    Found 33-bit register for signal <data_rd_reg>.
    Found 33-bit register for signal <data_read_reg>.
    Found 32-bit register for signal <data_write_reg>.
    Found 1-bit register for signal <dbg_AS_Strobe_i>.
    Found 1-bit register for signal <dbg_mem_access_i>.
    Found 1-bit register for signal <dbg_mem_read_reg>.
    Found 1-bit register for signal <dbg_stop_i>.
    Found 1-bit register for signal <Dbg_Write_DCache_i<0>>.
    Found 1-bit register for signal <Dbg_Write_ICache_i<0>>.
    Found 1-bit register for signal <mem_load_data_reg>.
    Found 32-bit register for signal <old_op2>.
    Found 4-bit register for signal <pc_hit<0:3>>.
    Found 16-bit register for signal <pc_hit_1>.
    Found 1-bit register for signal <prev>.
    Found 1-bit register for signal <prev0>.
    Found 8-bit register for signal <prev1>.
    Found 1-bit register for signal <prev_1>.
    Found 1-bit register for signal <prev_10>.
    Found 8-bit register for signal <prev_11>.
    Found 1-bit register for signal <read_memory>.
    Found 1-bit register for signal <read_pc>.
    Found 1-bit register for signal <read_register>.
    Found 1-bit register for signal <read_register_1>.
    Found 8-bit up counter for signal <shift_Count>.
    Found 1-bit register for signal <single_Step_N>.
    Found 1-bit register for signal <single_Step_TClk>.
    Found 1-bit register for signal <start_single_step>.
    Found 18-bit register for signal <status_reg>.
    Found 1-bit register for signal <stop_CPU_1>.
    Found 1-bit register for signal <tdi_1>.
    Found 2-bit register for signal <temp8<1:2>>.
    Found 7-bit register for signal <temp9<1:7>>.
    Found 1-bit register for signal <Want_to_Stop>.
    Found 1-bit register for signal <write_memory>.
    Found 1-bit register for signal <write_register>.
    Found 82 1-bit 2-to-1 multiplexers.
    Summary:
	inferred   1 Finite State Machine(s).
	inferred   1 Counter(s).
	inferred 346 D-type flip-flop(s).
	inferred  82 Multiplexer(s).
Unit <Debug> synthesized.


Synthesizing Unit <IOPB_Interface>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/iopb_interface.vhd.
WARNING:Xst:1780 - Signal <iFetch_d_CE> is never used or assigned.
WARNING:Xst:1780 - Signal <iFetch_d> is never used or assigned.
WARNING:Xst:1780 - Signal <select_Drop> is never used or assigned.
WARNING:Xst:1780 - Signal <select_Drop_In> is never used or assigned.
WARNING:Xst:646 - Signal <mux_YL> is assigned but never used.
WARNING:Xst:1780 - Signal <true_request> is never used or assigned.
    Found 1-bit register for signal <abort_Access_hold>.
    Summary:
	inferred   1 D-type flip-flop(s).
Unit <IOPB_Interface> synthesized.


Synthesizing Unit <DOPB_Interface>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/dopb_interface.vhd.
WARNING:Xst:647 - Input <Write_Strobe> is never used.
WARNING:Xst:1780 - Signal <timeout_d> is never used or assigned.
WARNING:Xst:1780 - Signal <mux_Data_Read_In> is never used or assigned.
WARNING:Xst:1780 - Signal <delay_dready> is never used or assigned.
WARNING:Xst:1780 - Signal <mux_Data_Read_YL> is never used or assigned.
WARNING:Xst:1780 - Signal <select_Drop> is never used or assigned.
WARNING:Xst:1780 - Signal <select_Drop_In> is never used or assigned.
WARNING:Xst:1780 - Signal <iDM_select_1> is never used or assigned.
WARNING:Xst:1780 - Signal <mux_Data_Read_S> is never used or assigned.
WARNING:Xst:646 - Signal <sel_LMB> is assigned but never used.
    Found 1-bit register for signal <DM_busLock>.
    Found 1-bit register for signal <abort_Access_hold>.
    Summary:
	inferred   2 D-type flip-flop(s).
Unit <DOPB_Interface> synthesized.


Synthesizing Unit <Byte_Doublet_Handle>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/byte_doublet_handle.vhd.
WARNING:Xst:647 - Input <Reset<0>> is never used.
WARNING:Xst:646 - Signal <Data_Read_To_Mux> is assigned but never used.
WARNING:Xst:646 - Signal <extend_Write_LSB1_YL> is assigned but never used.
WARNING:Xst:1780 - Signal <sel_LSB_1> is never used or assigned.
    Found 1-bit xor3 for signal <Low_Addr<0>>.
    Found 1-bit xor2 for signal <Low_Addr<1>>.
    Summary:
	inferred   1 Xor(s).
Unit <Byte_Doublet_Handle> synthesized.


Synthesizing Unit <Data_Flow>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/data_flow.vhd.
WARNING:Xst:647 - Input <Left_Shift> is never used.
WARNING:Xst:647 - Input <Start_Div> is never used.
WARNING:Xst:647 - Input <Arith_Shift> is never used.
WARNING:Xst:1780 - Signal <pc_Write_I> is never used or assigned.
WARNING:Xst:646 - Signal <not_Barrel_Op_i> is assigned but never used.
WARNING:Xst:646 - Signal <Div_Result> is assigned but never used.
WARNING:Xst:646 - Signal <not_Div_Op_i> is assigned but never used.
WARNING:Xst:646 - Signal <barrel_Result> is assigned but never used.
    Found 9 1-bit 2-to-1 multiplexers.
    Summary:
	inferred   9 Multiplexer(s).
Unit <Data_Flow> synthesized.


Synthesizing Unit <Decode>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/decode.vhd.
WARNING:Xst:1305 - Output <MB_Get_Read> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <Div_By_Zero> is never used.
WARNING:Xst:1305 - Output <Enable_Exceptions> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <word_r1_r2_unalignment> is never used.
WARNING:Xst:647 - Input <MB_Get_Control> is never used.
WARNING:Xst:647 - Input <MB_Put_Full> is never used.
WARNING:Xst:647 - Input <EIP_Active<0>> is never used.
WARNING:Xst:647 - Input <D_Exception> is never used.
WARNING:Xst:647 - Input <Enable_BusLock<0>> is never used.
WARNING:Xst:647 - Input <word_r1_imm_unalignment> is never used.
WARNING:Xst:1305 - Output <Reset_EIP> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <MB_Put_Write> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <Not_MB_Get_Op> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <Disable_Exceptions> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <Set_FSL_Error> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <MB_Get_Exists> is never used.
WARNING:Xst:647 - Input <halfword_unalignment> is never used.
WARNING:Xst:647 - Input <Exceptions_Enabled<0>> is never used.
WARNING:Xst:1305 - Output <Set_EIP> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <I_Exception> is never used.
WARNING:Xst:1305 - Output <Div_Zero_Exception> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <FSL_Control_Bit> is never assigned. Tied to value 0.
WARNING:Xst:1780 - Signal <MB_Put> is never used or assigned.
WARNING:Xst:1780 - Signal <of_Mnem> is never used or assigned.
WARNING:Xst:1780 - Signal <MB_nGet_i> is never used or assigned.
WARNING:Xst:646 - Signal <Div_Exception> is assigned but never used.
WARNING:Xst:1780 - Signal <ex_Mnem> is never used or assigned.
WARNING:Xst:1780 - Signal <if_Mnem> is never used or assigned.
WARNING:Xst:1780 - Signal <dbg_jump> is never used or assigned.
WARNING:Xst:1780 - Signal <MB_Put_i> is never used or assigned.
WARNING:Xst:646 - Signal <Illegal_Opcode_I> is assigned but never used.
WARNING:Xst:646 - Signal <DOPB_Exception> is assigned but never used.
WARNING:Xst:1780 - Signal <mb_Get_i> is never used or assigned.
WARNING:Xst:1780 - Signal <ex_Finished> is never used or assigned.
WARNING:Xst:1780 - Signal <word_unalignment> is never used or assigned.
WARNING:Xst:646 - Signal <unalignment_exc> is assigned but never used.
WARNING:Xst:1780 - Signal <MB_nGet> is never used or assigned.
WARNING:Xst:646 - Signal <interrupts_OK<0>> is assigned but never used.
WARNING:Xst:646 - Signal <quadlet_i<0>> is assigned but never used.
WARNING:Xst:1780 - Signal <halfword_unalignment_i> is never used or assigned.
WARNING:Xst:1780 - Signal <FSL_Control_Bit_i> is never used or assigned.
WARNING:Xst:1780 - Signal <MB_Get> is never used or assigned.
WARNING:Xst:1780 - Signal <MB_nPut> is never used or assigned.
WARNING:Xst:1780 - Signal <MB_nPut_i> is never used or assigned.
    Found 1-bit register for signal <Valid_Instr>.
    Found 1-bit register for signal <Interrupt_Taken>.
    Found 32-bit register for signal <Instr_EX>.
    Found 1-bit register for signal <Use_Store_Instr_Addr>.
    Found 1-bit register for signal <Sext8<0>>.
    Found 1-bit register for signal <Branch_Instr>.
    Found 1-bit register for signal <Not_Div_Op>.
    Found 1-bit register for signal <Shift_Carry_In>.
    Found 1-bit register for signal <Not_Mul_Op>.
    Found 1-bit register for signal <Sign_Extend<0>>.
    Found 1-bit register for signal <Compare_Instr>.
    Found 1-bit register for signal <Sext16<0>>.
    Found 2-bit register for signal <Shift_Oper>.
    Found 2-bit register for signal <Logic_Oper>.
    Found 1-bit register for signal <Select_Logic<0>>.
    Found 1-bit register for signal <Unsigned_Op>.
    Found 1-bit register for signal <Carry_In>.
    Found 2-bit register for signal <Result_Sel>.
    Found 1-bit xor2 for signal <$n0247>.
    Found 1-bit xor2 for signal <$n0248>.
    Found 1-bit xor2 for signal <$n0249>.
    Found 1-bit xor2 for signal <$n0250>.
    Found 1-bit xor2 for signal <$n0251>.
    Found 1-bit xor2 for signal <$n0257> created at line 2184.
    Found 1-bit xor2 for signal <$n0307> created at line 2184.
    Found 1-bit xor2 for signal <$n0308> created at line 2184.
    Found 1-bit xor2 for signal <$n0309> created at line 2184.
    Found 1-bit xor2 for signal <$n0310> created at line 2184.
    Found 1-bit register for signal <break_Pipe<0>>.
    Found 1-bit register for signal <byte_i<0>>.
    Found 1-bit register for signal <d_AS_I>.
    Found 2-bit register for signal <dbg_old_values>.
    Found 2-bit register for signal <dbg_rst_values>.
    Found 1-bit register for signal <dbg_set_values>.
    Found 1-bit register for signal <div_first<0>>.
    Found 1-bit register for signal <div_started>.
    Found 1-bit register for signal <doublet_i<0>>.
    Found 1-bit register for signal <doublet_Read_i<0>>.
    Found 1-bit register for signal <enable_Interrupts_I<0>>.
    Found 1-bit register for signal <ex_Valid<0>>.
    Found 1-bit register for signal <iFetch_In_Progress<0>>.
    Found 1-bit register for signal <inHibit_EX<0>>.
    Found 1-bit register for signal <jump2_I<0>>.
    Found 1-bit register for signal <load_Store_i<0>>.
    Found 1-bit register for signal <Load_Store_Instr_Addr_Stored>.
    Found 1-bit register for signal <missed_IFetch<0>>.
    Found 1-bit register for signal <mul_Executing<0>>.
    Found 1-bit register for signal <mul_first<0>>.
    Found 1-bit register for signal <mul_second<0>>.
    Found 1-bit register for signal <nonvalid_IFetch_n>.
    Found 1-bit register for signal <quadlet_Read_i<0>>.
    Found 1-bit register for signal <reset_BIP_I<0>>.
    Found 1-bit register for signal <select_ALU_Carry<0>>.
    Found 1-bit register for signal <set_BIP_I<0>>.
    Found 1-bit register for signal <Start_Div_i>.
    Found 1-bit register for signal <take_Break<0>>.
    Found 1-bit register for signal <take_NM_Break<0>>.
    Found 1-bit register for signal <using_Imm<0>>.
    Found 5-bit register for signal <write_Addr_I>.
    Found 1-bit register for signal <write_Carry_I<0>>.
    Found 1-bit register for signal <Write_DCache_I<0>>.
    Found 1-bit register for signal <Write_ICache_I<0>>.
    Found 1-bit register for signal <write_MSR_I<0>>.
    Found 1-bit register for signal <write_Reg<0>>.
    Found 1-bit register for signal <writing<0>>.
    Found 8 1-bit 2-to-1 multiplexers.
    Summary:
	inferred  95 D-type flip-flop(s).
	inferred   8 Multiplexer(s).
Unit <Decode> synthesized.


Synthesizing Unit <microblaze>.
    Related source file is //farside/proj/embedded/build/EDK_Gmm.HEADn/rtf/hw/XilinxProcessorIPLib/pcores/microblaze_v3_00_a/hdl/vhdl/microblaze.vhd.
WARNING:Xst:647 - Input <FSL0_S_Control> is never used.
WARNING:Xst:1305 - Output <DCACHE_FSL_IN_Read> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <FSL4_S_Exists> is never used.
WARNING:Xst:647 - Input <FSL1_S_Control> is never used.
WARNING:Xst:647 - Input <FSL4_M_Full> is never used.
WARNING:Xst:647 - Input <FSL6_S_Data> is never used.
WARNING:Xst:1305 - Output <DCACHE_FSL_OUT_Data> is never assigned. Tied to value 00000000000000000000000000000000.
WARNING:Xst:647 - Input <FSL1_S_Data> is never used.
WARNING:Xst:647 - Input <FSL2_S_Control> is never used.
WARNING:Xst:647 - Input <FSL3_S_Exists> is never used.
WARNING:Xst:1305 - Output <Trace_DCache_Hit> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <ICACHE_FSL_OUT_Write> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <ICACHE_FSL_IN_Exists> is never used.
WARNING:Xst:647 - Input <FSL3_S_Control> is never used.
WARNING:Xst:647 - Input <FSL3_M_Full> is never used.
WARNING:Xst:647 - Input <FSL5_S_Data> is never used.
WARNING:Xst:1305 - Output <Trace_Delay_Slot> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <Trace_ICache_Hit> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <ICACHE_FSL_IN_Data> is never used.
WARNING:Xst:647 - Input <DCACHE_FSL_IN_Control> is never used.
WARNING:Xst:647 - Input <FSL0_S_Data> is never used.
WARNING:Xst:647 - Input <FSL4_S_Control> is never used.
WARNING:Xst:647 - Input <FSL2_S_Exists> is never used.
WARNING:Xst:1305 - Output <ICACHE_FSL_OUT_Clk> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <Trace_DCache_Req> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <ICACHE_FSL_IN_Control> is never used.
WARNING:Xst:1305 - Output <ICACHE_FSL_OUT_Control> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <ICACHE_FSL_IN_Read> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <FSL5_S_Control> is never used.
WARNING:Xst:647 - Input <FSL7_S_Exists> is never used.
WARNING:Xst:647 - Input <FSL7_M_Full> is never used.
WARNING:Xst:647 - Input <ICACHE_FSL_OUT_Full> is never used.
WARNING:Xst:1305 - Output <ICACHE_FSL_IN_Clk> is never assigned. Tied to value 0.
WARNING:Xst:1305 - Output <Trace_ICache_Req> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <FSL2_M_Full> is never used.
WARNING:Xst:647 - Input <FSL4_S_Data> is never used.
WARNING:Xst:1305 - Output <DCACHE_FSL_OUT_Control> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <FSL6_S_Control> is never used.
WARNING:Xst:647 - Input <FSL1_S_Exists> is never used.
WARNING:Xst:1305 - Output <DCACHE_FSL_OUT_Write> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <DCACHE_FSL_IN_Exists> is never used.
WARNING:Xst:647 - Input <FSL7_S_Control> is never used.
WARNING:Xst:647 - Input <FSL6_S_Exists> is never used.
WARNING:Xst:647 - Input <FSL6_M_Full> is never used.
WARNING:Xst:647 - Input <FSL1_M_Full> is never used.
WARNING:Xst:647 - Input <FSL3_S_Data> is never used.
WARNING:Xst:647 - Input <FSL0_S_Exists> is never used.
WARNING:Xst:1305 - Output <ICACHE_FSL_OUT_Data> is never assigned. Tied to value 00000000000000000000000000000000.
WARNING:Xst:1305 - Output <DCACHE_FSL_IN_Clk> is never assigned. Tied to value 0.
WARNING:Xst:647 - Input <FSL5_S_Exists> is never used.
WARNING:Xst:647 - Input <DCACHE_FSL_OUT_Full> is never used.
WARNING:Xst:647 - Input <FSL5_M_Full> is never used.
WARNING:Xst:647 - Input <FSL7_S_Data> is never used.
WARNING:Xst:647 - Input <DCACHE_FSL_IN_Data> is never used.
WARNING:Xst:647 - Input <FSL0_M_Full> is never used.
WARNING:Xst:647 - Input <FSL2_S_Data> is never used.
WARNING:Xst:1305 - Output <DCACHE_FSL_OUT_Clk> is never assigned. Tied to value 0.
WARNING:Xst:1780 - Signal <dopb_Interrupt> is never used or assigned.
WARNING:Xst:646 - Signal <Command_Reg_D> is assigned but never used.
WARNING:Xst:646 - Signal <SW_Instr> is assigned but never used.
WARNING:Xst:653 - Signal <sext32<0>> is used but never assigned. Tied to value 0.
WARNING:Xst:646 - Signal <iRead_Strobe_No_Dbg> is assigned but never used.
WARNING:Xst:646 - Signal <Write_ICache<0>> is assigned but never used.
WARNING:Xst:646 - Signal <IOPB_Bus_Exception> is assigned but never used.
WARNING:Xst:646 - Signal <Load_EAR<0>> is assigned but never used.
WARNING:Xst:646 - Signal <Word_Access> is assigned but never used.
WARNING:Xst:646 - Signal <DCache_Enabled<0>> is assigned but never used.
WARNING:Xst:646 - Signal <op1> is assigned but never used.
WARNING:Xst:646 - Signal <iWrite_Strobe_No_Dbg> is assigned but never used.
WARNING:Xst:1780 - Signal <FSL_S_Exists> is never used or assigned.
WARNING:Xst:653 - Signal <hexlet_Read<0>> is used but never assigned. Tied to value 0.
WARNING:Xst:1780 - Signal <DOPB_Abort> is never used or assigned.
WARNING:Xst:646 - Signal <Load_ESR<0>> is assigned but never used.
WARNING:Xst:646 - Signal <Dbg_Write_DCache<0>> is assigned but never used.
WARNING:Xst:1780 - Signal <FSL_S_Read> is never used or assigned.
WARNING:Xst:1780 - Signal <FSL_S_Control> is never used or assigned.
WARNING:Xst:646 - Signal <Unaligned_Exception> is assigned but never used.
WARNING:Xst:1780 - Signal <iopb_Interrupt> is never used or assigned.
WARNING:Xst:1780 - Signal <FSL_M_Full> is never used or assigned.
WARNING:Xst:646 - Signal <Dbg_Write_ICache<0>> is assigned but never used.
WARNING:Xst:646 - Signal <FSL_Control_Bit> is assigned but never used.
WARNING:Xst:646 - Signal <Not_MB_Get_Op> is assigned but never used.
WARNING:Xst:646 - Signal <Illegal_Opcode_Exception> is assigned but never used.
WARNING:Xst:646 - Signal <MB_Put_Write> is assigned but never used.
WARNING:Xst:1780 - Signal <FSL_M_Data> is never used or assigned.
WARNING:Xst:646 - Signal <ICache_Enabled<0>> is assigned but never used.
WARNING:Xst:646 - Signal <Clr_ESR<0>> is assigned but never used.
WARNING:Xst:1780 - Signal <IOPB_Abort> is never used or assigned.
WARNING:Xst:646 - Signal <Div_Zero_Exception> is assigned but never used.
WARNING:Xst:646 - Signal <DOPB_Bus_Exception> is assigned but never used.
WARNING:Xst:646 - Signal <Control_Reg_D> is assigned but never used.
WARNING:Xst:1780 - Signal <FSL_S_Data> is never used or assigned.
WARNING:Xst:646 - Signal <MB_Get_Read> is assigned but never used.
WARNING:Xst:646 - Signal <Write_DCache<0>> is assigned but never used.
WARNING:Xst:1780 - Signal <FSL_M_Write> is never used or assigned.
    Found 1-bit register for signal <Trace_Data_Write>.
    Found 5-bit register for signal <Reg_Addr>.
    Found 4-bit register for signal <Prefetch_Addr>.
    Found 1-bit register for signal <Trace_AS>.
    Found 1-bit register for signal <Reg_Write>.
    Found 1-bit register for signal <Trace_Data_Read>.
    Found 32-bit register for signal <Trace_Data_Address>.
    Found 32-bit register for signal <Instr_Addr_Stored_1>.
    Found 10-bit register for signal <msr_2>.
    Found 1-bit register for signal <reset_i<0>>.
    Found 32 1-bit 2-to-1 multiplexers.
    Summary:
	inferred  88 D-type flip-flop(s).
	inferred  32 Multiplexer(s).
Unit <microblaze> synthesized.


Synthesizing Unit <microblaze_0_wrapper>.
    Related source file is C:/Data/EDKexamples/MB_Spartan3_Tutorial_6_3/synthesis/../hdl/microblaze_0_wrapper.vhd.
Unit <microblaze_0_wrapper> synthesized.

WARNING:Xst:638 - in unit Decode Conflict on KEEP property on signal of_PipeRun_s_I and of_PipeRun_s_II of_PipeRun_s_II signal will be lost.
WARNING:Xst:638 - in unit Decode Conflict on KEEP property on signal of_PipeRun_s_I and of_PipeRun_s_III of_PipeRun_s_III signal will be lost.

=========================================================================
*                       Advanced HDL Synthesis                          *
=========================================================================

Advanced RAM inference ...
Advanced multiplier inference ...
Advanced Registered AddSub inference ...
Selecting encoding for FSM_0 ...
Optimizing FSM <FSM_0> on signal <dbg_pipe_state> with one-hot encoding.
Dynamic shift register inference ...

=========================================================================
HDL Synthesis Report

Macro Statistics
# FSMs                             : 1
# Adders/Subtractors               : 2
 16-bit adder                      : 2
# Counters                         : 1
 8-bit up counter                  : 1
# Registers                        : 320
 4-bit register                    : 1
 32-bit register                   : 5
 5-bit register                    : 2
 10-bit register                   : 1
 1-bit register                    : 299
 2-bit register                    : 6
 8-bit register                    : 3
 3-bit register                    : 1
 16-bit register                   : 2
# Multiplexers                     : 120
 32-bit 2-to-1 multiplexer         : 1
 1-bit 2-to-1 multiplexer          : 117
 2-bit 2-to-1 multiplexer          : 1
 5-bit 2-to-1 multiplexer          : 1
# Xors                             : 16
 1-bit xor3                        : 1
 1-bit xor2                        : 15

=========================================================================

=========================================================================
*                         Low Level Synthesis                           *
=========================================================================
WARNING:Xst:1710 - FF/Latch  <pc_hit_1_15> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_14> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_13> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_12> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_11> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_10> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_9> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_8> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_7> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_6> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_5> (without init value) is constant in block <Debug>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <pc_hit_1_4> (without init value) is constant in block <Debug>.
WARNING:Xst:1291 - FF/Latch <prev1_7> is unconnected in block <Debug>.
WARNING:Xst:1291 - FF/Latch <prev1_6> is unconnected in block <Debug>.
WARNING:Xst:1291 - FF/Latch <prev_11_7> is unconnected in block <Debug>.
WARNING:Xst:1291 - FF/Latch <prev_11_6> is unconnected in block <Debug>.
WARNING:Xst:1291 - FF/Latch <control_reg_1> is unconnected in block <Debug_I>.
WARNING:Xst:1291 - FF/Latch <control_reg_2> is unconnected in block <Debug_I>.
WARNING:Xst:1291 - FF/Latch <read_pc> is unconnected in block <Debug_I>.
WARNING:Xst:1291 - FF/Latch <Dbg_Write_ICache_i_0> is unconnected in block <Debug_I>.
WARNING:Xst:1291 - FF/Latch <Dbg_Write_DCache_i_0> is unconnected in block <Debug_I>.
WARNING:Xst:1291 - FF/Latch <Write_DCache_I_0> is unconnected in block <Decode_I>.
WARNING:Xst:1291 - FF/Latch <Write_ICache_I_0> is unconnected in block <Decode_I>.
WARNING:Xst:1291 - FF/Latch <div_started> is unconnected in block <Decode_I>.
WARNING:Xst:1291 - FF/Latch <Not_Div_Op> is unconnected in block <Decode_I>.
WARNING:Xst:1291 - FF/Latch <Start_Div_i> is unconnected in block <Decode_I>.

Optimizing unit <microblaze_0_wrapper> ...

Optimizing unit <PreFetch_Buffer> ...

Optimizing unit <MUL_Unit> ...

Optimizing unit <Zero_Detect> ...

Optimizing unit <Register_File_Bit> ...

Optimizing unit <Register_File_Bit0> ...

Optimizing unit <Register_File_Bit1> ...

Optimizing unit <Register_File_Bit2> ...

Optimizing unit <Register_File_Bit3> ...

Optimizing unit <Register_File_Bit4> ...

Optimizing unit <Register_File_Bit5> ...

Optimizing unit <Register_File_Bit6> ...

Optimizing unit <Register_File_Bit7> ...

Optimizing unit <Register_File_Bit8> ...

Optimizing unit <Register_File_Bit9> ...

Optimizing unit <Register_File_Bit10> ...

Optimizing unit <Register_File_Bit11> ...

Optimizing unit <Register_File_Bit12> ...

Optimizing unit <Register_File_Bit13> ...

Optimizing unit <Register_File_Bit14> ...

Optimizing unit <Register_File_Bit15> ...

Optimizing unit <Register_File_Bit16> ...

Optimizing unit <Register_File_Bit17> ...

Optimizing unit <Register_File_Bit18> ...

Optimizing unit <Register_File_Bit19> ...

Optimizing unit <Register_File_Bit20> ...

Optimizing unit <Register_File_Bit21> ...

Optimizing unit <Register_File_Bit22> ...

Optimizing unit <Register_File_Bit23> ...

Optimizing unit <Register_File_Bit24> ...

Optimizing unit <Register_File_Bit25> ...

Optimizing unit <Register_File_Bit26> ...

Optimizing unit <Register_File_Bit27> ...

Optimizing unit <Register_File_Bit28> ...

Optimizing unit <Register_File_Bit29> ...

Optimizing unit <Register_File_Bit30> ...

Optimizing unit <Operand_Select_Bit> ...

Optimizing unit <Operand_Select_Bit31> ...

Optimizing unit <Operand_Select_Bit32> ...

Optimizing unit <Operand_Select_Bit33> ...

Optimizing unit <Operand_Select_Bit34> ...

Optimizing unit <Operand_Select_Bit35> ...

Optimizing unit <Operand_Select_Bit36> ...

Optimizing unit <Operand_Select_Bit37> ...

Optimizing unit <Operand_Select_Bit38> ...

Optimizing unit <Operand_Select_Bit39> ...

Optimizing unit <Operand_Select_Bit40> ...

Optimizing unit <Operand_Select_Bit41> ...

Optimizing unit <Operand_Select_Bit42> ...

Optimizing unit <Operand_Select_Bit43> ...

Optimizing unit <Operand_Select_Bit44> ...

Optimizing unit <Operand_Select_Bit45> ...

Optimizing unit <Operand_Select_Bit46> ...

Optimizing unit <Operand_Select_Bit47> ...

Optimizing unit <Operand_Select_Bit48> ...

Optimizing unit <Operand_Select_Bit49> ...

Optimizing unit <Operand_Select_Bit50> ...

Optimizing unit <Operand_Select_Bit51> ...

Optimizing unit <Operand_Select_Bit52> ...

Optimizing unit <Operand_Select_Bit53> ...

Optimizing unit <Operand_Select_Bit54> ...

Optimizing unit <Operand_Select_Bit55> ...

Optimizing unit <Operand_Select_Bit56> ...

Optimizing unit <Operand_Select_Bit57> ...

Optimizing unit <Operand_Select_Bit58> ...

Optimizing unit <Operand_Select_Bit59> ...

Optimizing unit <Operand_Select_Bit60> ...

Optimizing unit <Operand_Select_Bit61> ...

Optimizing unit <ALU_Bit> ...

Optimizing unit <ALU_Bit62> ...

Optimizing unit <ALU_Bit63> ...

Optimizing unit <ALU_Bit64> ...

Optimizing unit <ALU_Bit65> ...

Optimizing unit <ALU_Bit66> ...

Optimizing unit <ALU_Bit67> ...

Optimizing unit <ALU_Bit68> ...

Optimizing unit <ALU_Bit69> ...

Optimizing unit <ALU_Bit70> ...

Optimizing unit <ALU_Bit71> ...

Optimizing unit <ALU_Bit72> ...

Optimizing unit <ALU_Bit73> ...

Optimizing unit <ALU_Bit74> ...

Optimizing unit <ALU_Bit75> ...

Optimizing unit <ALU_Bit76> ...

Optimizing unit <ALU_Bit77> ...

Optimizing unit <Shift_Logic_Bit> ...

Optimizing unit <Shift_Logic_Bit78> ...

Optimizing unit <Shift_Logic_Bit79> ...

Optimizing unit <Shift_Logic_Bit80> ...

Optimizing unit <Shift_Logic_Bit81> ...

Optimizing unit <Shift_Logic_Bit82> ...

Optimizing unit <Shift_Logic_Bit83> ...

Optimizing unit <Shift_Logic_Bit84> ...

Optimizing unit <Shift_Logic_Bit85> ...

Optimizing unit <Shift_Logic_Bit86> ...

Optimizing unit <Shift_Logic_Bit87> ...

Optimizing unit <Shift_Logic_Bit88> ...

Optimizing unit <Shift_Logic_Bit89> ...

Optimizing unit <Shift_Logic_Bit90> ...

Optimizing unit <Shift_Logic_Bit91> ...

Optimizing unit <Shift_Logic_Bit92> ...

Optimizing unit <Shift_Logic_Bit93> ...

Optimizing unit <Shift_Logic_Bit94> ...

Optimizing unit <Shift_Logic_Bit95> ...

Optimizing unit <Shift_Logic_Bit96> ...

Optimizing unit <Shift_Logic_Bit97> ...

Optimizing unit <Shift_Logic_Bit98> ...

Optimizing unit <Shift_Logic_Bit99> ...

Optimizing unit <Shift_Logic_Bit100> ...

Optimizing unit <Shift_Logic_Bit101> ...

Optimizing unit <Shift_Logic_Bit102> ...

Optimizing unit <Shift_Logic_Bit103> ...

Optimizing unit <Shift_Logic_Bit104> ...

Optimizing unit <Shift_Logic_Bit105> ...

Optimizing unit <Shift_Logic_Bit106> ...

Optimizing unit <Shift_Logic_Bit107> ...

Optimizing unit <Shift_Logic_Bit108> ...

Optimizing unit <Result_Mux_Bit> ...

Optimizing unit <Result_Mux_Bit109> ...

Optimizing unit <Result_Mux_Bit110> ...

Optimizing unit <Result_Mux_Bit111> ...

Optimizing unit <Result_Mux_Bit112> ...

Optimizing unit <Result_Mux_Bit113> ...

Optimizing unit <Result_Mux_Bit114> ...

Optimizing unit <Result_Mux_Bit115> ...

Optimizing unit <Result_Mux_Bit116> ...

Optimizing unit <Result_Mux_Bit117> ...

Optimizing unit <Result_Mux_Bit118> ...

Optimizing unit <Result_Mux_Bit119> ...

Optimizing unit <Result_Mux_Bit120> ...

Optimizing unit <Result_Mux_Bit121> ...

Optimizing unit <Result_Mux_Bit122> ...

Optimizing unit <Result_Mux_Bit123> ...

Optimizing unit <Result_Mux_Bit124> ...

Optimizing unit <Result_Mux_Bit125> ...

Optimizing unit <Result_Mux_Bit126> ...

Optimizing unit <Result_Mux_Bit127> ...

Optimizing unit <Result_Mux_Bit128> ...

Optimizing unit <Result_Mux_Bit129> ...

Optimizing unit <Result_Mux_Bit130> ...

Optimizing unit <Result_Mux_Bit131> ...

Optimizing unit <Result_Mux_Bit132> ...

Optimizing unit <Result_Mux_Bit133> ...

Optimizing unit <Result_Mux_Bit134> ...

Optimizing unit <Result_Mux_Bit135> ...

Optimizing unit <Result_Mux_Bit136> ...

Optimizing unit <Result_Mux_Bit137> ...

Optimizing unit <Result_Mux_Bit138> ...

Optimizing unit <Result_Mux_Bit139> ...

Optimizing unit <MSR_Reg_Bit> ...

Optimizing unit <MSR_Reg_Bit140> ...

Optimizing unit <MSR_Reg_Bit141> ...

Optimizing unit <MSR_Reg_Bit142> ...

Optimizing unit <MSR_Reg_Bit143> ...

Optimizing unit <MSR_Reg_Bit144> ...

Optimizing unit <MSR_Reg_Bit145> ...

Optimizing unit <MSR_Reg_Bit146> ...

Optimizing unit <PC_Bit> ...

Optimizing unit <PC_Bit147> ...

Optimizing unit <PC_Bit148> ...

Optimizing unit <PC_Bit149> ...

Optimizing unit <PC_Bit150> ...

Optimizing unit <PC_Bit151> ...

Optimizing unit <PC_Bit152> ...

Optimizing unit <PC_Bit153> ...

Optimizing unit <PC_Bit154> ...

Optimizing unit <PC_Bit155> ...

Optimizing unit <PC_Bit156> ...

Optimizing unit <PC_Bit157> ...

Optimizing unit <PC_Bit158> ...

Optimizing unit <PC_Bit159> ...

Optimizing unit <PC_Bit160> ...

Optimizing unit <PC_Bit161> ...

Optimizing unit <Data_Read_Steering> ...

Optimizing unit <mux4_8> ...

Optimizing unit <OPB_Data_Mux> ...

Optimizing unit <mux2_32> ...

Optimizing unit <address_hit> ...

Optimizing unit <address_data_hit> ...

Optimizing unit <address_data_hit163> ...

Optimizing unit <Decode> ...

Optimizing unit <Byte_Doublet_Handle> ...

Optimizing unit <DOPB_Interface> ...

Optimizing unit <IOPB_Interface> ...

Optimizing unit <Debug> ...
WARNING:Xst:1710 - FF/Latch  <Dbg_Result_Sel_1> (without init value) is constant in block <Debug>.

Optimizing unit <Register_File> ...

Optimizing unit <Operand_Select> ...

Optimizing unit <ALU> ...

Optimizing unit <Shift_Logic_Module> ...

Optimizing unit <Result_Mux> ...

Optimizing unit <MSR_Reg> ...

Optimizing unit <PC_Module> ...

Optimizing unit <Data_Flow> ...

Optimizing unit <microblaze> ...
Loading device for application Xst from file '3s200.nph' in environment C:/ISE63.

Mapping all equations...
WARNING:Xst:1710 - FF/Latch  <microblaze_0/msr_2_0> (without init value) is constant in block <microblaze_0_wrapper>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <microblaze_0/Prefetch_Addr_0> (without init value) is constant in block <microblaze_0_wrapper>.
WARNING:Xst:1895 - Due to other FF/Latch trimming, FF/Latch  <microblaze_0/msr_2_1> (without init value) is constant in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Decode_I/Write_DCache_I_0> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Decode_I/Write_ICache_I_0> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Decode_I/div_started> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Decode_I/Not_Div_Op> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Decode_I/Start_Div_i> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Debug_I/control_reg_1> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Debug_I/control_reg_2> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Debug_I/read_pc> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Debug_I/Dbg_Write_ICache_i_0> is unconnected in block <microblaze_0_wrapper>.
WARNING:Xst:1291 - FF/Latch <microblaze_0/Debug_I/Dbg_Write_DCache_i_0> is unconnected in block <microblaze_0_wrapper>.
Building and optimizing final netlist ...
WARNING:Xst:382 - Register IM_select_I is equivalent to iOPB_MGrant_d_I
WARNING:Xst:382 - Register DM_select_I is equivalent to dOPB_MGrant_d_I
Register microblaze_0/Decode_I/Instr_EX_4 equivalent to microblaze_0/Decode_I/Logic_Oper_0 has been removed
Register microblaze_0/Decode_I/Instr_EX_25 equivalent to microblaze_0/Decode_I/Shift_Oper_0 has been removed
Register microblaze_0/Decode_I/Instr_EX_30 equivalent to microblaze_0/Decode_I/Unsigned_Op has been removed
Register microblaze_0/Decode_I/Logic_Oper_1 equivalent to microblaze_0/Decode_I/Instr_EX_5 has been removed
Register microblaze_0/Decode_I/Shift_Oper_1 equivalent to microblaze_0/Decode_I/Instr_EX_26 has been removed
WARNING:Xst:382 - Register microblaze_0/Debug_I/Dbg_Inhibit_EX_FDRSE is equivalent to microblaze_0/Debug_I/Stop_CPU_FDRSE
WARNING:Xst:382 - Register microblaze_0/Debug_I/Dbg_Inhibit_EX_FDRSE is equivalent to microblaze_0/Debug_I/Stop_CPU_FDRSE
WARNING:Xst:382 - Register IM_select_I is equivalent to iOPB_MGrant_d_I
WARNING:Xst:382 - Register DM_select_I is equivalent to dOPB_MGrant_d_I
WARNING:Xst:382 - Register microblaze_0/Debug_I/Dbg_Inhibit_EX_FDRSE is equivalent to microblaze_0/Debug_I/Stop_CPU_FDRSE
WARNING:Xst:382 - Register IM_select_I is equivalent to iOPB_MGrant_d_I
WARNING:Xst:382 - Register DM_select_I is equivalent to dOPB_MGrant_d_I
WARNING:Xst:382 - Register IM_select_I is equivalent to iOPB_MGrant_d_I
WARNING:Xst:382 - Register DM_select_I is equivalent to dOPB_MGrant_d_I
WARNING:Xst:382 - Register microblaze_0/Debug_I/Dbg_Inhibit_EX_FDRSE is equivalent to microblaze_0/Debug_I/Stop_CPU_FDRSE
WARNING:Xst:382 - Register IM_select_I is equivalent to iOPB_MGrant_d_I
WARNING:Xst:382 - Register DM_select_I is equivalent to dOPB_MGrant_d_I
FlipFlop microblaze_0/Debug_I/Dbg_Write_PC_0 has been replicated 1 time(s)

=========================================================================
*                            Final Report                               *
=========================================================================
Final Results
RTL Top Level Output File Name     : ../implementation/microblaze_0_wrapper/microblaze_0_wrapper.ngr
Top Level Output File Name         : ../implementation/microblaze_0_wrapper/microblaze_0_wrapper.ngc
Output Format                      : ngc
Optimization Goal                  : speed
Keep Hierarchy                     : no

Design Statistics
# IOs                              : 1300

Macro Statistics :
# Registers                        : 315
#      1-bit register              : 293
#      10-bit register             : 1
#      16-bit register             : 2
#      2-bit register              : 6
#      3-bit register              : 1
#      32-bit register             : 5
#      4-bit register              : 1
#      5-bit register              : 2
#      8-bit register              : 4
# Multiplexers                     : 120
#      2-to-1 multiplexer          : 120
# Adders/Subtractors               : 3
#      16-bit adder                : 2
#      8-bit adder                 : 1
# Xors                             : 1
#      1-bit xor3                  : 1

Cell Usage :
# BELS                             : 1787
#      GND                         : 8
#      LUT1                        : 44
#      LUT1_L                      : 2
#      LUT2                        : 290
#      LUT2_D                      : 3
#      LUT2_L                      : 12
#      LUT3                        : 391
#      LUT3_D                      : 5
#      LUT3_L                      : 12
#      LUT4                        : 470
#      LUT4_D                      : 9
#      LUT4_L                      : 43
#      MULT_AND                    : 32
#      MUXCY                       : 93
#      MUXCY_L                     : 90
#      MUXF5                       : 172
#      VCC                         : 7
#      XORCY                       : 104
# FlipFlops/Latches                : 896
#      FD                          : 90
#      FDC                         : 117
#      FDCE                        : 157
#      FDE                         : 203
#      FDP                         : 4
#      FDPE                        : 4
#      FDR                         : 62
#      FDRE                        : 112
#      FDRSE                       : 112
#      FDS                         : 4
#      FDSE                        : 31
# RAMS                             : 128
#      RAM16X1D                    : 128
# Shifters                         : 121
#      SRL16E                      : 121
# MULTs                            : 3
#      MULT18X18S                  : 3
=========================================================================

Device utilization summary:
---------------------------

Selected Device : 3s200ft256-4 

 Number of Slices:                    1126  out of   1920    58%  
 Number of Slice Flip Flops:           896  out of   3840    23%  
 Number of 4 input LUTs:              1530  out of   3840    39%  
 Number of MULT18X18s:                   3  out of     12    25%  


=========================================================================
TIMING REPORT

NOTE: THESE TIMING NUMBERS ARE ONLY A SYNTHESIS ESTIMATE.
      FOR ACCURATE TIMING INFORMATION PLEASE REFER TO THE TRACE REPORT
      GENERATED AFTER PLACE-and-ROUTE.

Clock Information:
------------------
-----------------------------------+------------------------+-------+
Clock Signal                       | Clock buffer(FF name)  | Load  |
-----------------------------------+------------------------+-------+
CLK                                | NONE                   | 937   |
DBG_CLK                            | NONE                   | 211   |
-----------------------------------+------------------------+-------+

Timing Summary:
---------------
Speed Grade: -4

   Minimum period: 9.997ns (Maximum Frequency: 100.029MHz)
   Minimum input arrival time before clock: 7.042ns
   Maximum output required time after clock: 7.641ns
   Maximum combinational path delay: 3.927ns

Timing Detail:
--------------
All values displayed in nanoseconds (ns)

-------------------------------------------------------------------------
Timing constraint: Default period analysis for Clock 'CLK'
Delay:               9.997ns (Levels of Logic = 8)
  Source:            microblaze_0/Decode_I/PreFetch_Buffer_I/SRL16E_I19 (FF)
  Destination:       microblaze_0/Data_Flow_I/Operand_Select_I/Operand_Select_Bit_I30/Op2_DFF (FF)
  Source Clock:      CLK rising
  Destination Clock: CLK rising

  Data Path: microblaze_0/Decode_I/PreFetch_Buffer_I/SRL16E_I19 to microblaze_0/Data_Flow_I/Operand_Select_I/Operand_Select_Bit_I30/Op2_DFF
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     SRL16E:CLK->Q        69   3.195   1.358  microblaze_0/Decode_I/PreFetch_Buffer_I/SRL16E_I19 (microblaze_0/reg2_Addr<3>)
     LUT4_D:I2->O          2   0.551   0.465  microblaze_0/Decode_I/Ker280051 (microblaze_0/Decode_I/N28007)
     LUT4:I0->O            1   0.551   0.240  microblaze_0/Decode_I/_n0442118_SW0 (N51807)
     LUT4_L:I3->LO         1   0.551   0.100  microblaze_0/Decode_I/_n0442118 (CHOICE622)
     LUT4:I1->O           32   0.551   1.321  microblaze_0/Decode_I/_n0442202 (microblaze_0/res_Forward2)
     begin scope: 'microblaze_0/Data_Flow_I'
     begin scope: 'Operand_Select_I'
     begin scope: 'Operand_Select_Bit_I22'
     LUT4:I2->O            1   0.551   0.000  Op2_Mux2_1 (op2_Reg)
     MUXF5:I0->O           1   0.360   0.000  Op2_MUXF5 (op2_I)
     FDRSE:D                   0.203          Op2_DFF
    ----------------------------------------
    Total                      9.997ns (6.513ns logic, 3.484ns route)
                                       (65.1% logic, 34.9% route)

-------------------------------------------------------------------------
Timing constraint: Default period analysis for Clock 'DBG_CLK'
Delay:               5.616ns (Levels of Logic = 3)
  Source:            microblaze_0/Debug_I/shift_Count_0 (FF)
  Destination:       microblaze_0/Debug_I/address_data_hit_10/SRL16E_data_12 (FF)
  Source Clock:      DBG_CLK rising
  Destination Clock: DBG_CLK rising

  Data Path: microblaze_0/Debug_I/shift_Count_0 to microblaze_0/Debug_I/address_data_hit_10/SRL16E_data_12
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDR:C->Q             11   0.720   0.836  microblaze_0/Debug_I/shift_Count_0 (microblaze_0/Debug_I/shift_Count_0)
     LUT4:I2->O            3   0.551   0.577  microblaze_0/Debug_I/Ker328861 (microblaze_0/Debug_I/N32888)
     LUT2:I1->O           16   0.551   0.995  microblaze_0/Debug_I/Ker330061 (microblaze_0/Debug_I/N33008)
     LUT4:I3->O            2   0.551   0.465  microblaze_0/Debug_I/SRL16_En0<0>1 (microblaze_0/Debug_I/SRL16_En0<0>)
     SRL16E:CE                 0.370          microblaze_0/Debug_I/address_data_hit_10/SRL16E_data_23
    ----------------------------------------
    Total                      5.616ns (2.743ns logic, 2.873ns route)
                                       (48.8% logic, 51.2% route)

-------------------------------------------------------------------------
Timing constraint: Default OFFSET IN BEFORE for Clock 'DBG_CLK'
Offset:              4.060ns (Levels of Logic = 3)
  Source:            DBG_REG_EN<2> (PAD)
  Destination:       microblaze_0/Debug_I/address_data_hit_10/SRL16E_data_12 (FF)
  Destination Clock: DBG_CLK rising

  Data Path: DBG_REG_EN<2> to microblaze_0/Debug_I/address_data_hit_10/SRL16E_data_12
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     LUT4:I0->O            3   0.551   0.577  microblaze_0/Debug_I/Ker328861 (microblaze_0/Debug_I/N32888)
     LUT2:I1->O           16   0.551   0.995  microblaze_0/Debug_I/Ker330061 (microblaze_0/Debug_I/N33008)
     LUT4:I3->O            2   0.551   0.465  microblaze_0/Debug_I/SRL16_En0<0>1 (microblaze_0/Debug_I/SRL16_En0<0>)
     SRL16E:CE                 0.370          microblaze_0/Debug_I/address_data_hit_10/SRL16E_data_23
    ----------------------------------------
    Total                      4.060ns (2.023ns logic, 2.037ns route)
                                       (49.8% logic, 50.2% route)

-------------------------------------------------------------------------
Timing constraint: Default OFFSET IN BEFORE for Clock 'CLK'
Offset:              7.042ns (Levels of Logic = 8)
  Source:            DREADY (PAD)
  Destination:       microblaze_0/Data_Flow_I/ALU_I/ALU_Bit_I0/I_ABus_DFF (FF)
  Destination Clock: CLK rising

  Data Path: DREADY to microblaze_0/Data_Flow_I/ALU_I/ALU_Bit_I0/I_ABus_DFF
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     LUT2:I0->O            2   0.551   0.465  microblaze_0/stop_Data_OPB1 (microblaze_0/stop_Data_OPB)
     begin scope: 'microblaze_0/Dopb_Interface_I'
     LUT2:I0->O            3   0.551   0.577  abort_Access_i1 (abort_Access_i)
     LUT4:I0->O            1   0.551   0.240  OPB_RESPONSE_I (opb_Response)
     LUT4:I0->O            5   0.551   0.658  dOPB_MGrant_Rst_I (dOPB_MGrant_Rst)
     LUT4:I1->O           32   0.551   1.321  Rst_DM_DBus1 (Rst_DM_DBus)
     end scope: 'microblaze_0/Dopb_Interface_I'
     FDRE:R                    1.026          microblaze_0/Byte_Doublet_Handle_I/M_DBus_DFF0
    ----------------------------------------
    Total                      7.042ns (3.781ns logic, 3.261ns route)
                                       (53.7% logic, 46.3% route)

-------------------------------------------------------------------------
Timing constraint: Default OFFSET OUT AFTER for Clock 'CLK'
Offset:              7.266ns (Levels of Logic = 65)
  Source:            microblaze_0/Decode_I/PreFetch_Buffer_I/FDS_I1 (FF)
  Destination:       INSTR_ADDR<0> (PAD)
  Source Clock:      CLK rising

  Data Path: microblaze_0/Decode_I/PreFetch_Buffer_I/FDS_I1 to INSTR_ADDR<0>
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     FDS:C->Q             68   0.720   1.357  microblaze_0/Decode_I/PreFetch_Buffer_I/FDS_I1 (microblaze_0/buffer_Addr<1>)
     LUT4_L:I0->LO         1   0.551   0.100  microblaze_0/Decode_I/_n04211 (microblaze_0/pc_Incr)
     begin scope: 'microblaze_0/Data_Flow_I'
     begin scope: 'PC_Module_I'
     begin scope: 'PC_Bit_I29'
     LUT4:I0->O            1   0.551   0.000  Sum_I (xor_Sum)
     MUXCY_L:S->LO         1   0.500   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I29'
     begin scope: 'PC_Bit_I28'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I28'
     begin scope: 'PC_Bit_I27'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I27'
     begin scope: 'PC_Bit_I26'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I26'
     begin scope: 'PC_Bit_I25'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I25'
     begin scope: 'PC_Bit_I24'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I24'
     begin scope: 'PC_Bit_I23'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I23'
     begin scope: 'PC_Bit_I22'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I22'
     begin scope: 'PC_Bit_I21'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I21'
     begin scope: 'PC_Bit_I20'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I20'
     begin scope: 'PC_Bit_I19'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I19'
     begin scope: 'PC_Bit_I18'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I18'
     begin scope: 'PC_Bit_I17'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I17'
     begin scope: 'PC_Bit_I16'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I16'
     begin scope: 'PC_Bit_I15'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I15'
     begin scope: 'PC_Bit_I14'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I14'
     begin scope: 'PC_Bit_I13'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I13'
     begin scope: 'PC_Bit_I12'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I12'
     begin scope: 'PC_Bit_I11'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I11'
     begin scope: 'PC_Bit_I10'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I10'
     begin scope: 'PC_Bit_I9'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I9'
     begin scope: 'PC_Bit_I8'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I8'
     begin scope: 'PC_Bit_I7'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I7'
     begin scope: 'PC_Bit_I6'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I6'
     begin scope: 'PC_Bit_I5'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I5'
     begin scope: 'PC_Bit_I4'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I4'
     begin scope: 'PC_Bit_I3'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I3'
     begin scope: 'PC_Bit_I2'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I2'
     begin scope: 'PC_Bit_I1'
     MUXCY_L:CI->LO        1   0.064   0.000  MUXCY_X (Carry_Out)
     end scope: 'PC_Bit_I1'
     begin scope: 'PC_Bit_I0'
     XORCY:CI->O           1   0.904   0.240  XOR_X (pc_Sum)
     LUT4:I0->O            2   0.551   0.000  NewPC_Mux (Instr_Addr)
     end scope: 'PC_Bit_I0'
     end scope: 'PC_Module_I'
     end scope: 'microblaze_0/Data_Flow_I'
    ----------------------------------------
    Total                      7.266ns (5.569ns logic, 1.697ns route)
                                       (76.6% logic, 23.4% route)

-------------------------------------------------------------------------
Timing constraint: Default OFFSET OUT AFTER for Clock 'DBG_CLK'
Offset:              7.641ns (Levels of Logic = 6)
  Source:            microblaze_0/Debug_I/SRL16E_I (FF)
  Destination:       DBG_TDO (PAD)
  Source Clock:      DBG_CLK rising

  Data Path: microblaze_0/Debug_I/SRL16E_I to DBG_TDO
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     SRL16E:CLK->Q         3   3.195   0.577  microblaze_0/Debug_I/SRL16E_I (microblaze_0/Debug_I/tdo_config_word1<0>)
     LUT4:I1->O            1   0.551   0.000  microblaze_0/Debug_I/TDO99_F (N52100)
     MUXF5:I0->O           1   0.360   0.240  microblaze_0/Debug_I/TDO99 (CHOICE70)
     LUT4:I3->O            1   0.551   0.240  microblaze_0/Debug_I/TDO113 (CHOICE71)
     LUT4:I2->O            2   0.551   0.465  microblaze_0/Debug_I/TDO194 (CHOICE85)
     LUT4:I0->O            1   0.551   0.000  microblaze_0/Debug_I/TDO240_F (N52058)
     MUXF5:I0->O           0   0.360   0.000  microblaze_0/Debug_I/TDO240 (DBG_TDO)
    ----------------------------------------
    Total                      7.641ns (6.119ns logic, 1.522ns route)
                                       (80.1% logic, 19.9% route)

-------------------------------------------------------------------------
Timing constraint: Default path analysis
Delay:               3.927ns (Levels of Logic = 5)
  Source:            DBG_REG_EN<2> (PAD)
  Destination:       DBG_TDO (PAD)

  Data Path: DBG_REG_EN<2> to DBG_TDO
                                Gate     Net
    Cell:in->out      fanout   Delay   Delay  Logical Name (Net Name)
    ----------------------------------------  ------------
     LUT3:I0->O            5   0.551   0.658  microblaze_0/Debug_I/Ker329211 (microblaze_0/Debug_I/N32923)
     LUT3:I0->O            1   0.551   0.240  microblaze_0/Debug_I/_n02661 (microblaze_0/Debug_I/Data_Read_Reg_En)
     LUT4:I0->O            2   0.551   0.465  microblaze_0/Debug_I/TDO194 (CHOICE85)
     LUT4:I0->O            1   0.551   0.000  microblaze_0/Debug_I/TDO240_F (N52058)
     MUXF5:I0->O           0   0.360   0.000  microblaze_0/Debug_I/TDO240 (DBG_TDO)
    ----------------------------------------
    Total                      3.927ns (2.564ns logic, 1.363ns route)
                                       (65.3% logic, 34.7% route)

=========================================================================
CPU : 83.93 / 186.23 s | Elapsed : 84.00 / 85.00 s
 
--> 

Total memory usage is 235876 kilobytes


