
bitinit version Xilinx EDK 6.3 Build EDK_Gmm.10
Copyright (c) Xilinx Inc. 2002.

Parsing MHS File system.mhs...
PM_SPEC -- Xilinx path component is <C:/EDK>
Sourcing tcl file
C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_v20_v1_10_b/data/opb_v20_v2_1_0.tcl
...Done
Sourcing tcl file
C:/EDK/hw/XilinxProcessorIPLib/pcores/lmb_bram_if_cntlr_v1_00_b/data/lmb_bram_if
_cntlr_v2_1_0.tcl ...Done
Sourcing tcl file
C:/EDK/hw/XilinxProcessorIPLib/pcores/lmb_v10_v1_00_a/data/lmb_v10_v2_1_0.tcl
...Done
Sourcing tcl file
C:/EDK/hw/XilinxProcessorIPLib/pcores/opb_emc_v1_10_b/data/opb_emc_v2_1_0.tcl
...Done

Overriding IP level properties ...
opb_intc (opb_intc_0) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\opb_intc_v1_00_c\data\opb_intc_v2_1_0.mpd:
32 - overriding c_family value virtex2 to 
bram_block (opb_bram_if_cntlr_1_bram) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a\data\bram_block_v2_1_0.
mpd:38 - overriding c_family value virtex2 to 
microblaze (microblaze_0) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\microblaze_v3_00_a\data\microblaze_v2_1_0.
mpd:55 - overriding c_family value virtex2 to 
microblaze (microblaze_0) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\microblaze_v3_00_a\data\microblaze_v2_1_0.
mpd:56 - overriding c_instance value microblaze to microblaze_0
bram_block (lmb_bram) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\bram_block_v1_00_a\data\bram_block_v2_1_0.
mpd:38 - overriding c_family value virtex2 to 
opb_mdm (debug_module) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\opb_mdm_v2_00_a\data\opb_mdm_v2_1_0.mpd:37
- overriding c_family value virtex2 to 
opb_gpio (push_buttons_3bit) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\opb_gpio_v3_01_a\data\opb_gpio_v2_1_0.mpd:
37 - overriding c_family value virtex2 to 
opb_gpio (leds_8bit) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\opb_gpio_v3_01_a\data\opb_gpio_v2_1_0.mpd:
37 - overriding c_family value virtex2 to 
opb_gpio (led_cathodes) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\opb_gpio_v3_01_a\data\opb_gpio_v2_1_0.mpd:
37 - overriding c_family value virtex2 to 
opb_gpio (led_anodes) -
C:\EDK\hw\XilinxProcessorIPLib\pcores\opb_gpio_v3_01_a\data\opb_gpio_v2_1_0.mpd:
37 - overriding c_family value virtex2 to 

Performing IP level DRCs on properties...

Running DRC Tcl procedures for OPTION IPLEVEL_DRC_PROC...
Sourcing tcl file
C:/EDK/hw/XilinxProcessorIPLib/pcores/emc_common_v2_00_a/data/emc_common_v2_1_0.
tcl ...Done
Address Map for Processor microblaze_0
  (0x00000000-0x00001fff) dlmb_cntlr	dlmb
  (0x00000000-0x00001fff) ilmb_cntlr	ilmb
  (0x80200100-0x802001ff) opb_intc_0	mb_opb
  (0x80200200-0x802002ff) debug_module	mb_opb
  (0x80200300-0x802003ff) RS232	mb_opb
  (0x80200400-0x802005ff) SRAM_256Kx32	mb_opb
  (0x80200600-0x802007ff) Push_Buttons_3Bit	mb_opb
  (0x80200800-0x802009ff) LEDs_8Bit	mb_opb
  (0x80200a00-0x80200bff) LED_cathodes	mb_opb
  (0x80200c00-0x80200dff) LED_anodes	mb_opb
  (0x80202000-0x80203fff) opb_bram_if_cntlr_1	mb_opb
  (0x80300000-0x803fffff) SRAM_256Kx32	mb_opb

Initializing Memory...
Checking ELFs associated with MICROBLAZE instance microblaze_0 for overlap...


Analyzing file TestApp/executable.elf...
Running Data2Mem with the following command:
data2mem -bm implementation/system_bd -bt implementation/system.bit  -bd
TestApp/executable.elf tag lmb_bram opb_bram_if_cntlr_1_bram  -o b
implementation/download.bit 
Memory Initialization completed successfully.

